RCP Plus

Reference

(RCP Version 3)

Specification

Firmware version | major | 4
| minor | 21
| build | 15

Copyright | This manual is the intellectual property of VCS and is protected by copyright. All rights are reserved. No part of this document may be reproduced or transmitted for any purpose, by whatever means, be they electronic or mechanical, without the express written permission of VCS. © Copyright 2001-2006 VCS Video Communication Systems AG
Note | This manual was compiled with the greatest of care and all information double checked. At the time of printing the description was complete and correct. Because of the further development of products, the content of the manual might change without prior notice. VCS will not be liable for damage which is directly or indirectly due to errors, incompleteness, or discrepancies between the manual and the product described.
Trade marks | All names used in this manual for hardware and software are very probably registered trade marks and must be treated as such.

# Table Of Contents

FUNCTIONAL_DESCRIPTION
CONNECTION
SYSTEM
ENCODER
VIDEO
AUDIO
ALARM
DIGITAL_IO
SERIAL
NETWORK
ISCSI
STORAGE
APPENDIX

Transport Protocol
The transport protocol for this remote control must be TCP. All VideoJets will establish a TCP listen socket on port 1756. Any remote control must be sent to this port. Multiple RCP connections from the same endpoints are allowed. The maximum number of RCP connections on a single endpoint is limited to 50 connections at the same time. Alternatively, a connection can be made using a HTTP tunnel. See this chapter for details.
Remote Control ProtocolPlus Protocol Header Layout
Version 3 (VIP, VideoJet and VipX Series and VIP110Version 6.0 and higher). The RCP Plus protocol header consists of 16 Bytes. The begin of the payload section is now on DWORD boundary.

16 | 32
Tag 2 Bytes | Data Type 1 Byte | Version 4 Bits | R/W 4 Bits
C 1 | Action 7 Bits | Reserved 1 Byte | Client ID 2 Bytes
Session ID 4 Bytes
Numeric Descriptor 2 Bytes | Payload Length 2 Bytes
8 | 24 |

Tag
Each tag is represented by two octets. It identifies the command which should be processed by the VideoJet.
Data Type
Specifies the data type of the payload section. These are the currently available data types:
Values:

F_FLAG |  | 0x00 (1 Byte)
T_OCTET |  | 0x01 (1 Byte)
T_WORD |  | 0x02 (2 Byte)
T_INT |  | 0x04 (4 Byte)
T_DWORD |  | 0x08 (4 Byte)
P_OCTET |  | 0x0C (N Byte)
P_STRING |  | 0x10 (N Byte)
P_UNICODE |  | 0x14 (N Byte)

Version
The current RCP version is 3. Backward compatibility to version 2 or version 0 is NOT provided.
R/W
Specifies whether the command should read or write. The Read/Write field is coded in the lower nibble of byte 4.
Values:

Read |  | 0x0
Write |  | 0x1

C
Continuation. This bit signals, when set, that this RCP+ packet is not terminated in the payload; additional packets with the full RCP+ header will follow immediately in the stream as long as this bit is cleared. The reassembly of the complete payload is up to the application and is beyond the scope of this document.
Action
Specifies the kind of the packet.
Values:

Request |  | 0x00
Reply |  | 0x01
Message |  | 0x02
Error |  | 0x03

Client ID
Each RCP client register results in a Client ID; this ID has to be provided in all following RCP commands.
Session ID
This ID is used for implementations which need to identify a once registered user in other applications or RCP sessions.
Numeric Descriptor
The Numeric Descriptor specifies an attribute for components which are installed more than one time inside the VideoJet, e.g. inputs or relays. The first component is always counted as 1. If this field is not applicable to the command in this packet, a value of zero should be inserted.
Payload Length
The number of data bytes inside the payload section. The length field itself is not counted.
Reserved
This byte is returned by the VideoJet unchanged. It is up to the user to setup a request ID here to assign the replies to multiple pending requests .
Packetizing in the TCP Stream
As TCP is a stream oriented protocol, packetizing information has to be inserted to achieve proper packet reconstruction. For this purpose the TPKT structure is used.

16 | 32
Version 1 Byte | Reserved 1 Byte | Length 2 Bytes
RCP Packet N Bytes
8 | 24 |

Version
TPKT version 3.
Reserved
Should be set to zero.
Length
Byte count of the complete packet; RCP packet length + TPKT length (4 Bytes).
RCP Protocol Procedure
Request / Reply
The VideoJet unit will send back a reply on each incoming request. In some protocol functions the reply will carry no data.
NOTE: A reply from a write command which is not readable will be an RCP_ERROR_READ_NOT_SUPPORTED (error code 0x90) This means that it is not possible to determine correct setting of the command.
Messages
A message will be generated on the VideoJet on certain events (see RCP command for details). If an RCP client is registered to receive a certain message (e.g. an input state has changed), the VideoJet will generate it. The message has the same payload format as the response to a Read command of the same tag, except the reserved byte. The reserved byte is used as sequence number.
RCP is capable of sending messages on certain events. Before an RCP client can receive these messages, a registration at the VideoJet is necessary.
RCP Errors
The packet will have the standard layout with the method field set to ‘Error’. The first bytes of the payload section contains error cause. If the error code is RCP_ERROR_COMMAND_SPECIFIC, then the command specific error (see RCP command for details) is included in the second byte. The following generic error codes are defined:

RCP_ERROR_UNKNOWN |  | 0xFF
RCP_ERROR_INVALID_VERSION |  | 0x10
RCP_ERROR_NOT_REGISTERED |  | 0x20
RCP_ERROR_INVALID_CLIENT_ID |  | 0x21
RCP_ERROR_INVALID_METHOD |  | 0x30
RCP_ERROR_INVALID_CMD |  | 0x40
RCP_ERROR_INVALID_ACCESS_TYPE |  | 0x50
RCP_ERROR_INVALID_DATA_TYPE |  | 0x60
RCP_ERROR_WRITE_ERROR |  | 0x70
RCP_ERROR_PACKET_SIZE |  | 0x80
RCP_ERROR_READ_NOT_SUPPORTED |  | 0x90
RCP_ERROR_INVALID_AUTH_LEVEL |  | 0xa0
RCP_ERROR_INVAILD_SESSION_ID |  | 0xb0
RCP_ERROR_TRY_LATER |  | 0xc0
RCP_ERROR_COMMAND_SPECIFIC |  | 0xe0

Note the error code 0xc0 RCP_ERROR_TRY_LATER indicates, that the VideoJet recognizes the command, but it cannot be processed immediately. The client should repeat this command later.
A list of all defined command specific error codes can be found in the Appendix.
RCP over a HTTP tunnel
Many network installations includes firewalls to protect network segments against unauthorisized access. In many cases, the HTTP port (80) is enabled by default to gain Internet access. For this purpose, RCP offers a second network port. As the VideoJet has a built in webserver, the connection can be made to the webserver, the token
“GET /rcp_tunnel HTTP1.0\r\n\r\n”
advices the webserver to pass this socket to the RCP server. From that point on, the client is connected to the RCP server and can immediately cointinue with RCP registration.
Note: the delimiters ‘\r’ and ‘\n’ are written here in C notation; in the TCP packet to the server these delimiters corresponds with the ASCII codes 0x0d and 0x0a.
Example:

1. Establish a TCP connection to port 80 at your Videjet
2. Send the string “GET /rcp_tunnel HTTP 1.0\r\n\r\n” (as HEX string: 0x47 0x45 0x54 0x20 0x2f 0x72 0x63 0x70 0x5f 0x74 0x75 0x6e 0x6e 0x65 0x6c 0x20 0x48 0x54 0x54 0x50 0x31 0x2e 0x30 0x0d 0x0a 0x0d 0x0a)
3. Proceed in the same manner as a normal RCP connection

Receiving media data
The VideoJet is capable for tunneling media data through HTTP. In some network environments this might be helpful.
When using this mechanism, the connect primitive must set the “RTP over TCP” for the media encapsulation protocol. The response for Media host and port can be ignored. After that, a TCP connection to the HTTP port must be established. By sending the string
GET /media_tunnel/SSSSSSSS/CC/DD/LL/CO HTTP 1.0\r\n\r\n

SSSSSSS |  | The session ID returned from the connect primitive (padded with leading zeros to 8)
CC |  | The media type (see connect primitive; 01=video, 02=audio)
DD |  | direction of media (01=receive media, 00=transmit media)
LL |  | the line input number
CO |  | The coder number

When the HTTP server inside the VideoJet received this string, it passes this socket to the RCP. From that point on, media data will be transferred over this socket using TPKT encapsulation (see chapter Packetizing in the TCP Stream).
When all sockets of a session are in data sending mode, a RCP message MEDIA_SOCKETS_COMPLETE with the associated session ID will be sent out to the initiator of the session. This is useful when a session is used for replay; the replay PLAY command can securely be applied when the MEDIA_SOCKETS_COMPLETE message has been arrived.
RCP over CGI
RCP+ command my also be encapsulated in CGI (Common Gateway Interface) using a standard web browsers URL. All needed parameters are passed to the HTTP server of the video server which tunnels the RCP+ commands to the RCP server. The reply returned is a text based XML structure.
The CGI interface may also be used by a HTTP client written from the scratch based on RFC 1945 (HTTP 1.0) using 'GET' method. The unit's HTTP server will only examine 'Connection: Keep-Alive' and optional 'Authorization: ' header fields. See RFC for implementing details.
Valid CGI parameters:
command
Values:

The RCP+ command tag number

type
Values:

F_FLAG
T_OCTET
T_WORD
T_DWORD
P_OCTET
P_STRING
P_UNICODE

direction
Values:

READ
WRITE

num
Values:

The numeric parameter

payload
Values:

The payload as readable string for payload type P_STRING
The payload as octet array with no spaces preceeded with 0x for payload type P_OCTET and P_UNICODE
The payload value in hex or decimal notion for all other payload types

Optional CGI parameters:
idstring
Values:

User defined parameter which will not be processed by the unit; will return unchanged in the reply

sessionid
Values:

Context specific session ID for this command

Multiple parameters are passed in CGI manner with '&' in between two parameter-value pairs.
A sample request to readout the units hardware version will look like
http://ip.ip.ip.ip/rcp.xml?command=0x002e&type=P_STRING&direction=READ
The reply XML structure will then have this format:
<rcp>
<command>
<hex>0x002e</hex>
<dec>46</dec>
</command>
<type>T_DWORD</type>
<direction>READ</direction>
<num>0</num>
<idstring />
<payload />
<cltid>0x00ff</cltid>
<result>
<hex>0xf0000f43</hex>
<dec>4026535747</dec>
</result>
</rcp>
The upper part contains the request, the <result> contains the reply. Numerical values are presented in <hex> and <dec>, strings, unicodes and p_octet in <str> sections. <cltid> shows the client number assiged by the RCP+ server.
Message handling
RCP+ messages will be processed and received by the CGI client using a poll mechansim. A CGI command set with the requested messages command tag numbers need to be issued. After issueing a request, the reply returns immedialty after a message has been sent or the default timeout of 1000 ms has been expired. When the timeout expires, a message count of 0 is returned. Otherwise the number of received messages is signaled. The default timeout can be altered by setting the 'collectms' CGI value to the approriate number of milliseconds.
Vailed CGI commands to control messages:
message
Values:

One or a list of requested message RCP+ command tag numbers separated by '$'

collectms
Values:

Time in milliseconds to collect messages before returning with 'No messages'; default is 1000 ms

The <msgcnt> section contains the number of vailed <msg> sections inside the reply.
A buffer mechanism (depth 64) ensures that no messages will be lost during two consecutive poll cycles. The <over> sections counts the number of lost messages. <clip> signals too small internal buffers; this should never occur.
The <poll> section counts the number of issued poll requests
A sample request to receive all connection related messages (CONF_CONNECT_TO) will look like
http://ip.ip.ip.ip/rcp.xml?message=0xffcc&collectms=5000
The reply XML structure will then have this format:
<message_list>
<stats>
<msgcnt>2</msgcnt>
<over>0</over>
<clip>0</clip>
<poll>1</poll>
</stats>
<cltid>0x002a</cltid>
<msg>
<no>1</no>
<command>0xffcc</command>
<num>0</num>
<sessionID>0x7063001f</sessionID>
<hex>0xa00a0034000000000101000001010001</hex>
</msg>
<msg>
<no>2</no>
<command>0xffcc</command>
<num>0</num>
<sessionID>0x70630020</sessionID>
<hex>0xa00a0034000000000101000001010001</hex>
</msg>
</message_list>
Authentication
The RCP+ server need proper authentication to process protected commands. The CGI interface provides three basic authentication schemes to be used.
Using http authentication
In this case, HTTP header authentication (basic or digest) must be present in the request. The internal HTTP server will pass the login information to the RCP+ server.
Using session cookie
For each successful HTTP authentication (for all available resources like html pages, images...) a session cookie will be returned by the HTTP server. When this cookie is present in any further HTTP connections, the same authorization level will be granted the same level as the originating connection. The session cookie will remain active as long as at least one HTTP connection remains open. In this case the internal HTTP server will pass the login information to the RCP+ server.
CGI inline
By passing the CGI parameter 'pwd' with a value of the identification string as defined in the CONF_RCP_CLIENT_REGISTRATION section for normal method. This information will be directly passed to the RCP+ server for validation.
Autodetecting Devices
VCS products are being detected on a network using an IP broadcast to UDP port 1757. The format for requesting an identification is shown below.
Request Packet

16 | 32
0x99 1 Byte | 0x39 1 Byte | 0xA4 1 Byte | 0x27 1 Byte
Sequence Number 4 Bytes
0x00 1 Byte | 0x00 1 Byte | Reply Port 2 Bytes
8 | 24 |

Sequence Number
This sequence number must be a randomized number.
Reply Port
Specifies the reply UDP port e.g. RP1 0x06; RP2 0xDE -> reply port: 1758
Additional information on hardware versions
32-Bit Hardware version Former Scheme:

16 | 32
ID 4 Bits | R 2 Bits | FL 2 Bits | Serial Number 2 Bytes | Net 4 Bits | opt 4 Bits
8 | 24 |

ID
Values:

NCID_NVR |  | 0x1
NCID_VJ8000 |  | 0x2
NCID_VIP10 |  | 0x3
NCID_VIP1000 |  | 0x4
NCID_VJ400 |  | 0x6
NCID_VIP100 |  | 0x7
NCID_VJEX |  | 0x8
NCID_VJ1000 |  | 0x9
NCID_VJ100 |  | 0xA
NCID_VJ10 |  | 0xB
NCID_VJ8008 |  | 0xC
NCID_VJ8004 |  | 0xD (latest unit carrying the old numbering scheme)
EscapeCode |  | 0xF (used to switch over to new detection)

FL
Values:

HARDWARE_TYPE_VIN |  | 0x0
HARDWARE_TYPE_VOUT |  | 0x1
HARDWARE_TYPE_VIN_OUT |  | 0x2

Net
Values:

Bit1 |  | HARDWARE_SYSTEM_OPT_ISDN
Bit3 |  | HARDWARE_SYSTEM_ETHERNET

opt
Values:

Bit1 |  | HARDWARE_OPT_AUDIO
Bit2 |  | HARDWARE_OPT_HDD

32-Bit Hardware version New Scheme:

16 | 32
Esc 4 Bits | R 1 | M 1 | FL 2 Bits | Reserved 8 Bits | ID 1 Byte | Net 4 Bits | Opt 4 Bits
8 | 24 |

Esc
Must be set to 0xF
M
Values:

Master |  | 0
Slave |  | 1

FL
Flavour
Values:

HARDWARE_TYPE_VIN |  | 0x0
HARDWARE_TYPE_VOUT |  | 0x1
HARDWARE_TYPE_VIN_OUT |  | 0x2

ID
Values:

HARDWARE_ID_VIPX1 |  | 0x01
HARDWARE_ID_VIPX2 |  | 0x02
HARDWARE_ID_VIPXDEC |  | 0x03
HARDWARE_ID_VJ_X10 |  | 0x05
HARDWARE_ID_VJ_X20 |  | 0x06
HARDWARE_ID_VJ_X40 |  | 0x07
HARDWARE_ID_VJ_X40_ECO |  | 0x08
HARDWARE_ID_VJ_X10_ECO |  | 0x09
HARDWARE_ID_VJ_X20_ECO |  | 0x0A
HARDWARE_ID_IP_PANEL |  | 0x0d
HARDWARE_ID_GEN4 |  | 0x0e
HARDWARE_ID_M1600 |  | 0x0f
HARDWARE_ID_FLEXIDOME |  | 0x11
HARDWARE_ID_M1600_DEC |  | 0x13
HARDWARE_ID_M1600_XFM |  | 0x15
HARDWARE_ID_AUTODOME |  | 0x16
HARDWARE_ID_NBC_225P |  | 0x1a
HARDWARE_ID_VIPX1_XF |  | 0x1e
HARDWARE_ID_NBC_225W |  | 0x1f
HARDWARE_ID_NBC_255P |  | 0x20
HARDWARE_ID_NBC_255W |  | 0x21
HARDWARE_ID_AUTODOME_EASY_II |  | 0x23
HARDWARE_ID_AUTODOME_EASY_II_E |  | 0x24
HARDWARE_ID_VIPX1_XF_E |  | 0x25
HARDWARE_ID_VIPX1_XF_P |  | 0x26
HARDWARE_ID_VIPX1_XF_EP |  | 0x27
HARDWARE_ID_VIPX1_XF_W |  | 0x28
HARDWARE_ID_NDC_455_P |  | 0x2a
HARDWARE_ID_NDC_455_P_IVA |  | 0x2b
HARDWARE_ID_NBC_455_P |  | 0x2c
HARDWARE_ID_NBC_455_P_IVA |  | 0x2d
HARDWARE_ID_VG4_AUTODOME |  | 0x2e
HARDWARE_ID_NDC_225_P |  | 0x2f
HARDWARE_ID_NDC_255_P |  | 0x30
HARDWARE_ID_VIPER |  | 0x32
HARDWARE_ID_DINION_2X |  | 0x35
HARDWARE_ID_DINION_2X_VCA |  | 0x36
HARDWARE_ID_FLEXIDOME_2X |  | 0x37
HARDWARE_ID_FLEXIDOME_2X_VCA |  | 0x38
HARDWARE_ID_DINION_720P |  | 0x39
HARDWARE_ID_DINION_720P_IVA |  | 0x3a
HARDWARE_ID_FLEXIDOME_720P |  | 0x3b
HARDWARE_ID_FLEXIDOME_720P_IVA |  | 0x3c
HARDWARE_ID_FLEXIDOME_NDC_265_P |  | 0x3d
HARDWARE_ID_FLEXIDOME_NBC_265_P |  | 0x3e
HARDWARE_ID_FLEXIDOME_NDC_225_PI |  | 0x3f
HARDWARE_ID_FLEXIDOME_NTC_255_PI |  | 0x3f
HARDWARE_ID_EX30_IR |  | 0x20
HARDWARE_ID_VRM |  | 0xfc
HARDWARE_ID_VIDOS_SERVER |  | 0xfd
HARDWARE_ID_VIDOS_MONITOR |  | 0xfe

1st Reply Packet

16 | 32
0x99 1 Byte | 0x39 1 Byte | 0xa4 1 Byte | 0x27 1 Byte
Sequence Number 4 Bytes
Harware Address 6 Bytes ...
| 0x03 1 Byte | ID 1 Byte
Device IP 4 Bytes
Subnet Mask 4 Bytes
Gatway IP 4 Bytes
Flavor 1 Byte | Connections 1 Byte | Reserved 1 Bytes | ID new 1 Bytes
8 | 24 |

Sequence Number
Returns the sequence number from the request packet.
Hardware Address
MAC address of the device.
ID
Unit Hardware ID returned from request (will be 0xff when the new version layout is used).
Device IP
Current IP address of the device.
Subnet Mask
Current Subnet mask of the device.
Gatway IP
Current Gateway of the device.
Flavor
Flavor of this device.
Connections
Number of active connections.
ID new
The ID filed of the new version layout.
2nd Reply Packet

    <?xml version="1.0"?>
    <root xmlns="OEMExtXX:device-1-0">
    <device>
       <deviceType>OEMExtXX:device:deviceIDYY</deviceType>
       <friendlyName>VideoJet</friendlyName>
       <unitName>UnitName</unitName>
       <serialNumber>XXXXXXXX:YYYYYYYY</serialNumber>
       <physAddress>XX-XX-XX-XX-XX-XX</physAddress>
       <sessionKey>XXXXXXXXXXXXXXXX</sessionKey>
       <unitIPAddress>XXX.XXX.XXX.XXX</unitIPAddress>
       <unitSubnetMask>XXX.XXX.XXX.XXX</unitSubnetMask>
       <unitGatewayIp>XXX.XXX.XXX.XXX</unitGatewayIp>
       <activeConnections>XX</activeConnections>
    </device>
    </root>

    <root xmlns="OEMExtXX:device-1-0">
    XX is the OEM Extension; 0x00 for VCS; OEM specific

    <deviceType>OEMExtXX:device:deviceIDYY</deviceType>
    XX is the OEM Extension; 0x00 for VCS; OEM specific
    YY is the VideoJet ID from the request packet

    <friendlyName>VideoJet</friendlyName>
    The name and type of the VideoJet; type and OEM specific

    <unitName>UnitName</unitName>
    The name of the unit coded in UTF-8

    <serialNumber>XXXXXXXX:YYYYYYYY</serialNumber>
    XXXXXXX is the Hardware version of the VideoJet
    YYYYYYY is the Softwareware version of the VideoJet

    <physAddress> XX-XX-XX-XX-XX-XX </physAddress>
    XX-XX-XX-XX-XX-XX is the MAC address of the VideoJet

    <sessionKey>XXXXXXXXXXXXXXXX</sessionKey>
    No common use

    <unitIPAddress> XXX.XXX.XXX.XXX </unitIPAddress>
    XXX.XXX.XXX.XXX is the current IP address of the VideoJet

    <unitSubnetMask>XXX.XXX.XXX.XXX</unitSubnetMask>
    XXX.XXX.XXX.XXX is the subnet mask of the VideoJet

    <unitGatewayIp>XXX.XXX.XXX.XXX</unitGatewayIp>
    XXX.XXX.XXX.XXX is the current gateway IP address of the VideoJet

    <activeConnections>XX</activeConnections>
    XX is the number of active media connections of the VideoJet

    <HTTPPort>XXXX</HTTPPort>
    XXXX is the current HTTP port number the VideoJet is listening to

    <ClusterMember>XXX.XXX.XXX.XXX</ClusterMember>
    XXX.XXX.XXX.XXX is one of the cluster members; there might be multiple entries including this device

    <ClusterID>XX</ClusterID>
    XX is index number of the above ClusterMember list of this device

Setting an IP Address using Broadcast Mechanism
If the current IP address of a device doesn’t match the subnet settings, this unit cannot be reached using the standard Remote Control Protocol. All IP parameters of a VideoJet can be set using a UDP broadcast message to port 1759.
Payload Structure

16 | 32
Hardware Address 6 Bytes ...
| Reserved 2 Bytes
IP Address 4 Bytes
Subnet Mask 4 Bytes
Gateway IP 4 Bytes
Reserved 4 Bytes
8 | 24 |

Hardware Address
MAC address of the device.
IP Address
IP address to set.
Subnet Mask
Subnet mask to set.
Gateway IP
Gateway IP address to set.
As all VideoJets will receive this message, only the unit matching the hardware address (HW1-HW6) will update its IP parameters.
NOTE: There will be no reply to this command.
NOTE: This command will only work if NO service password is set.
Request or setting of system or network parameters using Broadcast Mechanism
In addition to the SETTING_AN_IP_ADDRESS_USING_BROADCAST, an additional way to setup non network configured devices has been introduced. The device itself is selected using the ethernet mac address as the first parameter inside the command structure. A list of commands including payload length information may be added. All commands must be addressed using UDP broadcast message to port 1760.
Payload Structure

MAC address 6 Bytes ...
Reserved 2 Byte | Command ID 2 Byte
Payload length 2 Byte | Variable length payload
| n Bytes |

MAC address
MAC address of the unit to configure
Command ID
ID of broadcast setting command
LED_BLINK = 0x0000
Payload length 4 bytes. Requests the unit blink the power led; payload containin the number of seconds for blinking. NOTE duration is limited to 60 sec.
SWITCH DHCP = 0x0001
Payload length 4 bytes. Switches DHCP on (payload = 1) or off (payload=0).
NOTE: This command will only work if NO service password is set.
Payload length
Length of the payload section
Variable length payload
Payload; depending on Command ID
NOTE: There will be no reply to this command.
CONF_RCP_CLIENT_REGISTRATION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xff00 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | noprot |  | % |
| Write |  | p_octet |  | noprot |  | see detailed description |

The registration is a standard RCP packet with the command code 0xFF00 with data type P_OCTET (0x0c). The Numeric Descriptor is not used. The Client ID in the header section is ignored.
Payload Structure
Payload Structure

RegType 1 Byte | Reserved 1 Byte | Client ID 2 Byte
PE 1 Byte | PL 1 Byte | Nbr 2 Byte
Tag 1 2 Byte | N x 2 Bytes | Tag N 2 Byte ...
| Char 1 1 Byte | N x 1 Byte | Char N 1 Byte

RegType
Values:

Normal Registration |  | 0x01
Hook On Registration |  | 0x02
Hook Back Registration |  | 0x03

Client ID
Unused in Normal Registration. Must be provided in Hook On Registration.
PE
Password and User Delivery Encryption.
Values:

Plain text |  | 0x00
MD5 hash |  | 0x01

PL
Password and User String Length. Number of bytes to follow for the password string.
Nbr
Number of message tags inside this packet.
Tag 1 - N
Tag codes for the messages which should be passed to the RCP client (see tag code table for capability to generate messages) – A Tag code of 0xFFFF will force the VideoJet to generate a message on all possible events.
Char 1 - N
Password string itself. NOTE: No \0 termination!
Registration Procedure
Normal Registration

1. The client opens up a TCP connection to the VideoJet.
2. The client sends an RCP registration as mentioned above.
3. The RCP server (the VideoJet) will respond with the result code and the assigned Client ID.
4. The client is now allowed to send RCP Requests provided with the Client ID.

Hook On Registration
The ‘Hook On’ registration is applicable if a registered application running on one host can provide its Client ID to a second application on the same host. This application can now perform a register at the VideoJet without naming the password.

1. The client opens up a TCP connection to the VideoJet.
2. The client sends an RCP registration with the ‘Hook On’ command and an existing Client ID on the same host. The password is not needed in this case (PL set to 0).
3. The RCP server (the VideoJet) will check whether the other client is registered properly on the same host.
4. The RCP server (the VideoJet) will respond with the result code and a NEWLY assigned Client ID.
5. The client is now allowed to send RCP Requests provided with this Client ID.

Hook Back Registration
This mechanism is used during connection establishment only. A called host is requested to do a back register to the calling host. To achieve proper client allocation on the calling host, the Client ID of the server session on the called host must be provided in the ‘Hook back’ registration.
Format: XXXX@PasswordString

XXXX: |  | The Client ID in hexadecimal notation (4 digits)
PasswordString: |  | as defined below

Password and User Delivery and Encryption
There are currently three user levels on the videojet:

- live – For video access only; no control
- user – For video access and control over the video stream (e.g. caminput)
- service - for video and all administrative access

Plain text:
The identification string must have the following format: +Username:Password+
MD5 hash encryption:

1. A 16 character random string for MD5 hash calculation must be requested from the VideoJet (RCP command CONF_RCP_REG_MD5_RANDOM).
2. A string +random_string+++username:password+ must be formed.
3. The response MD5 hash over this string must be calculated.
4. The identification string in the register packet must have the following format: +Username:random_string:response_string+

NOTE: No additional whitespaces are allowed.
Server Reply

16 | 32
Result 1 Byte | Level 1 Byte | Client ID 2 Bytes
8 | 24 |

Result
Values:

Registration failed |  | 0x00
Registration successful |  | 0x01

Level
The level after this registration.
Client ID
Identification number under which the client is now registered at the VideoJet.
CONF_RCP_CLIENT_UNREGISTER

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xff01 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | noprot |  | % |
| Write |  | p_octet |  | noprot |  | see detailed description |

Request
The unregister is a standard RCP packet with the command code 0xFF01 with no payload section. The needed information (Client ID) will be taken from the header section.
Reply
The reply will have the following format:

16 | 32
Result 1 Byte | Level 1 Byte | Client ID 2 Bytes
8 | 24 |

Result
Values:

Unregister failed |  | 0x00
Unregister successful |  | 0x01

Level
The level before this unregister.
Client ID
Identification number under which the client was registered at the VideoJet.
NOTE: This command is NOT readable.
CONF_RCP_CLIENT_TIMEOUT_WARNING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xff03 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | not supported; will generate message if client idle timeout will happen in 1 minute |
| Write |  | f_flag |  | noprot |  | not supported; will generate message if client idle timeout will happen in 1 minute. see detailed description |

Timeout handling
The RCP server has to deal with lots of RCP connections at the same time. If an RCP client is going down without notification to the server, an orphan table entry will remain. To avoid this, a timeout mechanism is provided. Each RCP client must show any activity within 10 minutes. After this time the registration of a specific RCP client is invalid. For easy handling, the RCP client can register itself for an RCP_CLIENT_TIMEOUT_WARNIG message. The client will be notified 1 minute before the timeout occurs.
The timeout renewal can be achieved by any RCP read or write command. A good advise is to read the RCP_CLIENT_REGISTRATION.
CONF_RCP_REG_MD5_RANDOM

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xff05 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | returns a 16 char. random string to be used in MD5 hash encrypted registration. see detailed description |
| Write |  | % |  | noprot |  | % |

NOTE: To avoid ‘denial of service’ attacks, the RCP server will only grant up to 5 random strings at the same time. Maximum time from the request of a random string to its use: 5 seconds. Multiple requests from the same host are ignored.
CONF_RCP_TRANSFER_TRANSPARENT_DATA

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xffdd |  | yes |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | l_live |  | see detailed description |
| Write |  | p_octet |  | l_user |  | see detailed description |

The transparent data from and to the serial interfaces is handled by the RCP to achieve reliable transfer of information. To gather control over the remote serial interface a successful registration is necessary.
Request packet

Options 1 Byte | Reserved 1 Byte | Lease Time 2 Bytes
Trans. Data 1 1 Byte | N x 1 Byte | Trans. Data N 1 Byte |

Options
Currently no options used
Lease Time
Time in seconds the lease is requested
Values:

Only this packet should be sent out; no further control is requested |  | 0x0000
Indefinite lease time; request lease as long as the current registration is valid |  | 0xFFFF

NOTE: The lease time should be treated as a request; the VideoJet may switch leases before the requested time is over due to a higher prioritized RCP client
For this direction, an RCP Write command to a specific port (addressed by the Numeric Descriptor) is necessary. Once the VideoJet has received a TRANSFER_TRANSPARENT_DATA command, it checks whether the RCP client is in control or not. If the RCP client is allowed to send data to the serial interface, the reply will present an OK. If the RCP client is not allowed to send data, a FAIL will be returned. In this case another RCP client is controlling the serial out. The timeout and priority handling of the serial ports is beyond the scope of this document.
NOTE: This command is NOT readable.
Write reply packet

16 | 32
Code 1 Byte | Reserved 1 Byte | Reserved 2 Bytes
8 | 24 |

Code
Values:

Access to the serial port denied |  | 0x00
Access to the serial port granted |  | 0x01

Reading the TRANSFER_TRANSPARENT_DATA command
The reply to the Read command will be the same as the reply to the write command. The returned code will present the availability of the serial port.
NOTE: Despite a positive reply to a read command, the port may be locked by another RCP client in the time slice between the read and a following write command.
Serial IN -> RCP Client
The data coming from the serial input is delivered using an RCP message. All RCP clients which want to receive this data must be registered for the message 0xFFDD. Data is posted if the corresponding RCP client is in control only.
If no client has a lease on the serial port, a message to all registered clients will be generated.
NOTE: The received message will carry NO header.
CONF_CONNECT_PRIMITIVE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xff0c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | l_live |  | % |
| Write |  | p_octet |  | l_live |  | see detailed description |

Switching Media Channels
Each RCP client may have different media sources and media receivers. To connect these media channels, a low level connect/disconnect primitive is implemented. These low level primitives can be grouped together to more complex commands, which can connect more than one media channel at the same time.
The primitives are designed to be asserted by media sources or receivers itself. Manager software should use the high level commands (see next chapter).
Using GET
By sending a CONNECT GET to the remote endpoint, this endpoint will start sending media to the requested address. For example, a VideoJet receiver is registered at a VideoJet transmitter. On sending a ‘CONNECT GET video to port 1234’ to the transmitter, the transmitter starts to send video to the appropriate port at the receiver.
The endpoint requesting the media stream (the VideoJet receiver) must be prepared to receive the stream from the network.
The coding (and resolution bits for video) must b e set according to the receivers capability to decode the data stream). E.g. a Decoder capable of decoding MPEG2 and MPEG4 in QCIF, CIF and 4CIF resolution should set all these bits.
Using PUT
By sending a CONNECT PUT to the remote endpoint, the endpoint will prepare itself for receiving data from the one initiating the request. For example, a VideoJet transmitter is registered at a VideoJet receiver. On sending a ‘CONNECT PUT video to port 2222’ to the receiver, the receiver will prepare its network stack to receive data from the appropriate port.
The endpoint initiating the media stream (the VideoJet transmitter) must start sending the media stream to the network.
The coding (and resolution bits for video) must be set to a value suitable to the current encoding parameters inside the VideoJet. E.g. if a video encoder is set to encode MPEG4 in CIF mode, only a PUT request having these bits set is accepted.
The coder parameter is used to address a specific encoder/decoder inside the VideoJet. As the VideoJet may have a Dual-stream feature, one physical line input might be connected to more than one encoder. By setting a coder to another value than 0, the VideoJet only tries this specific coder to establish a connection. When the coder value is set to 0, all coders inside the system will be checked.
Each connect primitive will result in a Session ID for maintaining and controlling the media stream with other RCP commands. The Session ID can be treated as unique on the entire system.
DISCONNECT
By sending a DISCONNECT supplied with a valid Session ID, the receiver of the command will stop sending/receiving to/from the media stream. The endpoint initiating the DISCONNECT command must stop receiving/sending from/to the media stream.
Request Packet
Sequence of:

Method 1 Byte | Media 1 Byte | Reserved 1 Byte | Flags 1 Byte
Reserved 4 Bytes
Media Descriptor 1 M Bytes (Length depends on Media type)
N x M Bytes | Media Descriptor N M Bytes ...

Method
Values:

GET |  | 0x00
PUT |  | 0x01
Key transport |  | 0xE0

Media
Values:

Video |  | 0x01
Audio |  | 0x02
Data |  | 0x03

Flags
Bit1: Do reverse Login. This will control whether the called server will perform a reverse RCP Login.
Bit2: Free Running Connection. When this bit is set, the connection is not needed to retrigger by the command CONF_RCP_CONNECTIONS_ALIVE.
Bit3: Optional signalling for streaming (for correct connection list display)
Bit3: Media key request (when using GET) / Media key is appended at the end of this section (when using PUT)
Media Descriptors 1 - N

Video |  |
16 | 32
MEP 1 Byte | Flags 1 Byte | MTA Port 2 Bytes
MTA IP Address 4 Bytes
Coder 1 Byte | Line 1 Byte | MCTA Port 2 Bytes
MCTA IP Address 4 Bytes
Coding 2 Bytes | Resolution 2 Bytes
Linked Coder 1 Bytes | Linked Line 1 Bytes | Bandwidth 2 Bytes
8 | 24 |
MEP Media Encapsulation Protocol. Values:
RTP over UDP |  | 0x01
RTP over TCP |  | 0x04
notice: when using RTP over TCP, media channels must be established as described in 'RCP Protocol Procedure / Receiving media data' Flags Values:
Bit1 |  | Substitute connection (if an RX connection to the requested interface is already established, the old connection will be disconnected and substituted by a new connection coming with this request).
Bit2 |  | Use relative to line coder addressing.
MTA Port Media Transport Address - Network port. MTA IP Address Media Transport Address IP Address Values:
VideoJet will take address from the incoming TCP header |  | 0.0.0.0
VideoJet will take its configured multicast group IP |  | 224.0.0.0
Coder Specifies the internal coder number; when set to 0, the appropriate coder corresponding to the given line number and/or coding parameter is chosen by the VideoJet itself. Line Identifies the Line Input/Output channel for the specified coding engine. MCTA Port Media Control Transport Address Network Port. Currently unused. MCTA IP Address Media Control Transport Address IP Address. Currently unused. Coding Values:
Bit3 |  | MPEG-4 (elementary stream)
Bit4 |  | MPEG-2 (only video)
Bit5 |  | Meta Data (output from motion detector…)
Bit7 |  | H264
Bit8 |  | JPEG
Bit15 |  | Recorded Media
Bit16 |  | MPEG-2 (program stream)
Resolution Values:
Bit1 |  | QCIF
Bit2 |  | CIF
Bit3 |  | 2CIF
Bit4 |  | 4CIF
Linked Coder Use this field for signalling the callers local coder in the connection list of the called device. Linked Line Use this field for signalling the callers local line in the connection list of the called device. Bandwidth Initial bandwidth request in kBit/s Must have an value > 0. Only used on VJX00 series.
Audio |  |
16 | 32
MEP 1 Byte | Flags 1 Byte | MTA Port 2 Bytes
MTA IP Address 4 Bytes
Coder 1 Byte | Line 1 Byte | MCTA Port 2 Bytes
MCTA IP Address 4 Bytes
Coding 2 Bytes | Reserved 2 Bytes
Linked Coder 1 Bytes | Linked Line 1 Bytes | Reserved 2 Bytes
8 | 24 |
MEP Media Encapsulation Protocol. Values:
RTP over UDP |  | 0x01
RTP over TCP |  | 0x04
Flags Values:
Bit1 |  | Substitute connection (if an RX connection to the requested interface is already established, the old connection will be disconnected and substituted by a new connection coming with this request).
Bit2 |  | Use relative to line coder addressing.
MTA Port Media Transport Address - Network port. MTA IP Address Media Transport Address IP Address Values:
VideoJet will take address from the incoming TCP header |  | 0.0.0.0
VideoJet will take its configured multicast group IP |  | 224.0.0.0
Coder Specifies the internal coder number; when set to 0, the appropriate coder corresponding to the given line number and/or coding parameter is chosen by the VideoJet itself. Line Identifies the Line Input/Output channel for the specified coding engine. MCTA Port Media Control Transport Address Network Port. Currently unused. MCTA IP Address Media Control Transport Address IP Address. Currently unused. Coding Values:
Bit1 |  | G.711
Bit15 |  | Recorded Media
Bit16 |  | MPEG-2 (program stream)
Linked Coder Use this field for signalling the callers local coder in the connection list of the called device. Linked Line Use this field for signalling the callers local line in the connection list of the called device.
Data |  |
16 | 32
MEP 1 Byte | Reserved 1 Byte | Reserved 2 Bytes
MTA IP Address 4 Bytes
Coder 1 Byte | Line 1 Byte | Reserved 2 Bytes
Reserved 4 Bytes
Coding 2 Bytes | Reserved 2 Bytes
Linked Coder 1 Bytes | Linked Line 1 Bytes | Reserved 2 Bytes
8 | 24 |
MEP Media Encapsulation Protocol. Values:
RCP Intrinsic |  | 0x02
MTA IP Address Media Transport Address IP Address Values:
VideoJet will take address from the incoming TCP header |  | 0.0.0.0
Coder Informational. Line Identifies the Line Input/Output channel for the specified coding engine. Coding Values:
Bit1 |  | RCP
Bit15 |  | Recorded Media
Linked Coder Use this field for signalling the callers local coder in the connection list of the called device. Linked Line Use this field for signalling the callers local line in the connection list of the called device.
Span Replay |  |
16 | 32
MEP 1 Byte | Reserved 1 Byte | Media Handle 2 Byte
iSCSI Server IP 4 Bytes
Coder 1 Byte | Line 1 Byte | Reserved 2 Byte
Target Idx 1 Byte | Lun Idx 1 Byte | Span Idx 2 Byte
Coding 2 Byte | Resolution 2 Byte
Reserved 2 Byte | Bandwidth 2 Byte
8 | 24 |
MEP Media Encapsulation Protocol. Values:
API Callback |  | 0x06
Media Handle Identifier that is associated with the rtp data and is supplied with the rtp data in the callback function. iSCSI Server IP The IP address of the iSCSI server. Use 0xFFFFFFFF to connect to a span on a usb device that is locally connected to the device. Coder Specifies the internal coder number; when set to 0, the appropriate coder corresponding to the given line number and/or coding parameter is chosen by the VideoJet itself. Line Identifies the Line Input/Output channel for the specified coding engine. Target Idx The index of the target on the iSCSI Server. This index can be obtained by sending a disconver to the server. Lun Idx The index of the Lun of the specified target on the iscsi server. Span Idx The index of the span. Coding Values:
Bit15 |  | Recorded Media
Resolution Values:
Bit1 |  | QCIF
Bit2 |  | CIF
Bit3 |  | 2CIF
Bit4 |  | 4CIF
Bandwidth Initial bandwidth request in kBit/s Must have an value > 0. Only used on VJX00 series. NOTE: If this command is used with the vj api, an specific error of the following type may be returned
SPAN_ERR_INTERNAL |  | 0x01
SPAN_ERR_INV_SPN_IDX |  | 0x02
SPAN_ERR_INV_HDR_TYPE |  | 0x03
SPAN_ERR_NOT_MNTD |  | 0x05
SPAN_ERR_INV_FS |  | 0x06
SPAN_ERR_INV_LUN_NFO |  | 0x07
SPAN_ERR_BAD_HDR_CKSM |  | 0x08
SPAN_ERR_RD_ONLY |  | 0x0a
SPAN_ERR_NO_REC_DAT |  | 0x0b
SPAN_ERROR_INV_PART_NFO |  | 0x0c
ISCSI_ERROR_CONNECT |  | 0x31
ISCSI_ERROR_INV_LUN |  | 0x33
ISCSI_ERROR_LOGIN |  | 0x34
ISCSI_ERROR_INV_TRG_IDX |  | 0x35

Key transport
When the media key bit is selected in the header flags, a variable length key field is appended at the end of the media descriptor. The key field has the following structure

Sequence of:
16 | 32
method 1 Byte | bytes valid 1 Byte | status tag 1 Byte | reserved 1 Byte
key data 4 Bytes
8 | 24 |
method must be set to 'Key transport' 0xE0 bytes valid the number of valid key bytes in this header status tag must be set to 'Key transport tag' 0xE0 key data the key payload

The media key is transferred using a sequence of key headers all with the method field set to 0xE0. The end of the key section is marked by a header with less than 4 bytes (or zero) indicated in the bytes valid field.
The typical key length is 16 bytes (128 bit AES). In this case, four full key headers followed by one empty header must be transferred (4 x 4 bytes valid + 1 x 0 bytes valid = 16 bytes)
For backward compatibility, the header method 0xE0 will be skipped by units with former firmwares versions.
The key is located and stored on each media source (using the CONF_CRYPT_KEY* commands); When the system is configured to publish its keys (see CONF_PUBLISH_MEDIA_KEYS), then the media sources must fill in the secret by sending (PUT method) or replying to (GET method) the connect primitive.
For example, when sending a GET connect primitive to a device and the key transport is selected, then the device will fill in its key in the reply to the connect primitive.
NOTE: be sure to use a secure RCP connection, the keys in the connect primitive are tranferred in plain
Reply Packet
Sequence of:

Method 1 Byte | Media 1 Byte | Status 1 Byte | Reserved 1 Byte
Reserved 4 Bytes
Media Descriptor 1 M Bytes (Length depends on Media type)
N x M Bytes | Media Descriptor N M Bytes ...

Method
Values:

GET |  | 0x00
PUT |  | 0x01

Media
Values:

Video |  | 0x01
Audio |  | 0x02
data |  | 0x03

Status
Values:

Interface not available (Remark: former version may return this error in case of unknown method/media type) |  | 0x00
Access to this interface granted |  | 0x01
Access to this interface rejected |  | 0x02
Session ID invalid or connection no longer active |  | 0x03
Coding parameters incompatible |  | 0x04
Interface data will be supplied by another media descriptor |  | 0x05
The method field in the header does not carry a known method |  | 0x08
The media field in the header does not carry a known media type |  | 0x09

NOTE: Any wildcards used in the transport addresses will be replaced by the real used network addresses.
This command is NOT readable; to gain information on active connection refer to the ACTIVE_CONNECTION_LIST command.
NOTE: The Media Control sockets have currently no function
CONF_DISCONNECT_PRIMITIVE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xff0d |  | no |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | l_live |  | % |
| Write |  | p_octet |  | l_live |  | see detailed description |

Payload Structure

16 | 32
Status 1 Byte | Cause 1 Byte | Reserved 2 Bytes
Remote Host IP 4 Bytes
8 | 24 |

Status
Values:

Connection disconnected |  | 0x01
Connection identified by the given Session ID not found on this host |  | 0x02

Cause
Values:

Not closed |  | 0x00
Normal termination |  | 0x01
Abnormal termination |  | 0x02
No response |  | 0x03
Remote host terminated |  | 0x04
Timed out |  | 0x05
Remote login rejected |  | 0x06
No common media channels |  | 0x07
Connection substituted |  | 0x08
Automatic disconnect |  | 0x09
Stop streaming |  | 0x0a

Remote Host IP
IP address of the remote connected host.
NOTE: This command is NOT readable.
CONF_CONNECT_TO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xffcc |  | no |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | l_live |  | % |
| Write |  | p_octet |  | l_live |  | see detailed description |

Write Packet

16 | 32
Destination IP Address 4 Bytes
Reserved 1 Byte | Line 1 Byte | Flags 2 Bytes
Local Coder 1 Byte | Local Line 1 Byte | Put Channels 2 Bytes
Remote Coder 1 Byte | Remote Line 1 Byte | Get Channels 2 Bytes
8 | 24 |

Destination IP Address
The reception of this command will force the host to connect to the mentioned destination IP address.
Line
OBSOLETE
This parameter carries the number of the remote input (for get channels) or the local input (for put channels); For connection to the HDD, the Line byte must carry the partition number of the HD.
This parameter is updated by the local line/coder and remote line/coder settings.
Flags
NOTE: Only one video standard (MPEG2/4) can be used; setting all bits will result in best currently available mode.
Values:

Bit0 |  | Substitute an existing connection
Bit1 |  | Request video mode MPEG-4
Bit2 |  | Request video mode MPEG-2
Bit3 |  | Force the use of TCP as transportation protocol
Bit4 |  | Connect to the HDD to receive a recorded media stream
Bit6 |  | Connect a VCA meta data stream
Bit7 |  | Supress automatic media key exchange
Bit8 |  | Use SSL for the RCP control connection; if no destination port is specified, the remote port defaults to 443 (HTTPS) in case of SSL is requested otherwise 80(HTTP)
Bit9 |  | Request video mode H.264
Bit10 |  | Request video mode JPEG

Local Coder
This parameter carries the number of the local video input number. A wildcard of ‘0’ will result in first match.
Local Line
This parameter carries the number of the local video coder number. A wildcard of ‘0’ will result in first match.
Put Channels
Values:

Bit0 |  | Video
Bit1 |  | Audio
Bit2 |  | Data
Bit3-Bit15 |  | Reserved

Remote Coder
This parameter carries the number of the remote video coder number (at the destination IP). A wildcard of ‘0’ will result in first match.
Remote Line
This parameter carries the number of the remote video coder number (at the destination IP). A wildcard of ‘0’ will result in first match.
Get Channels
Values:

Bit0 |  | Video
Bit1 |  | Audio
Bit2 |  | Data
Bit3-Bit15 |  | Reserved

NOTE: For audio connections, the local and remote line parameter are taken from the video settings.
If this command is extended with the optional appendix, the remote port number for RCP login must be specified. This can be either 1756 for the normal RCP port or any available HTTP port at the remote host. When a port number different to 1756 is used, the login will use a HTTP tunnelling.
Optional Appendix

16 | 32
Dest. Port 2 Bytes | Reserved 2 Bytes
Reserved 4 Bytes
8 | 24 |

Dest. Port
This parameter carries the number of the remote TCP port number used for RCP login.
Reply / Read / Message
The reply to this command will present the same packet format as the outgoing. The result will contain the really established channels.
A message will be generated if all requested channels are established; if a channel fails, the appropriate bit will be cleared in the channel section.
CONF_ACTIVE_CONNECTION_LIST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xffc1 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | l_user |  | see detailed description |
| Write |  | % |  | l_user |  | % |

Payload Structure
Sequence of:

16 | 32
Destination IP Address 4 Bytes
Local Coder 1 Byte | Local Line 1 Byte | Flags 2 Bytes
Session ID 4 Bytes
Remote Coder 1 Byte | Remote Line 1 Byte | Reserved 2 Bytes
TX Channels 4 Bytes
RX Channels 4 Bytes
8 | 24 |

Destination IP Address
IP address to which the unit is connected.
Local Coder
The local connected coder (relative to line).
Local Line
The remote connected line
Flags
Values:

Bit0 |  | Connection is MPEG2 VES
Bit1 |  | Connection is MPEG2 PRG
Bit2 |  | Connection is MPEG4
Bit3 |  | Connection is to HDD replay
Bit4 |  | Connection is started as streaming
Bit5 |  | Connection is using multicast
Bit6 |  | Connection is using TCP for transportation
Bit7 |  | Data stream is encrypted
Bit8 |  | Connection is H.264
Bit9 |  | Connection is Jpeg

Session ID
Session identifier.
Remote Coder
The remote connected coder (relative to line).
Remote Line
The remote connected line.
TX Channels
See CONNECT_TO command for bit mask.
RX Channels
See CONNECT_TO command for bit mask.
CONF_MEDIA_SOCKETS_COMPLETE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xffc7 |  | - |  | yes (Message only) |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | l_user |  | % |
| Write |  | - |  | l_user |  | sends out a message when all TCP tunneled sockets of a session are connected |

CONF_RCP_CONNECTIONS_ALIVE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xffc2 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | l_live |  | retriggers a running connection identified by its session_id; returns the current number of active connections |
| Write |  | % |  | l_live |  | % |

CONF_CAPABILITY_LIST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xff10 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | % |  | noprot |  | % |

Reply payload Structure

0xBABA 2 Bytes | Version 2 Bytes | NbSection 2 Bytes | Section 1 | ... | Section N

Version
current version of the capabilities (0x0001)
NbSection
Number of following sections
Section Structure

Type 2 Bytes | Size 2 Bytes | NbElement 2 Bytes | Element 1 | ... | Element N

Type
Type of Element
Values:

Video |  | 0x0001
Audio |  | 0x0002
Serial |  | 0x0003
IO |  | 0x0004
Camera Data |  | 0x0005

Size
Size of the section including SectionType, Size and NbElement. If the section is unknown, you can skip to the next using the size
NbElement
determines how many Elements are following. The definition of each Element depends on the type of the section
Element Structure
For section type Video

Type 2 Bytes | Identifier 2 Bytes | Compr 2 Bytes | InputNo 2 Bytes | Resolution 2 Bytes |

Type
is one of the following
Values:

VIDEO_ENCODER |  | 0x0001
VIDEO_DECODER |  | 0x0002

Identifier
Identifier is the RCP numeric descriptor to use to address the entity. It should be unique when associated with the type and the compression.
Compression
is one or multiple of the following
Values:

VIDEO_COMP_MPEG2 |  | 0x0001
VIDEO_COMP_MPEG4 |  | 0x0002
VIDEO_COMP_H264 |  | 0x0004
VIDEO_COMP_JPEG |  | 0x0008

InputNo
InputNo is the number of the physical input from which the entity gets or puts its video
Resolution
is one or multiple of the following
Values:

VIDEO_RESO_QCIF |  | 0x0001
VIDEO_RESO_CIF |  | 0x0002
VIDEO_RESO_2CIF |  | 0x0004
VIDEO_RESO_4CIF |  | 0x0008
VIDEO_RESO_CUSTOM |  | 0x0010

Element Structure
For section type Audio

Type 2 Bytes | Identifier 2 Bytes | Compr 2 Bytes |

Type
is one of the following
Values:

AUDIO_ENCODER |  | 0x0001
AUDIO_DECODER |  | 0x0002

Identifier
Identifier is the RCP numeric descriptor to use to address the entity. It should be unique when associated with the type and the compression.
Compression
is one or multiple of the following
Values:

AUDIO_COMP_MPEG2 |  | 0x0001
AUDIO_COMP_G711 |  | 0x0002

Element Structure
For section type Serial

Type 2 Bytes | Identifier 2 Bytes |

Type
is one of the following
Values:

SERIAL_RS232 |  | 0x0001
SERIAL_RS485 |  | 0x0002
SERIAL_RS422 |  | 0x0004

Identifier
is the RCP numeric descriptor to use to address the entity.
Element Structure
For section type IO

Type 2 Bytes | Identifier 2 Bytes |

Type
is one of the following
Values:

IO_INPUT |  | 0x0001
IO_OUTPUT |  | 0x0002
IO_VIRTUAL_IN |  | 0x0003

Identifier
is the RCP numeric descriptor to use to address the entity.
Element Structure
For section type Camera Data

Type 2 Bytes | InputNo 2 Bytes |

Type
is one of the following
Values:

CAMDATA_BILINX |  | 0x0001

InputNo
InputNo is the number of the physical video input.
CONF_RCP_CODER_LIST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0xff11 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | % |  | noprot |  | % |

This command is used to retrieve the list of encoders and decoders from a VideoJet. There are two reply formats supported, the compact and the extended list view. The compact view only reports the absolute coder numbers available on a given line input or output. The extended view offers more information about coding capabilities and other parameters of a coder.
Request payload Structure

16 |
MediaType 1 Byte | Direction 1 Byte | Flags 1 Byte |
8 | 24 |

MediaType
Values:

Video |  | 0x01
Audio |  | 0x02
Data |  | 0x03

Direction
physical port is
Values:

Input |  | 0x00
Output |  | 0x01

Flags
one or multiple of
Values:

Request compact format |  | 0x00
Reqeust extended format list |  | 0x01

Compact format reply payload Structure

CoderNbr 1 1 Byte | N x 1 Byte | CoderNbr N 1 Byte |

CoderNbr 1 - N
List of the absolute coder numbers
Extended format video reply payload structure
Sequence of

16 | 32
CodingNbr 2 Byte | Coding Capabilities 2 Byte
Coding Current 2 Byte | Resolution Capabilities 2 Byte
Resolution Current 2 Byte | Reserved 2 Byte
Reserved 4 Byte
8 | 24 |

CoderNbr
The absolute coder number
Coding Capabilities
All coding capabilities is one or multiple of
Values:

H.263 |  | 0x0002
Mpeg4 |  | 0x0004
Mpeg2 |  | 0x0008
Meta Data |  | 0x0010
H.263-1998 |  | 0x0020
Recorded Media |  | 0x4000
Mpeg2 PrgStr |  | 0x8000

Coding Current
The current available coding capabilities (definitions see above)
Resolution Capabilities
All resolution capabilities is one or multiple of
Values:

QCIF |  | 0x0001
CIF |  | 0x0002
2CIF |  | 0x0004
4CIF |  | 0x0008
Custom |  | 0x0010

Resolution Current
The current available resolution capabilities (definitions see above)
Extended format audio reply payload structure
Sequence of

16 | 32
CodingNbr 2 Byte | Coding Capabilities 2 Byte
Coding Current 2 Byte | CodParameter Capabilities 2 Byte
CodParameter Current 2 Byte | Reserved 2 Byte
Reserved 4 Byte
8 | 24 |

CoderNbr
The absolute coder number
Coding Capabilities
All coding capabilities is one or multiple of
Values:

G.711 |  | 0x0001
Mpeg2 PrgStr |  | 0x8000

Coding Current
The current available coding capabilities (definitions see above)
Extended format data reply payload structure
Sequence of

16 | 32
CodingNbr 2 Byte | Coding Capabilities 2 Byte
Coding Current 2 Byte | CodParameter Capabilities 2 Byte
CodParameter Current 2 Byte | Reserved 2 Byte
Reserved 4 Byte
8 | 24 |

CoderNbr
The absolute coder number
Coding Capabilities
All coding capabilities is one or multiple of
Values:

RCP |  | 0x0001

Coding Current
The current available coding capabilities (definitions see above)
CodParameter Capabilities
All coding CodParameter capabilities is one or multiple of
Values:

RS232 |  | 0x0001
RS485 |  | 0x0002
RS422 |  | 0x0004

CodParameter Current
The current available coding capabilities (definitions see above)
CONF_PUBLISH_MEDIA_KEYS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09fc |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | switches wheather the media key of a media source are readable and transferred during the hw-hw connection setup |
| Write |  | f_flag |  | l_serv |  | switches wheather the media key of a media source are readable and transferred during the hw-hw connection setup |

CONF_CRYPT_KEYAUDIO_ENC

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09fe |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | l_serv |  | set key for AES Audio data encryption/decryption |
| Write |  | p_octet |  | l_serv |  | set key for AES encryption/decryption of audio data see detailed description |

Payload Structure

16 | 32
Key 16 Bytes ...
8 | 24 |

Key
The 16 Byte Masterkey for AES encryption/decryption of data
Comments:

- This description is valid for the the commands:
  CONF_CRYPT_KEYVIDEO_ENC,
  CONF_CRYPT_KEYVIDEO_DEC,
  CONF_CRYPT_KEYAUDIO_ENC,
  CONF_CRYPT_KEYAUDIO_DEC
- The numeric descriptor contains the number of the coder instance (absolute)
- Set all Key- and all Salt- Bytes to zero, if no encryption/decryption is wished.

CONF_CRYPT_KEYVIDEO_ENC

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ed |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | l_serv |  | set key for AES Video dataencryption/decryption |
| Write |  | p_octet |  | l_serv |  | set key for AES encryption/decryption of video data see detailed description |

Payload Structure

16 | 32
Key 16 Bytes ...
8 | 24 |

Key
The 16 Byte Masterkey for AES encryption/decryption of data
Comments:

- This description is valid for the the commands:
  CONF_CRYPT_KEYVIDEO_ENC,
  CONF_CRYPT_KEYVIDEO_DEC,
  CONF_CRYPT_KEYAUDIO_ENC,
  CONF_CRYPT_KEYAUDIO_DEC
- The numeric descriptor contains the number of the coder instance (absolute)
- Set all Key- and all Salt- Bytes to zero, if no encryption/decryption is wished.

CONF_CRYPT_KEYAUDIO_DEC

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ff |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | l_serv |  | set key for AES Audio data encryption/decryption |
| Write |  | p_octet |  | l_serv |  | set key for AES encryption/decryption of audio data see detailed description |

Payload Structure

16 | 32
Key 16 Bytes ...
8 | 24 |

Key
The 16 Byte Masterkey for AES encryption/decryption of data
Comments:

- This description is valid for the the commands:
  CONF_CRYPT_KEYVIDEO_ENC,
  CONF_CRYPT_KEYVIDEO_DEC,
  CONF_CRYPT_KEYAUDIO_ENC,
  CONF_CRYPT_KEYAUDIO_DEC
- The numeric descriptor contains the number of the coder instance (absolute)
- Set all Key- and all Salt- Bytes to zero, if no encryption/decryption is wished.

CONF_CRYPT_KEYVIDEO_DEC

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a00 |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | l_serv |  | set key for AES Video dataencryption/decryption |
| Write |  | p_octet |  | l_serv |  | set key for AES encryption/decryption of video data see detailed description |

Payload Structure

16 | 32
Key 16 Bytes ...
8 | 24 |

Key
The 16 Byte Masterkey for AES encryption/decryption of data
Comments:

- This description is valid for the the commands:
  CONF_CRYPT_KEYVIDEO_ENC,
  CONF_CRYPT_KEYVIDEO_DEC,
  CONF_CRYPT_KEYAUDIO_ENC,
  CONF_CRYPT_KEYAUDIO_DEC
- The numeric descriptor contains the number of the coder instance (absolute)
- Set all Key- and all Salt- Bytes to zero, if no encryption/decryption is wished.

CONF_CRYPT_KEY_GENERATE_ALL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a13 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | returns flag=0 when all key are cleared otherwise flag=1 |
| Write |  | f_flag |  | l_serv |  | generates a random key(flag=1) or clears all(flag=0) keys for AES encryption for all media encoders |

CONF_UNIT_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0024 |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | read the unit name |
| Write |  | p_unicode (max 32 unicode character) |  | l_serv |  | set unit name |

CONF_UNIT_ID

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0025 |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | read the unit ID |
| Write |  | p_unicode (max 32 unicode character) |  | l_serv |  | set unit ID |

CONF_CAMNAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0019 |  | video line |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | read the camera name |
| Write |  | p_unicode (max 32 unicode characters) |  | l_serv |  | set the camera name |

CONF_CAMNAME2

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a7e |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | read the camera name2 |
| Write |  | p_unicode (max 32 unicode characters) |  | l_serv |  | set the camera name2 |

CONF_HARDWARE_VERSION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x002e |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the hardware version |
| Write |  | void |  | noprot |  | not supported |

CONF_SOFTWARE_VERSION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x002f |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the software version |
| Write |  | void |  | noprot |  | not supported |

CONF_BOOTLOADER_VERSION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ef |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | read the bootloader version |
| Write |  | t_dword |  | noprot |  | not supported |

CONF_STARTPAGE_BACKGROUND_URL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x028d |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | get the URL of the startpage' background image (max 64 char) |
| Write |  | p_string |  | l_serv |  | set the URL of the startpage' background image (max 64 char) |

CONF_STARTPAGE_LOGO_URL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x028e |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | get the URL of the startpage' OEM logo image (max 64 char) |
| Write |  | p_string |  | l_serv |  | set the URL of the startpage' OEM logo image (max 64 char) |

CONF_STARTPAGE_PRESENTATION_SWITCHES

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x028f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get switches for HTML startpage presentation (usage is up the the user) |
| Write |  | t_dword |  | l_serv |  | set switches for HTML startpage presentation (usage is up the the user) |

CONF_DYNAMIC_HTML_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0298 |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | get the name for a dynamic HTML page (num range 1..4) |
| Write |  | p_string |  | l_user |  | set the name for a dynamic HTML page (num range 1..4) (max. 19 char) |

CONF_DYNAMIC_HTML_DATA

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0299 |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | set the data(content) for a dynamic HTML page (num range 1..4) (max. 2048 char) |
| Write |  | p_octet |  | l_user |  | set the data(content) for a dynamic HTML page (num range 1..4) (max. 2048 char) |

CONF_BROWSER_LANGUAGE_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01e3 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | read current set browser language |
| Write |  | t_octet |  | l_serv |  | set browser language (numbering depends on toolkit implementation) |

CONF_BROWSER_DATETIME_FORMAT_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01e9 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | read browser date/time format |
| Write |  | t_octet |  | l_serv |  | set browser date/time format (1=Europe, 2=USA, 3=Japan) |

CONF_DATE_WDAY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0027 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | "Sunday" ... "Saturday"; read the weekday according to the systems date setting |
| Write |  | void |  | l_serv |  | not supported |

CONF_DATE_DAY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0028 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet or p_string (2 chars length) |  | noprot |  | read the day of week |
| Write |  | t_octet |  | l_serv |  | set the day of week, not supported while recording is running |

CONF_DATE_MONTH

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0029 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet and p_string (2 chars length) |  | noprot |  | read the month |
| Write |  | t_octet |  | l_serv |  | set the month, not supported while recording is running |

CONF_DATE_YEAR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x002a |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word and p_string (4 chars length) |  | noprot |  | read the year |
| Write |  | t_word |  | l_serv |  | xx set the year; century needed, not supported while recording is running |

CONF_TIME_HRS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x002d |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet and p_string (2 chars length) |  | noprot |  | read the hours |
| Write |  | t_octet |  | l_serv |  | set the hours, not supported while recording is running |

CONF_TIME_MIN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x002c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet and p_string (2 chars length) |  | noprot |  | read the minutes |
| Write |  | t_octet |  | l_serv |  | set the minutes, not supported while recording is running |

CONF_TIME_SEC

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x002b |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet and p_string (2 chars length) |  | noprot |  | read the seconds |
| Write |  | t_octet |  | l_serv |  | set the seconds, not supported while recording is running |

CONF_TIMEZONE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x024e |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_int |  | noprot |  | the timezone in which the unit has to operate (GMT +- nbr of seconds +- nbr of seconds DLS), read only version 2.50 |
| Write |  | t_int |  | l_serv |  | the timezone in which the unit has to operate (GMT +- nbr of seconds +- nbr of seconds DLS), read only since version 2.50 |

CONF_UTC_ZONEOFFSET

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x031f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_int |  | noprot |  | the timezone in which the unit has to operate (GMT +- nbr of seconds) |
| Write |  | t_int |  | l_serv |  | the timezone in which the unit has to operate (GMT +- nbr of seconds) |

CONF_NTP_SERVER_IP_STR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x024f |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | reads the time servers ip address in "xxx.xxx.xxx.xxx" used to sync time from |
| Write |  | p_string |  | l_serv |  | sets the server ip in "xxx.xxx.xxx.xxx" to sync time from, not supported while recording is running |

CONF_DAY_LIGHT_SAVE_TIME_TABLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0987 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read 20 entries for daylight save time: UTC time in sec since 2000 (4byte) and associated offset in sec (4 signed bytes), unused entries have to be filled with zero |
| Write |  | p_octet |  | l_serv |  | write 20 entries for daylight save time: UTC time in sec since 2000 (4byte) and associated offset in sec (4 signed bytes), unused entries have to be filled with zero |

CONF_DAY_LIGHT_SAVE_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0988 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_int |  | noprot |  | read the currently used day light save time offset in seconds |
| Write |  | t_int |  | l_serv |  | write the day light save time offset in seconds; the device updates this from DAY_LIGHT_SAVE_TIME_TABLE to show current offset used |

CONF_FORCE_TIME_SET

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a0f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read the time, 8 bytes payload, offset 0: year (word); offset 2: month (octet); offset 3: day (octet); offset 4: hrs (octet); offset 5: min (octet); offset 6: sec (octet); offset 7: reserved (octet) |
| Write |  | p_octet |  | l_serv |  | set the time, if recording is running it will be stopped and restarted, parameter 8 bytes payload, offset 0: year (word); offset 2: month (octet); offset 3: day (octet); offset 4: hrs (octet); offset 5: min (octet); offset 6: sec (octet); offset 7: reserved (octet) |

CONF_PASSWORD_SETTINGS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x028b |  | password level |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | l_serv |  | get the unit password (scrambled). num parameter sets the password levels; 1=user, 2=service, 3=live |
| Write |  | p_string |  | l_serv |  | set the unit password. num parameter sets the password levels; 1=user, 2=service, 3=live |

CONF_REMOTE_PASSWORD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x010c |  | destination IP number |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | void |  | noprot |  | not supported |
| Write |  | p_string |  | l_serv |  | deposit the password of the called station |

CONF_MASTERPWD_CHALLENGE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x013f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | generates an password challenge which has to be passed to the operator for password reset |
| Write |  | p_string |  | noprot |  | not supported |

CONF_NBR_OF_TEMP_SENS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09c4 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | l_user |  | the number of temperature sensors |
| Write |  | t_dword |  | noprot |  | not supported |

CONF_TEMP_SENS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09c5 |  | temperature sensor |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | l_user |  | value of the temperature sensor specified by numdes |
| Write |  | t_dword |  | noprot |  | not supported |

CONF_REDUNDANT_POWER

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d7 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | l_user |  | reads the redundant power settings 0=off, 1=on |
| Write |  | t_dword |  | l_serv |  | sets the redundant power 0=off, 1=on |

CONF_POWER_SUPPLY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09dd |  | no |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | l_user |  | bit field of power supplies (supply n: supplybits = 1<<(n-1)) |
| Write |  | t_dword |  | l_serv |  | bit field of power supplies (supply n: supplybits = 1<<(n-1)) |

CONF_NBR_OF_FANS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d5 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | l_user |  | reads the number of fans |
| Write |  | t_dword |  | l_serv |  | not supported |

CONF_FAN_SPEED

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d6 |  | fan number |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | l_user |  | fan speed in RPM |
| Write |  | t_dword |  | l_serv |  | not supported |

CONF_MINIMUM_FAN_SPEED

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09de |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | l_user |  | minimum fan speed in RPM |
| Write |  | t_dword |  | l_serv |  | minimum fan speed in RPM |

CONF_BOOT_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e3 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | l_user |  | 100 if booted |
| Write |  | t_dword |  | l_serv |  | not supported |

CONF_UPLOAD_PROGRESS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0701 |  | - |  | yes (Message only) |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | noprot |  | % |
| Write |  | - |  | noprot |  | see detailed description |

Payload Structure

Progress 1 Byte |
8 |

Progress
informs about current progress of an upload or possible error states
Values

progress in percent |  | 1 ... 100
header error |  | 101
write error |  | 102
read back error |  | 103
verify error |  | 104
checksum mismatch (read back flash content vs. written data) |  | 105
checksum mismatch (announced in header vs. received data) |  | 106
magic error |  | 110
version too low |  | 111
flash type incompatible |  | 112
device check failed |  | 113
file entry marker failed |  | 114
chunk size error |  | 115
invalid file name |  | 130
ROM init error |  | 131
ROM write error |  | 132
ROM close error |  | 133
socket error |  | 134
overflow error |  | 135
final flush error |  | 136

Values in the range of 1 ... 100 represent the upload progress in percent. Other values need to be handled as error during the upload and inform about the kind of the error that was encountered during the upload.
CONF_VIPROC_ID

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0803 |  | video line |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the viproc interface id (0:= no viproc) |
| Write |  | t_dword |  | l_serv |  | not supported |

CONF_VIPROC_ONOFF

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0800 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | reads the VCA status 0=off, 1=on. command is obsolete with firmware 4.0 and replaced by VIPROC_MODE. |
| Write |  | flag |  | l_serv |  | switches on/off the video content analysis (VCA). command is obsolete with firmware 4.0 and replaced by VIPROC_MODE. |

CONF_VIPROC_CUSTOM_PARAMETERS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0802 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | reads the video content analysis (VCA) custom parameters, payload is beyond the scope of this document |
| Write |  | p_octet |  | l_serv |  | sets the VCA custom parameters, payload is beyond the scope of this document |

CONF_VIPROC_DLL_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0804 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | reads the name of currently selected VCA component |
| Write |  | p_string |  | l_serv |  | specify the name of the VCA component |

CONF_VIPROC_DLL_NAME_LIST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0808 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | list of viproc component names |
| Write |  | p_string |  | l_serv |  | list of viproc component names |

CONF_VIPROC_DLL_RELOAD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0809 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | not supported |
| Write |  | flag |  | l_serv |  | reload the viproc/VCA component |

CONF_VIPROC_SAVE_REFERENCE_IMAGE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0805 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | not supported |
| Write |  | f_flag |  | l_serv |  | triggers the VCA to create a reference image, but only if NOT a dome camera is used |

CONF_VIPROC_REFERENCE_IMAGE_FILENAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0806 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | reads the current reference image filename |
| Write |  | p_string |  | l_serv |  | not supported |

CONF_START_VIPROC_CONFIG_EDITING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a38 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | not supported |
| Write |  | t_dword |  | l_serv |  | Moves to the dome to the scene corresponding to the specified config and freezes the dome there. If already a config is in configuration mode, this command returns with a dword of 0. All subsequent viproc commands are related to this configuration. This command works also for non-dome devices. There it won't try to move the dome to the corresponding scene. |

CONF_STOP_VIPROC_CONFIG_EDITING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a39 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | not supported |
| Write |  | t_dword |  | l_serv |  | Stops editing of the specified config (see CONF_START_VIPROC_CONFIG_EDITING). If the specified scene does not match the currently edited config, a dword with value 0 is returned. |

CONF_CONT_VIPROC_CONFIG_EDITING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a3a |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | not supported |
| Write |  | t_dword |  | l_serv |  | Configuration of a config stops automatically after 20 seconds. This command can be used to keep configuration active for another 20 seconds. If the specified config is currently not in configuration mode, the command replys with a dword of 0. |

CONF_VIPROC_SCENE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a3b |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the scene for which the active config is defined. |
| Write |  | t_dword |  | l_serv |  | writes the scene number of the active viproc configuration |

CONF_NUMBER_OF_VIPROC_CONFIGS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a3c |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of configurations for the specified line. |
| Write |  | t_dword |  | l_serv |  | - |

CONF_ACTIVE_VIPROC_CONFIG

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a3f |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the config id activated by bool engine. |
| Write |  | t_dword |  | l_serv |  | Sets the specified config ID as active. The command has only an effect, if the VIPROC_MODE is set to SCRIPT mode (0xff). this command is not available on a gen4 dome. |

CONF_LOADED_VIPROC_CONFIG

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a3d |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the currently loaded config id. |
| Write |  | t_dword |  | l_serv |  | cannot be written. |

CONF_VIPROC_CONFIG_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a40 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | returns the name of the currently active viproc configuration. |
| Write |  | p_unicode |  | l_serv |  | writes the name of the currently active viproc configuration. The name can have at most 15 unicode characters. |

CONF_LIST_OF_VIPROC_SCENES

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a41 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | this command works only for Gen4 autodomes. It returns the list of defined scenes together with their names. Thereby the first byte specifies the scene number, followed by the length L of the scene name. The next L bytes belong to the scene name in unicode without 0 termination. This structure repeats until either the payload ends or the scene number is zero. |
| Write |  | t_dword |  | l_serv |  | - |

CONF_VIPROC_TAGGED_CONFIG

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a42 |  | video line |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read a list of viproc items in an atomar way. see detailed description . |
| Write |  | p_octet |  | l_serv |  | writes any viproc commands in an atomar way. see detailed description . |

This command is an extension of the already existing RCP+ commands CONF_VIPROC_DLL_NAME, CONF_VIPROC_ONOFF, CONF_VIPROC_SCENE, CONF_VIPROC_CONFIG_NAME, CONF_VIPROC_CUSTOM_PARAMETERS, CONF_VCD_OPERATOR_PARAMS, CONF_VIPROC_ALARM_MASK, CONF_VIPROC_ALARM_AGGREGATION_TIME, and CONF_VIPROC_MOTION_DEBOUNCE_TIME. Each of these commands can only access one specific item of the currently active viproc configuration. The new command allows an atomic access to an arbitrary subset of configuration items, not only of the currently active one but of any configuration of a line.
The payload has a tag structure which is as follows:

4 | 6 | 8 | 8+Length1 |  |  |  |  |
Config ID 4 Bytes | Tag1 2 Bytes | Length1 2 Bytes | Payload1 Length1 Bytes | Tag2 2 Bytes | Length2 2 Bytes | Payload2 Length2 Bytes | ... | 0 4 Bytes
RCP Payload N Bytes

where Config ID is an integer between 1 and the maximum number of configurations available for this line (this maximum number can be retrieved by the command CONF_NUMBER_OF_VIPROC_CONFIGS).
Num Value
The num value of the RCP command selects the video line to which the configuration belongs.
Return Value
For a read operation, payload of tags within the request are ignored. The reply payload contains all tags in the same order as in the request, however the size of the tags is adapted to fit the size of each item. If the structure of the request is invalid or an unknown tag is included, the command will fail.
For a write operation, the payload of tags must fit the size of the corresponding items. If this is not the case, the command will fail. If the CONF_VIPROC_CUSTOM_PARAMETERS and CONF_VCD_OPERATOR_PARAMS items are written for the currently active configuration, they are checked by the currently active viproc and ruleengine algorithms. If they are not accepted, the corresponding algorithm is set to default mode and the default parameters are put into the reply. To summarize, a write operation is successful, if the RCP+ command succeeds and the reply payload is identical to the request payload.
Tags
Values:
CONF_VIPROC_DLL_NAME
CONF_VIPROC_ONOFF
CONF_VIPROC_SCENE
CONF_VIPROC_CONFIG_NAME
CONF_VIPROC_CUSTOM_PARAMETERS
CONF_VCD_OPERATOR_PARAMS
CONF_VIPROC_ALARM_MASK
CONF_VIPROC_ALARM_AGGREGATION_TIME
CONF_VIPROC_MOTION_DEBOUNCE_TIME
Length
The length of the payload depends on the data type of the corresponding tag. The payload of a tag must be in network byte-order.
Values:
F_FLAG 1
T_WORD 2
T_DWORD 4
P_STRING string length
P_OCTET buffer length
The payload of a tag must be in network byte-order.
Example
The following payload example contains a configuration for the first configuration of a line. It consists of two tags, the first describing the CONF_VIPROC_CONFIG_NAME item, the second describing the CONF_VIPROC_ONOFF item.

4 | 6 | 8 | 15 | 17 | 19 | 20 | 24
Config ID 4 Bytes | Tag1 2 Bytes | Length1 2 Bytes | Payload1 7 Bytes | Tag2 2 Bytes | Length2 2 Bytes | Payload2 1 Byte | 0 4 Bytes
0x00 | 0x00 | 0x00 | 0x01 | 0x08 | 0x04 | 0x00 | 0x07 | "viproc" | 0x08 | 0x00 | 0x00 | 0x01 | 0x01 | 0x00 | 0x00 | 0x00 | 0x00
RCP Payload N Bytes

CONF_VIPROC_TAGGED_CONFIG_INTERNAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a43 |  | video line |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read a list of viproc items in an atomar way. |
| Write |  | p_octet |  | l_serv |  | writes any viproc commands in an atomar way. |

CONF_VIPROC_ALARM

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0807 |  | video line |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | p_octet |  | l_serv |  | - |

Payload Structure

16 | 32
Alarm Flags 2 Byte | Detector 2 Byte
ConfigId 1 Byte |
8 | 24 |

Alarm Flags
The message is sent whenever any of the bit values changes. Additionally it is sent once per 10 seconds when any of the bits is set.
Values:

Bit01 |  | Motion flag
Bit02 |  | global change flag
Bit03 |  | signal too bright flag
Bit04 |  | signal too dark flag
Bit05 |  | signal too noisy flag
Bit06 |  | image too blurry flag
Bit07 |  | signal loss flag
Bit08 |  | reference image check failed flag
Bit09 |  | invalid configuration flag

Detector
State of the detectors. The LSB corresponds to detector one.
ConfigId
Identifcation number of the VCA profile caused this alarm.
CONF_AUPROC_ALARM

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a79 |  | audio line |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | - |
| Write |  | p_octet |  | l_serv |  | - |

CONF_AUPROC_CONFIG

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a7a |  | yes (audio line) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read configuration of AUPROC |
| Write |  | p_octet |  | l_serv |  | write configuration of AUPROC |

Payload Structure

16 | 32 |
Version 4 Byte
Trigger Level 16 Byte
| Sensitivity 16 Byte
unused 1 Byte | Flags 1 Byte | reserved 2 Byte
8 | 24

Version
Unused.
Trigger Level
16 Values between 0 and 255 (1 Byte each), setting the fixed threshold for every frequency band and energy level.
First Byte is for the lowest frequency and the last for the energy level. Trigger level 0 indicates that this requency band is set off.
Sensitivity
16 Values between 1 and 100 (1 Byte each), setting the sensitivity for every frequency band and energy level.
First Byte is for the lowest frequency and the last for the energy level.
Flags
1 Byte for flags is reserved. The highest bit indicates audio alarm onoff.
Values:

Bit 8 |  | OnOff flag

CONF_AUPROC_MELPEGEL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a7b |  | yes (audio line) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read the recent pegel in the frequency bands: detailed decription |
| Write |  | p_octet |  | l_serv |  | not supported |

Payload Structure

16 | 32 |
recent melpegel 16 Byte
| adaptive threshold level 16 Byte

CONF_AUPROC_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a7c |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | - |
| Write |  | p_unicode |  | l_serv |  | - |

CONF_VIPROC_ALARM_MASK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a23 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read which of the 32 bits produced by the viproc+ruleengine are considered for the CONF_VIPROC_ALARM. see CONF_VIPROC_ALARM for the meaning of the 32 bits. |
| Write |  | p_octet |  | l_serv |  | configures which of 32 bits produced by the viproc+ruleengine are considered for the CONF_VIPROC_ALARM see CONF_VIPROC_ALARM for the meaning of the 32 bits. |

CONF_VIPROC_CONFIG_CHANGE_IN_RECORDING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a60 |  | video line |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | If the recording module detects a viproc configuration change, it sends this message. The payload of the message has the following structure: 8 Bytes - UTC timestamp int Time64 format, 1 Byte - config ID, 16 Bytes - MD5 Hash of the configuration. |
| Write |  | p_octet |  | l_serv |  | - |

CONF_VIPROC_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a65 |  | video line |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | octet |  | noprot |  | switches between silent motion(0)/manual(1..10)/off(0xfd)/scheduler(0xfe)/script mode(0xff) of the video content analysis (VCA). Returns current loaded id, if a dome is connected (if vca is turned off then 0xfd is returned). |
| Write |  | octet |  | l_serv |  | switches between silent motion(0)/manual(1..10)/off(0xfd)/scheduler(0xfe)/script mode(0xff) of the video content analysis (VCA). On the gen4 dome, the modes 0xfe and 0xff are not supported. Any value between 1 and 10 is interpreted as on. |

CONF_VIPROC_WEEKLY_SCHEDULE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a66 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Returns the weekly VCA schedule of the specified line. The format of the payload is the same as the one of the CONF_HD_RECORD_SCHEDULE command. |
| Write |  | p_octet |  | l_serv |  | Sets the weekly VCA schedule of the specified line. The format of the payload is the same as the one of the CONF_HD_RECORD_SCHEDULE command. |

CONF_VIPROC_HOLIDAYS_SCHEDULE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a67 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Returns the holidays VCA schedule of the specified line. The format of the payload is the same as the one of the CONF_HD_RECORD_HOLIDAYS command. |
| Write |  | p_octet |  | l_serv |  | Sets the holidays VCA schedule of the specified line. The format of the payload is the same as the one of the CONF_HD_RECORD_HOLIDAYS command. |

CONF_PTZ_CONTROLLER_AVAILABLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a51 |  | Message : no |  | Description : returns true if for the specified line a ptz controller is available which can be used by the VCA module. |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  |  |
| Write |  | flag |  | l_serv |  | is set to true if for the specified line a ptz controller is available which can be used by the VCA module. |

CONF_ENABLE_VCA

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0813 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | This command is used to configure the dome. Note that we write the information in the second bit of ptz_controller_available. |
| Write |  | flag |  | l_serv |  | This command is used to configure the dome. Note that we write the information in the second bit of ptz_controller_available. |

CONF_VIPROC_ALARM_AGGREGATION_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aca |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | read the alarm aggregation time of the video line (4,3s == 43). Note, this parameter belongs to a viproc config. |
| Write |  | t_octet |  | l_serv |  | write the duration of the alarm aggregation of the video line (1,6sec == 16). Note, this parameter belongs to a viproc config. |

CONF_VIPROC_MOTION_DEBOUNCE_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0acb |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | read the motion alarm debounce time of the video line (4,3s == 43). Note, this parameter belongs to a viproc config. |
| Write |  | t_octet |  | l_serv |  | write the duration of the motion alarm debounce time of the video line (1,6sec == 16). Note, this parameter belongs to a viproc config. |

CONF_VCA_FRAME_RESOLUTION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0814 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | d_word |  | noprot |  | read the current frame resolution of the video line |
| Write |  | t_dword |  | l_serv |  | read the current frame resolution of the video line |

CONF_REQUEST_FPGA_RTI

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0abd |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | not supported |
| Write |  | f_flag |  | l_serv |  | invokes a restart of the FPGA |

CONF_VIPROC_RESET

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a86 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | not supported |
| Write |  | f_flag |  | l_serv |  | Reset the viproc algorithm |

CONF_VIPROC_INSERT_CONFIG_INFO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a87 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | not supported |
| Write |  | p_octet |  | l_serv |  | Insert configuration information into the VCD stream of the VCA algorithm. This data will be added after the next FrameInfoTag of the output stream. |

CONF_VIPROC_VIDEO_FORMAT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a88 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Get the VCA video format |
| Write |  | p_octet |  | l_serv |  | Set the VCA video format |

This command reads or writes the video format parameters for the viproc algorithm. The payload components are also part of the ENC_META_FRAME_INFO struct (see viproc_frame_info.h).
The payload has the following structure:

4 | 8 | 12 | 16
Rows 4 Bytes | Columns 4 Bytes | StrideLuma 4 Bytes | StrideChroma 4 Bytes
SkipRatio 4 Bytes | FieldMode 4 Bytes | PicFreqNum 4 Bytes | PicFreqDenom 4 Bytes
AspectX 4 Bytes | AspectY 4 Bytes | ColorMode 4 Bytes | ChromaSubRate 4 Bytes

FieldMode
Values:
0: progressive
1: interlaced top field first
ColorMode
Values:
0: YUV
1: HSV
ChromaSubRate
Values:
0: 4:4:4
1: 4:2:2
2: 4:2:0
3: 4:1:1
CONF_VCA_TASK_RUNNING_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a96 |  | yes (camera line input number) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | returs the current processing state of the VCA engine; TRUE when vca engine is running with no problems; FALSE if vca engine lack cpu performance |
| Write |  | - |  | l_serv |  | not supported |

CONF_VIPROC_VERSION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ab2 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | viproc interface version on FPGA VCA devices |
| Write |  | p_octet |  | l_serv |  | viproc interface version on FPGA VCA devices |

CONF_VIPROC_STATUS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0abe |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | viproc status on FPGA VCA devices |
| Write |  | p_octet |  | l_serv |  | viproc status on FPGA VCA devices |

CONF_VIPROC_FLUSH

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0abf |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | viproc flush VCD data on FPGA VCA devices |
| Write |  | f_flag |  | l_serv |  | viproc flush VCD data on FPGA VCA devices |

CONF_SELECT_VCA_SCALER

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ae5 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | not supported |
| Write |  | t_dword |  | l_serv |  | force to use a specific input buffer from ambarella (first byte selects buffer for luma and second for chroma) |

CONF_HEARTBEAT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ab1 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get heartbeat |
| Write |  | t_dword |  | l_serv |  | get heartbeat |

CONF_OEM_DEVICE_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x097c |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | get the oem device name |
| Write |  | p_string |  | l_serv |  | not supported |

CONF_OEM_EXT_ID

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x097d |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | get the oem extension id |
| Write |  | t_octet |  | l_serv |  | not supported |

CONF_OEM_DEVICE_DOMAIN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e9 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | get the oem device domain |
| Write |  | p_string |  | l_serv |  | get the oem device domain |

CONF_DEFAULTS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x093d |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | - |  | noprot |  | not supported |
| Write |  | flag |  | l_serv |  | sets config to default values exept IP,mcIP,subnet and gateway, reset is necessary to apply all default settings |

CONF_FACTORY_DEFAULTS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09a0 |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | - |  | noprot |  | not supported |
| Write |  | flag |  | l_serv |  | set the configuration to factory defaults and reset the board |

CONF_BOARD_RESET

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0811 |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | not supported |
| Write |  | flag |  | l_serv |  | reset the board |

CONF_BOOT_DEFAULT_APP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x099f |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | not supported |
| Write |  | flag |  | l_serv |  | boot the default application |

CONF_VIDEO_TX_BITRATE_REQUEST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0301 |  | { |  | if (!SessionID) |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | noprot |  | % |
| Write |  | % |  | l_serv |  | % |

CONF_VIDEO_ENC_PRIO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a81 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | reads the video encoder priorisation 0:= no, 1:=h26x, 2:=jpeg |
| Write |  | t_dword |  | l_serv |  | writes the video encoder priorisation 0:=no, 1:=h26x, 2:=jpeg |

CONF_LED_BLINKING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x013d |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | always 1 |
| Write |  | flag |  | noprot |  | 1=power LED will flash for 7 sec |

CONF_JPEG

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x099e |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | l_live |  | 20 byte write payload: byte1: 0=QCIF, 1=CIF, 2=2CIF 3=4CIF; byte1:jpeg quality (0 is best); byte2,3 reserved; bytes 4-15: 3 int values for lastdc offset YUV, 16:=borderY, 17:=borderU, 18:= border V, 19:= borderWidth; (only on request allowed, cmd fails if a previous request is still in work) |
| Write |  | not supported |  | l_live |  | - |

CONF_CLUSTER_GROUP_SETTING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ca |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | list of (DWORD ip, DWORD flags, OCTET[6] mac, WORD reserved) cluster members including this unit |
| Write |  | p_octet |  | noprot |  | list of (DWORD ip, DWORD flags, OCTET[6] mac, WORD reserved) cluster members including this unit |

CONF_CLUSTER_ID

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09cb |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the logical position inside a cluster (0=stand alone, >0=slot nbr.) |
| Write |  | t_dword |  | l_serv |  | only in generic_dll: set vrm instance (0 <= ClusterId < 32) |

CONF_APP_OPTION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e0 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | reads if optional packages has been activated |
| Write |  | void |  | l_serv |  | not supported |

CONF_APP_OPTION_UNIT_ID

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e1 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read out the unique unit id (installation code) for setting application options |
| Write |  | void |  | l_serv |  | not supported |

CONF_APP_OPTION_SET

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e2 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | returns a readable string with the result code of the last applied set option |
| Write |  | p_string |  | l_serv |  | a key, generated by the license server to enable a specific application option; after entering a key, the APP_OPTION command returns the current activated application options |

CONF_CPU_LOAD_IDLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a06 |  | host=1, coproc=2 |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | cpu load idle in percent |
| Write |  | t_dword |  | l_serv |  | not supported |

CONF_CPU_LOAD_CODER

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a07 |  | host=1, coproc=2 |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | cpu load coder in percent |
| Write |  | t_dword |  | l_serv |  | not supported |

CONF_CPU_LOAD_CODER_INST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a7d |  | host=1, coproc=2 |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | cpu load of coder inst in percent (array of 13 bytes: 4 coder lines, each line has 3 coder instances, one entry for scaler) |
| Write |  | p_octet |  | l_serv |  | not supported |

CONF_CPU_LOAD_VCA

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a08 |  | host=1, coproc=2 |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | cpu load vca in percent |
| Write |  | t_dword |  | l_serv |  | not supported |

CONF_CPU_LOAD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a0a |  | host=1, coproc=2 |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | cpu load vca in percent (byte 0=idle, byte 1 = coder, byte 2=vca) |
| Write |  | p_octet |  | l_serv |  | not supported |

CONF_CPU_COUNT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a09 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | number of cpus |
| Write |  | t_dword |  | l_serv |  | not supported |

CONF_SANITY_CHECK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09da |  | no |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read the array of sanity bits (bit0: hdd, bit1: device error host, bit2: device error coproc) |
| Write |  | p_octet |  | l_serv |  | set the array of sanity bits (bit0:hdd) |

CONF_NIGHT_MODE_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aa2 |  | - |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 0=night mode off; 1=night mode on (only for devices supporting night mode) |
| Write |  | void |  | l_serv |  | not supported |

CONF_BLOCK_BASED_STORAGE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0adf |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | l_serv |  | read 512 byte memory blocks from flash (service for 3rd party modules like imgage-pipe dll or fpga) |
| Write |  | p_octet |  | l_serv |  | store 512 byte memory blocks in flash (service for 3rd party modules like imgage-pipe dll or fpga) |

Payload Structure

16 | 32
Domain 4 Bytes
Operation 4 Bytes
PageIndex 4 Bytes
PageCount 4 Bytes
Padding 16 Bytes ...
Payload n x 512 Bytes ...
8 | 24 |

Domain
Identifies the memory area to be accessed. Each module may have its own areas. The areas and their size have to be predefined by the firmware. Some may be permanent and some may get erased by the factory reset button.
Operation
Type of operation to be performed
Values:

BBSS_OP_READ |  | 0
BBSS_OP_WRITE |  | 1

PageIndex
Index of the first 512 byte page to be accessed
Values:

Index |  | 0..n-1

PageCount
Number of 512 byte pages to be accessed
Padding
Padding up to a total hdr size of 32 bytes
Values:

Should be zero |  | 0

Payload
n * 512 bytes payload to be read or written
Description
Read or write n blocks of 512 bytes to flash. All single blocks can be simply overwritten. A explicit erase is not required. Write is atomic on block basis which means that also in case of power-loss-while-write either the consistent old version or the new version of a single block is read back next time after reboot therefore doublebuffering is not required.
CONF_MPEG_AUDIO_SAMPLING_FREQ

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0932 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | mpeg audio sampling frequency (Hz) |
| Write |  | t_dword |  | l_serv |  | not supported |

CONF_MPEG4_CURRENT_PARAMS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0600 |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the current profile preset number for the specified encoder (NumDesc) |
| Write |  | t_dword |  | l_serv |  | sets the video encoder (given by NumDesc) to a preset (payload) |

CONF_MPEG4_CURRENT_PARAMS_REL_CODER

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x061c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get the current profile preset number for the specified encoder (relative to line). |
| Write |  | p_octet |  | l_serv |  | sets the video encoder (relative to line) to a preset. |

Payload Structure

16 | 32
Line 1 Byte | Coder 1 Byte | Coding Capabilities 2 Bytes
Preset 1 Byte | Reserved 1 Byte | Reserved 1 Byte | Reserved 1 Byte
8 | 24 |

Line
Video input line
Coder
Relative coder number (relative to line)
Coding Capabilities
Coding capabilities of encoder. All coding capabilities are one or multiple of:
Values:

H.263 |  | 0x0002
Mpeg 4 |  | 0x0004
Mpeg 2 |  | 0x0008
H.264 |  | 0x0040

Preset
Number of the encoder preset profile
Notes:
When reading the preset profile, the according byte in the payload will be set.
CONF_MPEG4_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0602 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | get the name of the preset given by the Numeric Descriptor |
| Write |  | p_string |  | l_serv |  | sets the name of the preset number given by the Numeric Descriptor |

CONF_MPEG4_BANDWIDTH_KBPS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0607 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | reads the bandwidth of selected preset |
| Write |  | t_dword |  | l_serv |  | sets the bandwidth of selected preset |

CONF_MPEG4_BANDWIDTH_KBPS_SOFT_LIMIT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0612 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | reads the bandwidth soft limit (in KBPS) of selected preset |
| Write |  | t_dword |  | l_serv |  | sets the bandwith soft limit (in KBPS) of selected preset |

CONF_MPEG4_BANDWIDTH_KBPS_HARD_LIMIT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0613 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the bandwidth hard limit (in KBPS) of selected preset |
| Write |  | t_dword |  | l_serv |  | sets the bandwidth hard limit (in KBPS) of selected preset |

CONF_MPEG4_INTRA_FRAME_DISTANCE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0604 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the intra frame distance of selected preset |
| Write |  | t_dword |  | l_serv |  | sets the intra frame distance of selected preset (not supported while recording is running) |

CONF_MPEG4_FRAME_SKIP_RATIO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0606 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets Mpeg4 frame skip ratio (1=all frames ,...) |
| Write |  | t_dword |  | l_serv |  | set Mpeg4 frame skip ratio (1=all frames ,...) |

CONF_MPEG4_RESOLUTION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0608 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the spatial resolution (0=QCIF, 1=CIF, 2=2CIF, 3=4CIF, 4=(1/2 D1), 5=(2/3D1), 6=QVGA, 7=VGA for selected preset |
| Write |  | t_dword |  | l_serv |  | sets the spatial resolution (0=QCIF, 1=CIF, 2=2CIF, 3=4CIF, 4=(1/2 D1), 5=(2/3D1), 6=QVGA, 7=VGA for selected preset |

CONF_MPEG4_FIELD_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x060e |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | get Mpeg4 field mode (0=progressive, 1=merged, 2=separated) |
| Write |  | t_octet |  | l_serv |  | set Mpeg4 field mode (0=progressive, 1=merged field, 2=separated field) |

CONF_MPEG4_DEFAULTS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0601 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | void |  | noprot |  | not supported |
| Write |  | flag |  | l_serv |  | set the selected preset params to the default values (recording has to be stopped, otherwise the iframe distance cannot be set to zero) |

CONF_MPEG4_I_FRAME_QUANT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x060a |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the I frame quantizer (1-31,0=auto) for selected preset |
| Write |  | t_dword |  | l_serv |  | sets the I frame quantizer (1-31,0=auto) of selected preset |

CONF_MPEG4_P_FRAME_QUANT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x060b |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the P frame quantizer (1-31,0=auto) for selected preset |
| Write |  | t_dword |  | l_serv |  | sets the P frame quantizer (1-31,0=auto) for selected preset |

CONF_MPEG4_PARAMS_MAX_NUM

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0614 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | Number of MPEG4 presets |
| Write |  | % |  | l_serv |  | % |

CONF_MPEG4_AVC_I_FRAME_QUANT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0615 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the I frame quantizer (9-51,0=auto) for selected preset |
| Write |  | t_dword |  | l_serv |  | sets the I frame quantizer (0=auto,9-51) for selected preset |

CONF_MPEG4_AVC_P_FRAME_QUANT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0616 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the P frame max quantizer (9-51,0=auto) for selected preset |
| Write |  | t_dword |  | l_serv |  | sets the P frame max quantizer (0=auto,9...51) for selected preset |

CONF_MPEG4_AVC_P_FRAME_QUANT_MIN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0620 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the P frame min quantizer (9-51,0=auto) for selected preset |
| Write |  | t_dword |  | l_serv |  | sets the P frame min quantizer (0=auto,9...51) for selected preset |

CONF_MPEG4_AVC_DELTA_IPQUANT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0621 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_int |  | noprot |  | gets the difference (-10..+10) between I and P-Frame quantization for selected preset |
| Write |  | t_int |  | l_serv |  | sets the difference (-10..+10) between I- and P-Frame quantization for selected preset |

CONF_MPEG4_AVC_DEBLOCKING_ENABLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0617 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_flag |  | noprot |  | gets the deblocking filter status for selected preset |
| Write |  | flag |  | l_serv |  | enables/disables the H264 deblocking filter |

CONF_MPEG4_AVC_DEBLOCKING_ALPHA

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0618 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_int |  | noprot |  | gets the alpha coefficient of the H264 deblocking filter for the selected preset |
| Write |  | t_int |  | l_serv |  | set the alpha H264 deblocking coefficent (-5...5) |

CONF_MPEG4_AVC_DEBLOCKING_BETA

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0619 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_int |  | noprot |  | gets the beta coefficient of the H264 deblocking filter for the selected preset |
| Write |  | t_int |  | l_serv |  | set the beta H264 deblocking coefficent (-5...5) |

CONF_MPEG4_AVC_CHROMA_QUANT_OFF

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x061a |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_int |  | noprot |  | gets the chroma quantisation offset for the selected preset |
| Write |  | t_int |  | l_serv |  | set the chroma quantisation offset (-12...12) |

CONF_MPEG4_AVC_CODING_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a45 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | gets the coding mode of the selected preset ( 0=frame; 1=field; 2=makro block adaptive ff; 3=picture adaptive ff ) |
| Write |  | t_octet |  | l_serv |  | sets the coding mode for the selected preset ( 0=frame; 1=field; 2=makro block adaptive ff; 3=picture adaptive ff ) |

CONF_MPEG4_AVC_GOP_STRUCTURE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a94 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | gets the GOP structure of the selected preset ( 0=IP; 1=IBP; 2=IBBP; 3=IBBRBP ) |
| Write |  | t_octet |  | l_serv |  | sets the GOP structure for the selected preset ( 0=IP; 1=IBP; 2=IBBP; 3=IBBRBP ) |

CONF_MPEG4_AVC_CABAC

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aa6 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | gets cabac for the selected preset ( 0=off; 1=on ) |
| Write |  | t_octet |  | l_serv |  | sets cabac for the selected preset ( 0=off; 1=on ) |

CONF_VIDEO_QUALITY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a82 |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the video quality for a selected preset (0=auto, 1(worst)..100(best)) |
| Write |  | t_dword |  | l_serv |  | sets the video quality for a selected preset (0=auto, 1(worst)..100(best)) |

CONF_JPEG_BANDWIDTH_KBPS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x061d |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the jpeg bandwidth (in KBPS) of selected preset |
| Write |  | t_dword |  | l_serv |  | sets the bandwith for jpeg streaming |

CONF_JPEG_BANDWIDTH_KBPS_SOFT_LIMIT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x061e |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the jpeg bandwidth soft limit(in KBPS) of selected preset |
| Write |  | t_dword |  | l_serv |  | sets the bandwith soft limit for jpeg streaming |

CONF_JPEG_BANDWIDTH_KBPS_HARD_LIMIT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x061f |  | profile preset |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the jpeg bandwidth hard limit(in KBPS) of selected preset |
| Write |  | t_dword |  | l_serv |  | sets the bandwith hard limit for jpeg streaming |

CONF_VID_ENCODER_ON

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0262 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | =1: video encoder is enabled on establishing a new connection; =0 video encoder is not enabled on establishing a new connection |
| Write |  | flag |  | l_serv |  | =1 enables the video encoder on establishing a new connection; =0 disables the video encoder on establishing a new connection |

CONF_VIDEO_ENCODER_STATUS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09df |  | coder instance |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get encoder status (8bytes) 4 (high order) bytes 10*frames per sec, 4 (low order) bytes KBPS |
| Write |  | p_octet |  | l_serv |  | not supported |

CONF_VIDEO_ENCODER_STATUS_EXT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a90 |  | coder instance |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get encoder status (20 bytes) 1st DWORD: 10*frames per sec, 2nd DWORD: KBPS, 3rd DWORD: nbr of dropped frames by the encoder due to bandwidth or system limitation, 4th DWORD: nbr of lost frames by capture hardware, 5th DWORD nbr of skipped frames as configured in profile |
| Write |  | p_octet |  | l_serv |  | not supported |

CONF_ENC_GET_SPS_AND_PPS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a1d |  | Coder |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Gets the sequence and picture parameter from H264 encoder |
| Write |  | p_octet |  | l_serv |  | not supported |

CONF_NAME_STAMP_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0084 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 0=name stamping off; 1=name stamping on bottom; 2=name stamping on top; 3=name stamping with custom attributes |
| Write |  | t_octet |  | l_user |  | 0=set name stamping off; 1=set name stamping on bottom; 2=set name stamping on top; 3=set name stamping with custom attributes which can be set with the CONF_STAMP_ATTR_NAME tag |

CONF_TIME_STAMP_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0085 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 0=time stamping off; 1=time stamping on bottom; 2=time stamping on top; 3=time stamping with custom attributes |
| Write |  | t_octet |  | l_user |  | 0=set time stamping off; 1=set time stamping on bottom; 2=set time stamping on top; 3=set time stamping with custom attributes which can be set with the CONF_STAMP_ATTR_TIME tag |

CONF_TIME_STAMP_RESOLUTION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a7f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 0=second, 1=ms |
| Write |  | t_octet |  | l_user |  | 0=second, 1=ms |

CONF_ALARM_DISP_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x008e |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 1=alarm display off; 2=alarm display on; 3=alarm stamping with custom attributes |
| Write |  | t_octet |  | l_serv |  | 1=disable alarm display; 2=enable alarm display; 3=alarm stamping with custom attributes which can be set with the CONF_STAMP_ATTR_ALARM tag |

CONF_ALARM_STRING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0090 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | get the alarm string |
| Write |  | p_unicode (max 32 unicode characters) |  | l_serv |  | set the alarm string |

CONF_STAMP_DEC_FREEZE_STRING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x092f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | string displayed on the local monitor if DEC_SHOW_FREEZE is enabled and no vido data is coming in |
| Write |  | p_string |  | l_serv |  | string displayed on the local monitor if DEC_SHOW_FREEZE is enabled and no vido data is coming in |

CONF_STAMP_ENC_NO_VIDEO_STRING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0930 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | string displayed on the remote monitor if no video has locked on the encoder |
| Write |  | p_string |  | l_serv |  | string displayed on the remote monitor if no video has locked on the encoder |

CONF_STAMP_NO_LINK_STRING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0931 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | string displayed on the local monitor if there is no ethernet link |
| Write |  | p_string |  | l_serv |  | string displayed on the local monitor if there is no ethernet link |

CONF_STAMP_ATTR_DEC_FREEZE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0933 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |
| Write |  | p_octet |  | l_serv |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |

CONF_STAMP_ATTR_ENC_NO_VIDEO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0934 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |
| Write |  | p_octet |  | l_serv |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |

CONF_STAMP_ATTR_NO_LINK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0935 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |
| Write |  | p_octet |  | l_serv |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |

CONF_STAMP_ATTR_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0936 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |
| Write |  | p_octet |  | l_serv |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |

CONF_STAMP_ATTR_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0937 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |
| Write |  | p_octet |  | l_serv |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |

CONF_STAMP_ATTR_ALARM

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0938 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |
| Write |  | p_octet |  | l_serv |  | 12 bytes: byte 0= pos x (0-255), byte 1= pos y (0-255), byte 3-11 reserved (set to zero) |

CONF_STAMP_WIDTH

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a93 |  | video line (1,..) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read the width of the current stamping in pixels. See detailed description |
| Write |  | void |  | l_serv |  | not supported |

Payload Structure

16 | 32
Stamping Type 2 Byte | Reserved 2 Byte
Width 4 Byte
8 | 24 |

Note: This command can only be read. The payload defines the stamping which should be read and returns the width in the corresponding field.
Stamping Type
Defines the stamping type of which the width should be determined. The type can be one of the following:
Values:

Time Stamp |  | 0x0001
Name Stamp row 1 |  | 0x0002
Name Stamp row 2 |  | 0x0003
Alarm Stamp |  | 0x0004
Info Stamp |  | 0x0005

Width
Width of the stamping in pixels (hex)
CONF_VIDEO_CURRENT_PARAMS_CODNBR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0982 |  | Message : no |  | Description : get the current profile preset number for the specified encoder (NumDesc) |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | noprot |  | % |
| Write |  | % |  | l_serv |  | % |

CONF_MAX_NBR_OF_ENC_STREAMS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x029e |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | Number of encoder streams |
| Write |  | t_dword |  | l_serv |  | read only |

CONF_WATERMARK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0924 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 0=watermark is disabled; 1=watermark is enabled |
| Write |  | t_octet |  | l_serv |  | 0=disables watermark; 1=enables watermark |

CONF_CODER_VIDEO_OPERATION_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a9c |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get video operation mode of the coder (given by NumDesc) (1 = h263, 2 = h264 ) (payload) |
| Write |  | t_dword |  | l_serv |  | set the coder (given by NumDesc) to a video operation mode (1 = h263, 2 = h264 ) (payload); (has only effect if coder is an video encoder); live connections will be dropped; only applicable if no recording is active |

CONF_CODER_VIDEO_OPERATION_OPTION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aa4 |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the coder (given by NumDesc) to a video option (has only effect if coder is an video encoder) (0 = no options (std), 1 = h.264 compatibility mode ) NOTE: this command will be depricated; use VIDEO_H264_ENC_BASE_OPERATION_MODE instead |
| Write |  | t_dword |  | l_serv |  | set the coder (given by NumDesc) to a video option (has only effect if coder is an video encoder) (0 = no options (std), 1 = h.264 compatibility mode ); for h.264 compatibility mode, the encoder will automatically switched to h.264 mode; NOTE: this command will be depricated; use VIDEO_H264_ENC_BASE_OPERATION_MODE instead |

CONF_VIDEO_H264_ENC_CONFIG

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ad2 |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get the profile for each h.264 encoder per line for each time. DWORD 1: Mode, 0=live mode, 1-10: schedule number; DWORD 2: profile for first stream, DWORD 3: profile for second stream... |
| Write |  | p_octet |  | l_serv |  | set the profile for each h.264 encoder per line for each time. DWORD 1: Mode, 0=live mode, 1-10: schedule number; DWORD 2: profile for first stream, DWORD 3: profile for second stream... |

CONF_VIDEO_H264_ENC_CONFIG_BULK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ad9 |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get the profiles for each h.264 encoder per line for each time; this request will supply all Modes 0-10 in one reply; returns: DWORD 1: NbrOfStreamsPerMode, remaining payload 11x payload of VIDEO_H264_ENC_CONFIG |
| Write |  | p_octet |  | l_serv |  | set the profiles for each h.264 encoder per line for each time; this request must supply all Modes 0-10 in one request; DWORD 1: NbrOfStreamsPerMode, remaining payload 11x payload of VIDEO_H264_ENC_CONFIG |

CONF_VIDEO_H264_ENC_BASE_OPERATION_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ad3 |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get the base operation mode of the h.264 encoders per line. first DWORD stream 1, second DWORD stream 2...; 0=disabled, 1=compatibility mode to H2.64 BP+, 2:h.264 MP high efficiency, 3: h.264 MP low latency |
| Write |  | p_octet |  | l_serv |  | set up the base operation mode of the h.264 encoders per line. first DWORD stream 1, second DWORD stream 2...; 0=disabled, 1=compatibility mode to H2.64 BP+, 2:h.264 MP high efficiency, 3: h.264 MP low latency |

CONF_VIDEO_H264_ENC_CURRENT_PROFILE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ad4 |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | returns the current active profile number for the h.264 streams (first DWORD: stream 1, second DWORD: stream 2...) |
| Write |  | - |  | l_serv |  | not supported |

CONF_JPEG_STREAM_SETUP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ad5 |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | returns the configuration of the JPEG encoder; DWORD 1:resolution (0=QCIF, 1=CIF, 2=2CIF, 3=4CIF, 6=QVGA, 7=VGA for selected preset), DWORD 2: fps in mHz, DWORD 3: quality (0=auto, 1(worst)..100(best)) |
| Write |  | p_octet |  | l_serv |  | Description : write the configuration of the JPEG encoder; DWORD 1:resolution (0=QCIF, 1=CIF, 2=2CIF, 3=4CIF, 6=QVGA, 7=VGA for selected preset), DWORD 2: fps in mHz, DWORD 3: quality (0=auto, 1(worst)..100(best)) |

CONF_REQ_FAST_UPDATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01d3 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | not supported |
| Write |  | flag |  | noprot |  | request a video intra frame, SessionID is mandatory |

CONF_MPEG4_INTRA_FRAME_REQUEST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0605 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | void |  | noprot |  | not supported |
| Write |  | t_dword |  | noprot |  | request a video intra frame, SessionID is mandatory |

CONF_LOW_LIGHT_MIN_FPS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ad8 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | min allowed frame rate for video sensor if low light mode is active value in mHz |
| Write |  | t_dword |  | l_serv |  | min allowed frame rate for video sensor if low light mode is active value in mHz |

CONF_VID_IN_CONTRAST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x092b |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | reads the contrast value (0-255) |
| Write |  | t_octet |  | l_serv |  | sets the contrast value (0-255) |

CONF_VID_IN_SATURATION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x092c |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | reads the saturation value (0-255) |
| Write |  | t_octet |  | l_serv |  | sets the saturation value (0-255) |

CONF_VID_IN_BRIGHTNESS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x092a |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | reads the brightness value (0-255) |
| Write |  | t_octet |  | l_serv |  | sets the brightness value (0-255) |

CONF_VID_IN_SAMPLING_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aa3 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  |  |
| Write |  | p_octet |  | l_serv |  |  |

Payload Structure

16 | 32
SamplingMode 4 Bytes
SamplingRateInmHz 4 Bytes
ExposureTimeInuSec 4 Bytes
BandingFilterConfig 4 Bytes
8 | 24 |

SamplingMode
0=Auto (exposure time is selected by camera)1=Manual ( if possible exposure time selected by ExposureTimeInuSec is used) 2=Banding filter (avoid banding effect caused by light sources with a flicker frequency of 2 x BandingFilterConfig)
SamplingRateInmHz
Defines the sampling rate in mHz
ExposureTimeInuSec
Defines the exposure time in uSec (1/1000000 Sec)
BandingFilterConfig
Defines the net frequency in mHz, avoids flickering of the camera if a light source is used which flickers with net frequency
Common usage for write: First read VID_IN_SAMPLING_MODE to get actual defined values, change the values which should be changed and write VID_IN_SAMPLING_MODE
CONF_VID_IN_WHITE_BALANCE_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aa8 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | 0=Auto White Balance,1=Manual White Balance actual RGB-Gain values are used, see CONF_VID_IN_RGB_GAIN |
| Write |  | t_dword |  | l_serv |  | 0=Auto White Balance; 1=Manual White Balance actual RGB-Gain values are used, see CONF_VID_IN_RGB_GAIN; 2=Hold AWB actual RGB-Gain values are saved (only possible, if AWB-Mode is active), they can be accessed by CONF_VID_IN_RGB_GAIN |

CONF_VID_IN_RGB_GAIN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aa9 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | 3 bytes: byte 0 =Red gain (0-255); byte 1 =Green gain (0-255), byte 2 =Blue gain (0-255) |
| Write |  | p_octet |  | l_serv |  | 3 bytes: byte 0 =Red gain (0-255); byte 1 =Green gain (0-255), byte 2 =Blue gain (0-255) |

CONF_VID_IN_MIRROR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aaa |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 0=deactivate image mirror; 1=activate image mirror |
| Write |  | flag |  | l_serv |  | 0=deactivate image mirror; 1=activate image mirror |

CONF_VIDEO_TERMINATION_RESISTOR_ON

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0274 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 1=analog video termination resistor is enabled (75 Ohms on); 0=analog video termination resistor is disabled (75 Ohms off) |
| Write |  | flag |  | l_serv |  | 1=enables the analog video termination resistor (75 Ohms on); 0=disables the analog video termination resistor (75 Ohms off) |

CONF_VIDEO_TERMINATION_RESISTOR_OFF

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0275 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 1=analog video termination resistor is disabled (75 Ohms off); 0=analog video termination resistor is enabled (75 Ohms on) |
| Write |  | flag |  | l_serv |  | 1=disables the analog video termination resistor (75 Ohms off); 0=enables the analog video termination resistor (75 Ohms on) |

CONF_VIDEO_INPUT_FORMAT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0504 |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the video input format 0=no, 1=PAL, 2=NTSC, 3=VGA, 4=720P |
| Write |  | t_dword |  | l_serv |  | set the VI norm 0=Autodetect; 1=PAL; 2=NTSC |

CONF_INPUT_SOURCE_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0086 |  | yes (line) |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | =1: camera; =2: vcr |
| Write |  | t_octet |  | l_serv |  | =1: camera; =2: vcr; =3: color_plane |

CONF_NBR_OF_VIDEO_IN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01d6 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of installed video inputs |
| Write |  | void |  | noprot |  | not supported |

CONF_PRIV_MSK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ab7 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | 1byte mode (0:=off,1:=black,2:=white,3:=grey), 1byte enable mask (bit 1 ==> rectangles 1 etc.), 2bytes reserved, 8 rectangles each 4bytes (x0,y0,x1,y2) |
| Write |  | p_octet |  | l_serv |  | 1byte mode (0:=off,1:=black,2:=white,3:=grey), 1byte enable mask (bit 1 ==> rectangles 1 etc.), 2bytes reserved, 8 rectangles each 4bytes (x0,y0,x1,y2) |

CONF_VIN_BASE_FRAMERATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ad6 |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the base input framerate in mHz |
| Write |  | - |  | l_serv |  | not supported |

CONF_ILLUMINATION_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ae4 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | get illumination mode (0: "IR illumination auto"; 1: "IR illumination off"; 2: "IR illumination on") |
| Write |  | t_octet |  | l_serv |  | set illumination mode (0: "IR illumination auto"; 1: "IR illumination off"; 2: "IR illumination on") |

CONF_VIDEO_OUT_STANDARD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0700 |  | output line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | get video output standard: 1=PAL; 2=NTSC; 3, 4, 5,...=VGA modes |
| Write |  | t_octet |  | l_serv |  | select video output standard: 1=PAL; 2=NTSC; 3, 4, 5,...=VGA modes |

CONF_MONITOR_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x028a |  | number of video output line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | read the video monitor name |
| Write |  | p_unicode (max 32 unicode characters) |  | l_serv |  | set the video monitor name |

CONF_VID_DECODER_ON

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0264 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | =1: video decoder is enabled on establishing a new connection; =0 video encoder is not deabled on establishing a new connection |
| Write |  | flag |  | l_serv |  | =1 enables the video decoder on establishing a new connection; =0 disables the video decoder on establishing a new connection |

CONF_LOGO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0939 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 0 := show "logo.h263" from toolkit 1:= no logo |
| Write |  | t_octet |  | l_serv |  | 0 := show "logo.h263" from toolkit 1:= no logo 2:= screen saver |

CONF_DEC_SHOW_FREEZE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x092e |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | freeze string: 0=off, 1=on, n=on (n * 40ms delayed) |
| Write |  | t_octet |  | l_serv |  | freeze string: 0=off, 1=on, n=on (n * 40ms delayed) |

CONF_DECODER_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0812 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | octet |  | noprot |  | decoder mode =0: low delay; =1: A/V sync; |
| Write |  | octet |  | l_serv |  | decoder mode =0: low delay; =1: A/V sync; |

CONF_DECODER_LAYOUT_LIST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09a1 |  | video out line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | list of supported layouts (0001=single view, 0002=quad view) |
| Write |  | p_octet |  | l_user |  | not supported |

CONF_DECODER_LAYOUT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09a2 |  | video out line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | first word (2bytes) is the layout, followed by the coder list in bytes (000101 for first monitor singleview, 000201020304 for quadview with chronological order) |
| Write |  | p_octet |  | l_user |  | first byte is the layout, followed by the coder list |

CONF_VIDEO_OUT_STANDARD_SPEC

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0706 |  | yes: corresponding video output standard number (see CONF_VIDEO_OUT_STANDARD) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | obtain video output standard specification |
| Write |  | p_octet |  | l_serv |  | configure video output standard (use zero payload size to reset to default) |

Payload Structure

16 | 32
pixelClock 4 Bytes
width 2 Byte | height 2 Byte
border_lft 2 Byte | border_rgt 2 Byte
border_top 2 Byte | border_bot 2 Byte
retrace_width 2 Byte | retrace_height 2 Byte
hsync_start 2 Byte | vsync_start 2 Byte
hsync_width 2 Byte | vsync_width 2 Byte
border_width 2 Byte | border_height 2 Byte
border_red 1 Byte | border _green 1 Byte | border_blue 1 Byte | reserved 4 Bits | h 1 | v 1 | sy 2
reserved 28 Bytes ...
8 | 24 |

pixelClock
pixel clock frequency in Hz
width
width of active screen in pixel
height
height of active screen in pixel
border_lft
width of the additional border left of the active screen
border_rgt
width of the additional border right of the active screen
border_top
height of the additional border above the active screen
border_bot
height of the additional border below active screen
retrace_width
duration of horizontal blanking period in pixel clock cycles
retrace_height
duration of vertical blanking period in scan line units
hsync_start
start of the horizontal sync impulse in pixel clock cycles past the beginning of the horizontal blanking period (signed 2s-complement)
vsync_start
start of the vertical sync impulse in scan lines past the beginning of the vertical blanking period (signed 2s-complement)
hsync_width
duration of the horizontal sync impulses in pixel clock cycles
vsync_width
duration of the vertical sync impulses in scan line units
border_width
(minimum) border width between the active subscreens in split screen mode
border_height
(minimum) border height between the active subscreens in split screen mode
border_red
intensity of the red channel of the border colour around the active screen and between subscreens
border _green
corresponding intensity of the green channel
border_blue
corresponding intensity of the blue channel
reserved
reserved for future extensions
hsync mode
polarity of horizontal sync signal
Values:

positive polarity (active high) |  | 0
negtive polarity (active low) |  | 1

vsync mode
polarity of vertical sync signal
Values:

positive polarity (active high) |  | 0
negative polarity (active low) |  | 1

sync signals
Values:

separate H-/V-sync signals |  | 0
composite sync signal |  | 1
illegal |  | 2
composite sync on green |  | 3

reserved
reserved for future extensions
Notes
In order to be selectable via CONV_VIDEO_OUT_STANDARD or CONV_VIDEO_OUT_CURRENT_SPEC, the corresponding parameters must comply with the currently active output device limits (see CONF_VIDEO_OUT_MONITOR_SPEC).
The resulting scan line frequency can be calculated by:
f_hsync = pixelClock / (width+border_lft+border_rgt+retrace_width)
The resulting vertical refresh frequency can be calculated by
f_vsync=f_hsync/(height+border_top+border_bot+retrace_height)
Negative values for sync_start and/or vsync_start are not guaranteed to work.
Depending on the hardware, the actual border colour may be different from the selected one and even different between the border around the active screen and the border between the subscreens in split screen mode.
Not all sync mode combinations are supported by the hardware.
The values returned on read may be different from the values set via the last write access, even if the supplied values are within the range supported by the output display as configured via CONF_VIDEO_OUT_MONITOR_SPEC.
CONF_VIDEO_OUT_CURRENT_SPEC

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0707 |  | yes: video out line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read active specification on a video out line |
| Write |  | p_octet |  | l_serv |  | temporarily change specification for a video out line |

Payload Structure

16 | 32
pixelClock 4 Bytes
width 2 Byte | height 2 Byte
border_lft 2 Byte | border_rgt 2 Byte
border_top 2 Byte | border_bot 2 Byte
retrace_width 2 Byte | retrace_height 2 Byte
hsync_start 2 Byte | vsync_start 2 Byte
hsync_width 2 Byte | vsync_width 2 Byte
border_width 2 Byte | border_height 2 Byte
border_red 1 Byte | border _green 1 Byte | border_blue 1 Byte | reserved 4 Bits | h 1 | v 1 | sy 2
reserved 28 Bytes ...
8 | 24 |

pixelClock
pixel clock frequency in Hz
width
width of active screen in pixel
height
height of active screen in pixel
border_lft
width of the additional border left of the active screen
border_rgt
width of the additional border right of the active screen
border_top
height of the additional border above the active screen
border_bot
height of the additional border below active screen
retrace_width
duration of horizontal blanking period in pixel clock cycles
retrace_height
duration of vertical blanking period in scan line units
hsync_start
start of the horizontal sync impulse in pixel clock cycles past the beginning of the horizontal blanking period (signed 2s-complement)
vsync_start
start of the vertical sync impulse in scan lines past the beginning of the vertical blanking period (signed 2s-complement)
hsync_width
duration of the horizontal sync impulses in pixel clock cycles
vsync_width
duration of the vertical sync impulses in scan line units
border_width
(minimum) border width between the active subscreens in split screen mode
border_height
(minimum) border height between the active subscreens in split screen mode
border_red
intensity of the red channel of the border colour around the active screen and between subscreens
border _green
corresponding intensity of the green channel
border_blue
corresponding intensity of the blue channel
reserved
reserved for future extensions
hsync mode
polarity of horizontal sync signal
Values:

positive polarity (active high) |  | 0
negtive polarity (active low) |  | 1

vsync mode
polarity of vertical sync signal
Values:

positive polarity (active high) |  | 0
negative polarity (active low) |  | 1

sync signals
Values:

separate H-/V-sync signals |  | 0
composite sync signal |  | 1
illegal |  | 2
composite sync on green |  | 3

reserved
reserved for future extensions
Notes
In order to be selectable via CONV_VIDEO_OUT_STANDARD or CONV_VIDEO_OUT_CURRENT_SPEC, the corresponding parameters must comply with the currently active output device limits (see CONF_VIDEO_OUT_MONITOR_SPEC).
The resulting scan line frequency can be calculated by:
f_hsync = pixelClock / (width+border_lft+border_rgt+retrace_width)
The resulting vertical refresh frequency can be calculated by
f_vsync=f_hsync/(height+border_top+border_bot+retrace_height)
Negative values for sync_start and/or vsync_start are not guaranteed to work.
Depending on the hardware, the actual border colour may be different from the selected one and even different between the border around the active screen and the border between the subscreens in split screen mode.
Not all sync mode combinations are supported by the hardware.
The values returned on read may be different from the values set via the last write access, even if the supplied values are within the range supported by the output display as configured via CONF_VIDEO_OUT_MONITOR_SPEC.
CONF_VIDEO_OUT_MONITOR_SPEC

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0708 |  | yes: video out line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read active monitor specification of a video out line |
| Write |  | p_octet |  | l_serv |  | override default monitor timing spec |

Payload Structure

16 | 32
width_mm 2 Byte | height_mm 2 Byte
native_width 2 Byte | native_height 2 Byte
hSyncMin 4 Bytes
hSyncMax 4 Bytes
vSyncMin 4 Bytes
vSyncMax 4 Bytes
dotClockMax 4 Bytes
reserved 23 Bits | s 1 | compSync 4 Bits | sepSync 4 Bits
reserved 32 Bytes ...
8 | 24 |

width_mm
physical width of the actual display region in mm
height_mm
physical height of the actual display region in mm
native_width
(maximum) width of the active display in pixel
native_height
(maximum) height of the active display in pixel
hSyncMin
lowest supported scan line (hsync) frequency in Hz
hSyncMax
highest supported scan line (hsync) frequency in Hz
vSyncMin
lowest supported vertical refresh frequency in mHz
vSyncMax
highest supported vertical refresh frequency in mHz
dotClockMax
upper limit on the pixel clock
reserved
reserved for future extensions
syncOnGreen
sync on green support:
Values:

unsupported |  | 0
supported |  | 1

compSync
bitmask of supported composite sync signals:
Values:

h-sync active high, v-sync active high |  | 1
h-sync active low, v-sync active high |  | 2
h-sync active high, v-sync active low |  | 4
h-sync active low, v-sync active low |  | 8

sepSync
bitmask of supported separate sync signals:
Values:

h-sync active high, v-sync active high |  | 1
h-sync active low, v-sync active high |  | 2
h-sync active high, v-sync active low |  | 4
h-sync active low, v-sync active low |  | 8

reserved
reserved for future extensions
Notes
In addition to the specified limits, default modes corresponding to the respective physical connector (e.g. standard VGA timing on a VGA connector, PAL/NTSC on BNC) are typically also assumed to be supported by the display device. The device will only allow video output timings (see CONF_VIDEO_OUT_CURRENT_SPEC, CONF_VIDEO_OUT_STANDARD) within these limits and may use the mentioned default timings as fallback values.
CONF_VIDEO_OUT_OVERSCAN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0709 |  | line number, 0=default line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word or t_dword |  | noprot |  | configure overscan area; arg = (monitor_overscan<<16) + intended_overscan; 100 % = 65536, values >= 50 % are forced to tolerable values |
| Write |  | t_dword |  | l_serv |  | configure overscan area; arg = (monitor_overscan<<16) + intended_overscan; 100 % = 65536, values >= 50 % are forced to tolerable values |

CONF_DECODED_FRAMES

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a1a |  | yes (coder number) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of decoded video frames of one deocder instance |
| Write |  | % |  | l_serv |  | % |

CONF_NBR_OF_VIDEO_OUT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01d7 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of installed video outputs |
| Write |  | t_dword |  | noprot |  | returns the number of installed video outputs |

CONF_ENABLE_OSD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0810 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | octet |  | noprot |  | osd on trimedia |
| Write |  | octet |  | l_serv |  | enable osd on trimedia |

CONF_OSD_ACCESS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x098a |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | not supported |
| Write |  | p_octet |  | l_serv |  | access to the OSD via RCP command |

Up to version 4.50 this command only applies to decoders to display text onto the video output. The num field carries the video output number; 0 indicates that the text should be displayed on all screens. From version 4.50 on this command also applies to encoders. In that case, the encoder will embed the text information into the RTP data stream to be overlayed by the receiving decoder. The attribute and flag fields are not applicable to the decoder's video output. The num field applies to the video input number.
Payload Structure

ID 2 Byte | len 2 Byte
x 1 Byte | y 1 Byte | reserved 2 Bytes ...
attributes 4 Bytes
flags 4 Bytes
String 1 1 Byte | N x 1 Byte | String N 1 Byte |

ID
Tag ID, for addressing different strings. Values 0x04-0x08 are possible.
len
Length of the complete payload
x
X-Position (0...255) where the string should be displayed (0 is left)
y
Y-Position (0...255) where the string should be displayed (0 is up)
reserved
Reserved fields for internal settings
attributes
Values:

Bit 11 |  | Centered display (0=off, 1=on)
Bit 13-15 |  | Fontsize (0=small, 1=big)

flags
Values:

Bit 0 |  | Interpret text as unicode characters (UTF-16)

String 1 - N
The string value which should be displayed
CONF_OSD_POS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ae0 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | not supported |
| Write |  | p_octet |  | l_serv |  | access to the OSD via RCP command |

Set the position of OSD objects (see CONF_OSD_ACCESS). The num field carries the video number; 0 indicates that the string positions on all video lines will be set.
Payload Structure

ID 2 Byte | x 1 Byte | y 1 Byte

ID
Tag ID, for addressing different strings. Values 0x04-0x08 are possible.
x
X-Position (0...255) where the string should be displayed (0 is left)
y
Y-Position (0...255) where the string should be displayed (0 is up)
CONF_AUDIO_INPUT_LEVEL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x000a |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets current level of audio input. Range: 0 to AUDIO_INPUT_MAX |
| Write |  | dword |  | l_serv |  | sets level of audio input. Range: 0 to AUDIO_INPUT_MAX |

CONF_AUDIO_OUTPUT_LEVEL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09b7 |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets level of audio input. Range: 0 to AUDIO_INPUT_MAX |
| Write |  | t_dword |  | l_serv |  | sets level of audio input. Range: 0 to AUDIO_INPUT_MAX |

CONF_AUDIO_G711

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x000c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 0=G.711 audio mode is not set, 1=G.711 audio mode is set |
| Write |  | flag |  | l_serv |  | set G.711 audio mode (0=off, 1=on) (has no effect on a running recording, to have the effect in recording, restart of recording is nessessary) |

CONF_AUDIO_STARTUP_SOUND

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09b6 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | turn on/off audio startup sound |
| Write |  | flag |  | l_serv |  | turn on/off audio startup sound |

CONF_AUDIO_INPUT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09b8 |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | dword |  | noprot |  | 0=Line, 1=Mic |
| Write |  | dword |  | l_serv |  | 0=Line, 1=Mic, 2=Mute (only supported by arm based products) |

CONF_AUDIO_OUTPUT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09b9 |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | 0=Decoder, 1=Sine, 2=Loop, 3=Mute, 4=Sample |
| Write |  | t_dword |  | l_serv |  | 0=Decoder, 1=Sine, 2=Loop, 3=Mute, 4=Sample |

CONF_AUDIO_INPUT_MAX

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ba |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the maximum input level that can be adjusted |
| Write |  | % |  | l_serv |  | % |

CONF_AUDIO_OUTPUT_MAX

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09bb |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets the maximum output level that can be adjusted |
| Write |  | % |  | l_serv |  | % |

CONF_AUDIO_MIC_LEVEL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09bc |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | dword |  | noprot |  | gets level of mic input. Range: 0 to AUDIO_MIC_MAX |
| Write |  | dword |  | l_serv |  | sets level of mic input. Range: 0 to AUDIO_MIC_MAX |

CONF_AUDIO_MIC_MAX

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09bd |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | dword |  | noprot |  | gets the maximum mic level that can be adjusted |
| Write |  | % |  | l_serv |  | % |

CONF_AUDIO_LOUDSPEAKER_ON_OFF

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09be |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | Gets Loudspeaker if on or off |
| Write |  | flag |  | l_serv |  | Sets Loudspeaker on or off |

CONF_AUDIO_OPTIONS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09bf |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | gets options for Audio, Bit 0=Line In, Bit 1=Line Out, Bit 2=Mic, Bit 3=Loudspeaker |
| Write |  | % |  | l_serv |  | % |

CONF_AUDIO_INPUT_PEEK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09c6 |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the max iabs of the audio input signal (clears the value) |
| Write |  | t_dword |  | l_serv |  | get the max iabs of the audio input signal (clears the value) |

CONF_AUDIO_OUTPUT_PEEK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09c7 |  | audio line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the max iabs of the audio output signal (clears the value) |
| Write |  | t_dword |  | l_serv |  | get the max iabs of the audio output signal (clears the value) |

CONF_NBR_OF_AUDIO_OUT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01d9 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of audio outputs |
| Write |  | % |  | l_serv |  | % |

CONF_NBR_OF_AUDIO_IN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01d8 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of audio inputs |
| Write |  | % |  | l_serv |  | % |

CONF_ALARM_INPUT_LH_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x008d |  | alarm input |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 1=alarm pin high active; 2=alarm pin low active |
| Write |  | t_octet |  | l_serv |  | 1=set alarm pin high active; 2=set alarm pin low active |

CONF_INPUT_PIN_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0108 |  | alarm in |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | read the description for an input alarm |
| Write |  | p_unicode (max 32 unicode characters) |  | l_serv |  | set the description for an input alarm |

CONF_VCD_OPERATOR_PARAMS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a1b |  | video line |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read parametrization of vcd operator which corresponds to line |
| Write |  | p_octet |  | l_serv |  | configures the vcd manager. if configuration fails an error is returned. |

CONF_CAMERA_MOTION_ALARM_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09b2 |  | motion area (1..4) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | turn on/off the motion alarm of the dinion camera. |
| Write |  | flag |  | l_serv |  | turn on/off the motion alarm of the dinion camera. |

CONF_ALARM_CONNECT_TO_IP_STR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0081 |  | destination IP number |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the alarm IP using string notation (xxx.xxx.xxx.xxx) |
| Write |  | p_string |  | l_serv |  | set alarm IP using string notation (xxx.xxx.xxx.xxx) |

CONF_ALARM_CONNECT_TO_IP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0041 |  | destination IP number |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | read the connect on alarm event IP address |
| Write |  | t_dword |  | l_serv |  | specify the connect on alarm event IP address |

CONF_NBR_OF_ALTERNATIVE_ALARM_IPS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0303 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the number of available alarm ip addresses (total presets) |
| Write |  | void |  | l_serv |  | not supported |

CONF_AUTO_DISCONNECT_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x030d |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | 0=no auto disconnect; 0 |
| Write |  | t_dword |  | l_serv |  | 0=no auto disconnect; 0 |

CONF_DEFAULT_CONNECTION_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0289 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | noprot |  | % |
| Write |  | t_octet |  | l_serv |  | get the default connection mode: 0=MPEG2, 1=MPEG4, 2=MPEG4/AVC, 3=JPEG |

CONF_STD_MEDIA_CONNECTION_DIRECTION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x030c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | =0: outgoing media for alarm connections; =1: req. incoming media for alarm connections; =2: req. bidirectional media for alarm connections |
| Write |  | t_octet |  | l_serv |  | =0: outgoing media for alarm connections; =1: req. incoming media for alarm connections; =2: req. bidirectional media for alarm connections |

CONF_STD_MEDIA_ENCAPSULATION_PROTOKOL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0309 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | defines the standard media encapsulation protokol: 1=RTP over UDP, 2=TCP |
| Write |  | t_octet |  | l_serv |  | defines the standard media encapsulation protokol: 1=RTP over UDP, 2=TCP |

CONF_DEFAULT_CAM

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01af |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | reads the default camera for alarm connections |
| Write |  | t_octet |  | l_serv |  | defines the default camera for alarm connections |

CONF_ALARM_CONNECTION_DESTINATION_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a15 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | returns the network destination port on outgoing alarm connections |
| Write |  | t_word |  | l_serv |  | selects the destination network port for outgoing alarm connections; all other than 1756 (default RCP port) will use the HTTP tunneling protocol. In this case, this must be the HTTP/HTTPS port of the called host. |

CONF_ALARM_CONNECTION_USE_SSL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a16 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | use RCP SSL for outgoing alarm connections |
| Write |  | flag |  | l_serv |  | use RCP SSL for outgoing alarm connections |

CONF_CONNECT_URL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a1e |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | get the connect url |
| Write |  | p_string |  | l_serv |  | set the connect url |

CONF_VIDEO_ALARM_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01c2 |  | video line |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 0=video alarm is off; 1=video alarm is on |
| Write |  | void |  | noprot |  | not supported |

CONF_INPUT_PIN_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01c0 |  | alarm in |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 0=alarm input off; 1= alarm input on |
| Write |  | void |  | noprot |  | not supported |

CONF_MOTION_ALARM_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01c3 |  | video line |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 0=motion alarm off; 1=motion alarm on (at elast one of the CONF_VIPROC_ALARM alarmbit (except the video loss alarm) is set |
| Write |  | flag |  | noprot |  | not supported |

CONF_RELAY_OUTPUT_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01c1 |  | relay output |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | returns the current logical level of an relay output |
| Write |  | flag |  | l_user |  | set the logical level of an relay output |

CONF_NBR_OF_ALARM_IN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01db |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of installed alarm input contacts (possible masterswitch included) |
| Write |  | void |  | l_priv |  | not supported |

CONF_NBR_OF_ALARM_OUT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01dc |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of installed alarm output contacts |
| Write |  | void |  | l_priv |  | not supported |

CONF_NBR_OF_MOTION_DETECTORS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09af |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of installed motion detectors |
| Write |  | % |  | l_priv |  | % |

CONF_HD_MGR_SIGNAL_ALARM

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0915 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | - |  | noprot |  | not supported |
| Write |  | flag |  | l_serv |  | signal alarm: only one alarm per second is allowed, |

CONF_VIRTUAL_ALARM_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a8b |  | virtual alarm line 1 - 4 |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 0=virtual alarm off; 1=virtual alarm on |
| Write |  | flag |  | l_serv |  | 0=virtual alarm off; 1=virtual alarm on |

CONF_RELAIS_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0109 |  | relay output |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_unicode |  | noprot |  | read the description for a relay output |
| Write |  | p_unicode (max 32 unicode characters) |  | l_serv |  | set the description for a relay output |

CONF_RELAIS_SWITCH

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0094 |  | relay output |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | return the current relay state |
| Write |  | flag |  | l_serv |  | switch the relais immediately |

CONF_SERIAL_PORT_APP_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01f1 |  | physical port |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 0=serial port application is in terminal mode; 0xFF=serial port application is in transparent datamode; values 1-10: camera type mode |
| Write |  | t_octet |  | l_serv |  | 0=sets the serial port application in terminal mode; 0xFF=sets the serial port application in transparent datamode; values 1-10: sets to camera type mode |

CONF_SERIAL_PORT_RATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x027e |  | physical port |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | bitrate=300; bitrate=600; bitrate=1200; bitrate=2400; bitrate=4800; bitrate=9600; bitrate=19200 |
| Write |  | t_dword |  | l_serv |  | bitrate=300; bitrate=600; bitrate=1200; bitrate=2400; bitrate=4800; bitrate=9600; bitrate=19200 |

CONF_SERIAL_PORT_BITS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x027f |  | physical port |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 7=seven data bits; 8=eight data bits |
| Write |  | t_octet |  | l_serv |  | 7=set to seven data bits; 8=set to eight data bits |

CONF_SERIAL_PORT_STBITS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0280 |  | physical port |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 1=modemport stopbits are set to 1; 2=modemport stopbits are set to 2 |
| Write |  | t_octet |  | l_serv |  | 1=modemport stopbits are set to 1; 2=modemport stopbits are set to 2 |

CONF_SERIAL_PORT_PAR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0281 |  | physical port |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 0=no parity; 1=even parity; 2=odd parity |
| Write |  | t_octet |  | l_serv |  | 0=set to no parity; 1=set to even parity; 2=set to odd parity |

CONF_SERIAL_PORT_MODE_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0208 |  | physical port |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 1=port mode is set to RS232; 2=port mode is set to RS422/RS485 (NOT avalibale in conventional VideoJet) |
| Write |  | t_octet |  | l_serv |  | 1=set port mode to RS232; 2=set port mode to RS422/RS485 |

CONF_SERIAL_PORT_HD_MODE_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x020b |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | =0: halfduplex mode is set to off; =1:halfduplex mode is set to on; =2: halfduplex mode is set to on and buffered data (NOT avalibale in conventional VideoJet) |
| Write |  | t_octet |  | l_serv |  | =0: set halfduplex mode to off; =1:set halfduplex mode to on; =2: set halfduplex mode to on and buffered data |

CONF_SERIAL_PORT_HANDSHAKE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09a9 |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | get type of handshake (internal use only) |
| Write |  | t_octet |  | l_serv |  | set type of handshake (internal use only) |

CONF_BICOM_COMMAND

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09a5 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | not supported |
| Write |  | p_octet |  | l_user |  | Sends a BICOM read or write command to the local camera frontend, see detailed description |

Payload Structure

16 | 32
Flags 1 Byte | Bicom Server ID 2 Byte | Object ID 2 Byte ...
| Operation 1 Byte | Bicom Payload 30 Bytes ...
8 | 24 |

Flags
Transmission-Flags
Values:

Return_Payload (Must be set to 1 if return payload is expected) |  | Bit 0
Best_Effort (Set to 1 to transmitt as best effort frame) |  | Bit 1
Native_Errors (Set to 1 to receive the native BICOM errors) |  | Bit 2
unused set to 0 |  | Bit 3
unused set to 0 |  | Bit 4
unused set to 0 |  | Bit 5
unused set to 0 |  | Bit 6
Flags_Available (Must be always set to 1) |  | Bit 7

Bicom Server ID
e.g. Device-Server or IO-Server (See BICOM Application Doku)
Object ID
e.g. Device Type (= 0x100) (See BICOM Application Doku)
Operation
See BICOM Application Doku
Values:

GET |  | 0x01
SET |  | 0x02
SET_GET |  | 0x03
INC |  | 0x04
INC_GET |  | 0x05
DEC |  | 0x06
DEC_GET |  | 0x07
SET_DFLT |  | 0x08

Bicom Payload
Bicom Payload
Example for a RCP Request:

81 |  | Return payload expected
00 02 |  | Device = 2 = "Device server"
01 50 |  | Parameter IdString
01 |  | Operation Read

Example for a RCP Response:

81 |  | Return payload expected
00 02 |  | Device = 2 = "Device server"
01 50 |  | Parameter IdString
01 |  | Operation Read
00 68 00 68 00 68 00 68 00 20 00 20 00 20 00 20 00 20 00 20 00 20 00 20 00 20 00 20 00 20 00 20 00 20 |  | 34 Bytes Unicode ID String

CONF_BICOM_SRV_CONNECTED

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a19 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | return true if the device is connected to the BICOM server (Camera) |
| Write |  | % |  | l_user |  | % |

CONF_BICOM_UPLOAD_PACKET

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09c9 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | l_serv |  | % |
| Write |  | p_octet |  | l_serv |  | writes a sub-module firmware upload block |

CONF_BICOM_SUBCOMPONENTS_LIST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aa5 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Read List of FamilyIDs and Firmware Versions for Subcomponents of Gen4 (Future Dinion?) |
| Write |  | p_octet |  | l_priv |  | Read List of FamilyIDs and Firmware Versions for Subcomponents of Gen4 (Future Dinion?) |

CONF_KBD_CONFIG_CAMERA

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a31 |  | yes (camera number on keyboard) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read configuration of camera numbers on keyboard |
| Write |  | p_octet |  | l_serv |  | configure camera numbers on keyboard; assign parameters to a number (given by num) |

Payload Structure

16 | 32
IP 4 Bytes
Line 1 Byte | Coder 1 Byte | Preset 1 Byte | Reserved 1 Byte
8 | 24 |

IP
Encoder/Camera IP
Line
Video input line
Coder
Relative coder number (relative to line)
Preset (optional)
(Dome-) Preset Position. (Every Preset of a Dome can be treated as a seperate camera).
CONF_KBD_CONFIG_MONITOR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a32 |  | yes (monitor number on keyboard) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read configuration of monitor numbers on keyboard |
| Write |  | p_octet |  | l_serv |  | configure monitor numbers on keyboard; assign parameters to a number (given by num) |

Payload Structure

16 | 32
IP 4 Bytes
Line 1 Byte | Coder 1 Byte | Reserved 1 Byte | Reserved 1 Byte
8 | 24 |

IP
Decoder/Monitor IP
Line
Video output line
Coder
Relative coder number (relative to line)
CONF_KBD_CONNECT_PARAMS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a33 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read parameters for connections established via keyboard |
| Write |  | p_octet |  | l_serv |  | set parameters for connections established via keyboard |

Payload Structure

16 | 32
Flags 2 Bytes | Reserved 2 Bytes
8 | 24 |

Flags (optional)
Values:

Bit 0 |  | Request audio TX (listen at decoder side)
Bit 1 |  | Request audio RX (speak at decoder side)

CONF_KBD_PASSWORD_CAMERA

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a34 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | l_serv |  | get the password (scrambled) for all cameras used on keyboard |
| Write |  | p_string |  | l_serv |  | deposit a password for all cameras used on keyboard |

CONF_KBD_PASSWORD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a69 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | l_serv |  | get the password (scrambled) of the keyboard |
| Write |  | p_string |  | l_serv |  | deposit a password for the keyboard |

CONF_KBD_CONFIG_SALVO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a3e |  | yes (salvo number) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read configuration of salvos for keyboard |
| Write |  | p_octet |  | l_serv |  | configure salvos used for keyboard; assign parameters to a salvo number (given by num) |

Payload Structure

16 | 32
Duration 2 Bytes | Reserved 2 Bytes
Camera Num 1 1 Byte | N x 1 Byte | Camera Num N 1 Byte |
8 | 24 |

Duration
Duration of one salvo position in seconds
Camera Num N
Camera number for salvo position N (note: Camera number has to be specified using CONF_KBD_CONFIG_CAMERA)
CONF_KBD_KEY_LABEL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a44 |  | yes (key number; must be >0) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read a label of a key used for the alarm task editor. The label is shown on the keyboard display. |
| Write |  | p_string |  | l_serv |  | deposit a label for a key used for the alarm task editor. The label is shown on the keyboard display. |

CONF_KBD_SET_ALARM

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a68 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | - |  | noprot |  | not supported |
| Write |  | f_flag |  | noprot |  | send alarm to keyboard |

CONF_MAC_ADDRESS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x00bc |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read out the systems MAC address |
| Write |  | void |  | noprot |  | not supported |

CONF_IP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0001 |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | read the unit's IP address |
| Write |  | t_dword |  | l_serv |  | set the unit's IP address |

CONF_IP_STR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x007c |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the unit's IP address using string notation (xxx.xxx.xxx.xxx) |
| Write |  | p_string |  | l_serv |  | set unit's IP address using string notation (xxx.xxx.xxx.xxx) |

CONF_SUBNET

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0002 |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | read the unit's subnet |
| Write |  | t_dword |  | l_serv |  | set the unit's subnet |

CONF_GATEWAY_IP_STR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x007f |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the gateway IP using string notation (xxx.xxx.xxx.xxx) |
| Write |  | p_string |  | l_serv |  | set gateway IP using string notation (xxx.xxx.xxx.xxx) |

CONF_DNS_SERVER_IP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a1f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get dns server ip |
| Write |  | t_dword |  | l_serv |  | set dns server ip |

CONF_ETH_LINK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x092d |  | yes; num=0 is the mode of the external state on single ethernet port units or the internal link mode on multiple ethernet port units; num>=1 is the mode of the corresponding port on multiple ethenet port units (SFP Fiber port is always the last counted port). On module based units, only the master module is capable of setting the external port modes. |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | (half duplex=HD, full duplex =FD) 0=auto, 1=10MbitHD, 2=10MbitFD, 3=100MbitHD, 4=100MbitFD |
| Write |  | t_octet |  | l_serv |  | (half duplex=HD, full duplex =FD) 0=auto, 1=10MbitHD, 2=10MbitFD, 3=100MbitHD, 4=100MbitFD, 5=1000FD |

CONF_ETH_LINK_STATUS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a24 |  | yes; num=0 returns the status of the external state on single ethernet port units or the internal link state on multiple ethernet port units; num>=1 returns the state of the corresponding port on multiple ethenet port units (SFP Fiber port is always the last counted port). On module based units, only the master module is capable of returning the external states. |  | yes |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | (half duplex=HD, full duplex =FD) 0=No link, 1=10MbitHD, 2=10MbitFD, 3=100MbitHD, 4=100MbitFD, 5=1000FD; |
| Write |  | void |  | l_serv |  | not suported |

CONF_ETH_LINK_TROUGHPUT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a80 |  | Message : no |  | Description : lower 16 bit: downlink KBPS, upper 16 bit: uplink KBPS |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | noprot |  | % |
| Write |  | void |  | l_serv |  | not suported |

CONF_NBR_OF_EXT_ETH_PORTS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a28 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of external ethernet ports of a device |
| Write |  | void |  | l_serv |  | not supported |

CONF_NBR_OF_EXT_ETH_COPPER_PORTS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a29 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of external copper ethernet ports of a device |
| Write |  | t_dword |  | l_serv |  | returns the number of external copper ethernet ports of a device |

CONF_NBR_OF_EXT_ETH_FIBER_PORTS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a2a |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the number of external fiber ethernet ports of a device |
| Write |  | t_dword |  | l_serv |  | returns the number of external fiber ethernet ports of a device |

CONF_ENABLE_TRAFFIC_LED

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09a6 |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | network activity LED (Dinion, NBC-255 camera): 0=off, 1=on |
| Write |  | t_octet |  | l_serv |  | Enables or disables the network activity LED (Dinion, NBC-255 camera) |

CONF_SND_MSS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a02 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | max tcp send mss for all connections |
| Write |  | t_dword |  | l_serv |  | set the global tcp send mss; use this to reduce the max. send segment size for all tcp connections; higher settings than default will only be used by iSCSI connections (0 means default) |

CONF_SND_MSS_ISCSI

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a22 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | max tcp send mss for iscsi |
| Write |  | t_dword |  | l_serv |  | set the max. tcp send mss for iSCSI connections; NOTE: this setting will also adjust the global setting SND_MSS |

CONF_EAP_IDENTITY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ea |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the EAP identity |
| Write |  | p_string |  | l_serv |  | write the EAP identity |

CONF_EAP_ENABLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09eb |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | read the EAP/802.1x status (0: off/don't do EAP/802.1x; 1: on/use EAP/802.1x) |
| Write |  | t_octet |  | l_serv |  | write the EAP/802.1x status (0: off/don't do EAP/802.1x; 1: on/use EAP/802.1x) |

CONF_EAP_PASSWORD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ec |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the EAP password |
| Write |  | p_string |  | l_serv |  | write the EAP password |

CONF_SWITCH_TRUNKING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a6b |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | external ports bitwise members of a trunk |
| Write |  | t_octet |  | l_serv |  | external ports bitwise members of a trunk |

CONF_SWITCH_LACP_ENABLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a6c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | external ports bitwise enabling LACP+RSTP mode, 0: off, 1:on |
| Write |  | t_octet |  | l_serv |  | external ports bitwise enabling LACP+RSTP mode, 0: off, 1:on |

CONF_SWITCH_LACP_KEY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a6d |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | LACP Key for external ports, 1-255, 0: auto |
| Write |  | t_octet |  | l_serv |  | LACP Key for external ports, 1-255, 0: auto |

CONF_SWITCH_RSTP_PRIO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a6e |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | RSTP Priority val in range of 0 ... 61440, must be multiple of 4096 |
| Write |  | t_dword |  | l_serv |  | RSTP Priority val in range of 0 ... 61440, must be multiple of 4096 |

CONF_SWITCH_RSTP_HELLO_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a6f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | RSTP Hello Time in range of 1...10, default 2 |
| Write |  | t_octet |  | l_serv |  | RSTP Hello Time in range of 1...10, default 2 |

CONF_SWITCH_RSTP_MAX_AGE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a70 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | RSTP Max Age in range of 6...40, default 20 |
| Write |  | t_octet |  | l_serv |  | RSTP Max Age in range of 6...40, default 20 |

CONF_SWITCH_RSTP_FWD_DELAY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a71 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | RSTP Forward Delay in range of 4...30, default 15 |
| Write |  | t_octet |  | l_serv |  | RSTP Forward Delay in range of 4...30, default 15 |

CONF_SWITCH_RSTP_VERSION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a72 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | RSTP Version, 0: STP compatible, 2: RSTP |
| Write |  | t_octet |  | l_serv |  | RSTP Version, 0: STP compatible, 2: RSTP |

CONF_SWITCH_RSTP_PORT_ENABLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a74 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | external ports bitwise enabling RSTP-only mode, 0: off, 1:on |
| Write |  | t_octet |  | l_serv |  | external ports bitwise enabling RSTP-only mode, 0: off, 1:on |

CONF_SWITCH_RSTP_PORT_EDGE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a75 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | external ports bitwise determining if RSTP edge port |
| Write |  | t_octet |  | l_serv |  | external ports bitwise determining if RSTP edge port |

CONF_SWITCH_RSTP_PORT_PATHCOST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a76 |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | RSTP pathcost of external ports in range of 1...200000000, while 0 means auto |
| Write |  | t_dword |  | l_serv |  | RSTP pathcost of external ports in range of 1...200000000, while 0 means auto |

CONF_BACKPLANE_TYPE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a78 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | type of backplane 0xff: no backplane, 0xfe: old, 0: full-flavoured, 1: eco, 2: diplan |
| Write |  | % |  | l_serv |  | % |

CONF_BACKPLANE_FW_VERSION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a84 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | firmware version on backplane 0: error / no (valid) backplane, else: firmware revision |
| Write |  | % |  | l_serv |  | % |

CONF_SWITCH_IGMP_IP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a95 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | IP address that the VIPX1600 backplane uses as source IP in IGMP queries |
| Write |  | t_dword |  | l_serv |  | IP address that the VIPX1600 backplane uses as source IP in IGMP queries |

CONF_SWITCH_IGMP_SNOOPING_ENABLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a9a |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | enable IGMP snooping on Vitesse backplane switch, 0: off, 1: on |
| Write |  | t_dword |  | l_serv |  | enable IGMP snooping on Vitesse backplane switch, 0: off, 1: on |

CONF_SWITCH_MAC_IS_SET

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a9d |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | determine of backplane has a valid MAC address: 0: invalid, 1: not yet known, ask later (during boot process), 2: valid |
| Write |  | % |  | l_serv |  | % |

CONF_REBOOT_SWITCH

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a9e |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | % |  | l_serv |  | % |
| Write |  | t_dword |  | l_serv |  | reboot switch |

CONF_WLAN_SSID

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0943 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the WLAN ssid |
| Write |  | p_string |  | l_serv |  | write the WLAN ssid |

CONF_WLAN_WPA_PSK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ac3 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the WPA pre shared key |
| Write |  | p_string |  | l_serv |  | write the WPA pre shared key |

CONF_PORT_FC_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0abb |  | yes; num=0 is the flow control mode of the external state on single ethernet port units or the internal fc mode on multiple ethernet port units; num>=1 is the fc mode of the corresponding port on multiple ethenet port units (SFP Fiber port is always the last counted port). On module based units, only the master module is capable of setting the external port fc modes. |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 0=off, 1=on |
| Write |  | t_octet |  | l_serv |  | 0=off, 1=on |

CONF_WLAN_SCAN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ac6 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Performs a WLAN network scan, see detailed description |
| Write |  |  |  | l_serv |  | not supported |

Payload Structure

16 | 32
Number of Entries 4 Bytes

Sequence of:

SSID 32 Bytes
MAC Address 6 Bytes
| Strength 4 Bytes
| Channel 4 Bytes
| Flags 4 Bytes
16 | 32

SSID
Name of Network.
MAC Address
MAC Address of AccessPoint.
Strength
Signal Strength [0;5]
Channel
Channel used by AccessPoint [0; 14]
Flags
Values:

Bit0 |  | WEP encryption supported
Bit1 |  | WPA encryption supported
Bit2 |  | WPA2 encryption supported

CONF_WLAN_OPERATING_MODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ac7 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Gets the operating mode of WLAN (0="off", 1="auto") |
| Write |  | t_octet |  | l_serv |  | Sets the operating mode of WLAN (0="off", 1="auto") |

CONF_SWITCH_POST_UPDATE_ACTION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ac5 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | id that indicates which action is to be executed as the switch firmware was updated (0: none) |
| Write |  | t_octet |  | l_serv |  | id that indicates which action is to be executed as the switch firmware was updated (0: none) |

CONF_WLAN_REGION_CODE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0acf |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | Gets the region code for WLAN adapter (0x10="US", 0x20="CA", 0x30="EU", 0x31="SPN", 0x32="FR", 0x40="JPN", 0x41="JPN") |
| Write |  | t_word |  | l_serv |  | Sets the region code for WLAN adapter (0x10="US", 0x20="CA", 0x30="EU", 0x31="SPN", 0x32="FR", 0x40="JPN", 0x41="JPN") |

CONF_MULTICAST_GROUP_IP_STR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01b4 |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the multicast group address |
| Write |  | p_string |  | l_serv |  | set the multicast group address (range: 224.0.0.10 .. 239.255.255.255) |

CONF_MULTICAST_GROUP_IP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01b1 |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | read the multicast group address |
| Write |  | t_dword |  | l_serv |  | set the multicast group address (range: 224.1.0.0 .. 239.255.255.255) |

CONF_MULTICAST_MPEG4_PORT_STR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0288 |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the mpeg4 multicast UDP port number |
| Write |  | p_string |  | l_serv |  | set the multicast video mpeg 4 UDP port (even port numbers only) |

CONF_MULTICAST_MPEG4_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0286 |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | read the mpeg4 multicast UDP port number |
| Write |  | t_word |  | l_serv |  | set the multicast video mpeg 4 UDP port (even port numbers only) |

CONF_MULTICAST_AUDIO_PORT_STR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01b5 |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the g711 multicast UDP port number |
| Write |  | p_string |  | l_serv |  | set the multicast audio G711 UDP port (even port numbers only) |

CONF_MULTICAST_AUDIO_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01b2 |  | coder instance |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | read the g711 multicast UDP port number |
| Write |  | t_word |  | l_serv |  | set the multicast audio G711 UDP port (even port numbers only) |

CONF_MULTICAST_TTL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0267 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | get the TTL (time to live) in IP-Header for multicast packets |
| Write |  | t_octet |  | l_serv |  | set the TTL (time to live) in IP-Header for multicast packets |

CONF_IGMP_VERSION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e5 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | read the igmp(internet group management protocol) version (0: Automatic from network; 1: Version1; 2: Version2; 3: Version3) |
| Write |  | t_octet |  | l_serv |  | Set the igmp version (0: Automatic from network; 1: Version1; 2: Version2; 3: Version3). Reboot necessary. |

CONF_STREAMING_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01b9 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | =0: set multicast streaming mode to off; =1: set multicast streaming mode mpeg4 to on; =2: set multicast streaming mode mpeg2 to on; =3: set multicast streaming mode mpeg4+mpeg2 to on |
| Write |  | t_octet |  | l_serv |  | =0: set multicast streaming mode to off; =1: set multicast streaming mode mpeg4 to on; =2: set multicast streaming mode mpeg2 to on; =3: set multicast streaming mode mpeg4+mpeg2 to on |

CONF_VIDEO_ENC_STREAMING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x099a |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | video streaming on coder (video encoder n: coderbits=1<<(n-1)) |
| Write |  | t_dword |  | l_serv |  | enable video streaming on coder. (video encoder n: coderbits=1<<(n-1)) |

CONF_AUDIO_ENC_STREAMING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x099b |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | audio streaming on coder (audio encoder n: coderbits=1<<(n-1)) |
| Write |  | t_dword |  | l_serv |  | enable audio streaming on coder (audio encoder n: coderbits=1<<(n-1)) |

CONF_JOIN_STREAM_NOW

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x01d4 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | void |  | noprot |  | not supported |
| Write |  | flag |  | l_live |  | start joining a multicast stream from the alarm IP |

CONF_DYNDNS_SERVER

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x030f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | IP address of VCS dynamic DNS server |
| Write |  | t_dword |  | l_serv |  | IP address of VCS dynamic DNS server |

CONF_DYNDNS_TIMEOUT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0310 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | time in sec when the VJ should retrigger its VCS dynamic server registration (30 .. 86400) |
| Write |  | t_dword |  | l_serv |  | time in sec when the VJ should retrigger its VCS dynamic server registration (30 .. 86400) |

CONF_DYNDNS_SERVER_REPLY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0311 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | not supported; will generate message when server answers |
| Write |  | p_string |  | l_serv |  | not supported; will generate message when server answers |

CONF_DYNDNS_HOST_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a56 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | l_serv |  | read the dyndns host name that is to be registered at dyndns.com |
| Write |  | p_string |  | l_serv |  | write the dyndns host name that is to be registered at dyndns.com |

CONF_DYNDNS_USER_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a57 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | l_serv |  | read the user name of account at dyndns.com |
| Write |  | p_string |  | l_serv |  | write the user name of account at dyndns.com |

CONF_DYNDNS_PASSWORD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a58 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | l_serv |  | read the password of account at dyndns.com |
| Write |  | p_string |  | l_serv |  | write the password of account at dyndns.com |

CONF_DYNDNS_ENABLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a59 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | 1: enable, 0: disable registering at dyndns.com |
| Write |  | t_octet |  | l_serv |  | enable/disable registering at dyndns.com |

CONF_DYNDNS_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a5a |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | state of registering at dyndns.com, see detailed description |
| Write |  | % |  | l_serv |  | % |

Payload Structure

State 1 Byte |
8 |

State
the current state of the process of registering the device at dyndns.com
Values:

successfully updated |  | 0
updated with unchanged cfg |  | 1
dyndns username or password wrong |  | 2
not fully qualified domain name (e.g. not in form host.dyndns.org) |  | 3
wrong host name for this dyndns user account |  | 4
too many hosts in last update |  | 5
host name is blocked by dyndns for update abuse |  | 6
no user agent submitted or http method not permitted |  | 7
dyndns server error dns related |  | 8
dyndns server error maintenance related |  | 9
update not done due to misconfiguration |  | 252
fatal error during update process |  | 253
update in process |  | 254
switched off |  | 255

CONF_DYNDNS_LAST_REGISTER

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a5b |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | data of last successful registration at dyndns.com, 8 bytes, first DWORD: register time in secs since 2000, second DWORD: last registered IP |
| Write |  | p_octet |  | l_serv |  | data of last successful registration at dyndns.com, 8 bytes, first DWORD: register time in secs since 2000, second DWORD: last registered IP |

CONF_DYNDNS_FORCE_REGISTER_NOW

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a5c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | l_serv |  | writing forces registering at dyndns.com / reading checks if forcing is allowed (has not been done since bootup) |
| Write |  | t_octet |  | l_serv |  | writing forces registering at dyndns.com / reading checks if forcing is allowed (has not been done since bootup) |

CONF_AUTODETECT_REPLY_GROUP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0956 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the multicast group to which (when set) to VJ will listen for multicast autodetect requests |
| Write |  | t_dword |  | l_serv |  | set the multicast group to which (when set) to VJ will listen for multicast autodetect requests on port 1800; when set to an invalid multicast address, the default address of 225.86.67.83 is used |

CONF_UNSOLICITED_AUTODETECT_REPLY_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0957 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the time in seconds, when the VJ shall send out unsolicited autodetect reply to the RCP port(off when set to 0) |
| Write |  | t_dword |  | l_serv |  | set the time in seconds, when the VJ shall send out unsolicited autodetect reply to port 1800 (off when set to 0); uses broadcast, and multicast if AUTODETECT_REPLY_GROUP is set |

CONF_DISCOVER_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0976 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | get the discover port |
| Write |  | t_word |  | l_serv |  | set the discover port |

CONF_LOCAL_HTTP_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0954 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | get the local HTTP port for browser access |
| Write |  | t_word |  | l_serv |  | set the local HTTP port for browser access (NOTE: it is not allowed to turn both, HTTP and HTTPS, of at the same time) |

CONF_LOCAL_HTTPS_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a0e |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | get the local HTTPS port for browser access |
| Write |  | t_word |  | l_serv |  | set the local HTTPS port for browser access (NOTE: it is not allowed to turn both, HTTP and HTTPS, of at the same time) |

CONF_RCP_SERVER_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a17 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | get the local RCP server TCP port number |
| Write |  | t_word |  | l_serv |  | set the local RCP server TCP port number, allowed: 0 or 1756 (Reboot necessary) |

CONF_TELNET_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a18 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | get the local Telnet TCP port number |
| Write |  | t_word |  | l_serv |  | set the local Telnet TCP port number, allowed: 0 or 23 (Reboot necessary) |

CONF_RTSP_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a63 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | reads the LocalRtspPort |
| Write |  | t_dword |  | l_serv |  | sets the local Rtsp port (0: Rtsp off) |

CONF_ENABLE_UPNP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ade |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flags |  | noprot |  | 0: Upnp disabled; 1: Upnp enabled |
| Write |  | flag |  | l_serv |  | 0: Upnp disabled; 1: Upnp enabled |

CONF_DHCP_VAL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x00af |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | read the DHCP state (0=OFF, 1=ON); |
| Write |  | t_octet |  | l_serv |  | set DHCP ip configuration value (0=OFF, 1=ON, 2=ON, but do not kick mechanism now) |

CONF_DHCP_ON

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x00ad |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | read the DHCP ON state |
| Write |  | f_flag |  | l_serv |  | enable DHCP ip configuration |

CONF_DHCP_OFF

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x00ae |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | f_flag |  | noprot |  | read the DHCP OFF state |
| Write |  | f_flag |  | l_serv |  | disable DHCP ip configuration |

CONF_DHCP_STABLE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ac8 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | read whether DHCP machine is in possession of an IP |
| Write |  | % |  | l_serv |  | % |

CONF_DHCP_COMPLIANCY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ada |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | mode of dhcp operation, 0: use of last-assigned ip during non-available dhcp server allowed; 1: no fallback ips used, more compliant to rfc 2131 |
| Write |  | t_octet |  | l_serv |  | mode of dhcp operation, 0: use of last-assigned ip during non-available dhcp server allowed; 1: no fallback ips used, more compliant to rfc 2131 |

CONF_SNMP_SRV_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a25 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | Read the snmp server port |
| Write |  | t_word |  | l_serv |  | Set the snmp server port (reset nescessary) |

CONF_SNMP_TRAPS_HOST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x00b6 |  | yes |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | void |  | noprot |  | not supported |
| Write |  | void |  | l_serv |  | not documented |

CONF_SNMP_TRAPS_HOST_STR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x00b7 |  | yes |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | void |  | noprot |  | not documented |
| Write |  | void |  | l_serv |  | not documented |

CONF_NBR_OF_TRAPS_HOSTS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x029d |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | Number of hosts snmp traps can be sent to |
| Write |  | t_dword |  | l_serv |  | read only |

CONF_SNMP_TRAP_LIST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a11 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | List of commands to be posted as snmp trap. See detailed description. |
| Write |  | p_octet |  | l_serv |  | List of commands to be posted as snmp trap. see detailed description |

Payload Structure

Trap Descriptor 1 4 Bytes
N x 4 Bytes | Trap Descriptor N 4 Bytes ...

Trap Descriptor 1 - N
Sequence of:

16 | 32
RCP Message Code 2 Bytes | Flags 2 Bytes
8 | 24 |

RCP Msg Code
The code of the RCP message that is to be forwarded as SNMP trap.
Flags
Values:

SNMP_TRAP_ENABLED |  | 1

CONF_PMPP_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aba |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | gets the Pmpp Port of the Pmpp server(0: off) |
| Write |  | t_word |  | l_serv |  | sets the Pmpp Port of the pmpp server(0: off) |

CONF_PMPP_ADDRESS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ab9 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | gets the Pmpp Address (allowed values: 1-63;) |
| Write |  | t_octet |  | l_serv |  | sets the Pmpp Address (allowed values: 1-63;) |

CONF_SYSCONTACT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x00ba |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the system contact required in SNMP |
| Write |  | p_string |  | l_serv |  | write the system contact required in SNMP |

CONF_SYSLOCATION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x00bb |  | no |  | no |  | yes |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | read the system location required in SNMP |
| Write |  | p_string |  | l_serv |  | write the system location required in SNMP |

CONF_ISCSI_IP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09aa |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | deprecated in fw > 4.00 |
| Write |  | t_dword |  | l_serv |  | deprecated in fw > 4.00 |

CONF_ISCSI_PORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ab |  | yes (since fw > 4.00) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_word |  | noprot |  | numdes 0: connect port, 1: tunnel port, 2: server port |
| Write |  | t_word |  | l_serv |  | numdes 0: connect port, 1: tunnel port, 2: server port |

CONF_ISCSI_LUN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ac |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | deprecated in fw > 4.00 |
| Write |  | t_dword |  | l_serv |  | deprecated in fw > 4.00 |

CONF_ISCSI_TARGET_IDX

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09f9 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | deprecated in fw > 4.00 |
| Write |  | t_dword |  | l_serv |  | deprecated in fw > 4.00 |

CONF_ISCSI_TARGET

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ad |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | gets the iscsi target name string |
| Write |  | p_string |  | l_serv |  | deprecated in fw > 4.00 |

CONF_ISCSI_TCP_CONNECTIONS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ae |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the number of concurrent tcp connections to iscsi target |
| Write |  | t_dword |  | l_serv |  | set the number of concurrent tcp connections to iscsi target |

CONF_ISCSI_DISCOVERY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09cc |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | performs a discovery and returns the result in an XML-like string; parameter ip (DWORD) and pwd string (64 char) structure in p_octet |
| Write |  | void |  | l_serv |  | not supported |

CONF_ISCSI_TARGET_PWD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09ce |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | l_user |  | set the password to authenticate at the iSCSI server. FW version >= 4.00: This command sets the password of the first entry of the CONF_ISCSI_AUTH list. If all characters of the string are the '*', the old stored value is not replaced. deprecated! use CONF_ISCSI_AUTH |
| Write |  | p_string |  | l_serv |  | get the password to authenticate at the iSCSI server. FW version >= 4.00: This command returns the password of the first entry of the CONF_ISCSI_AUTH list. deprecated! use CONF_ISCSI_AUTH |

CONF_ISCSI_LOCK_OVERRIDE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d2 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | see detailed description |
| Write |  | p_string |  | l_serv |  | see detailed description |

Payload
A String with the following structure - ip_addr:target_idx:lun
This string identifies the iscsi lun on which the lock is to be overwritten. This option clears its value after a successful override.
Note
The datatype of this command was FLAG and changed to STRING with fw 2.50
CONF_ISCSI_LOCK_RELEASE_ON_LEAVE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e4 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | returns wheather the next iSCSI logout should use the release action |
| Write |  | flag |  | l_serv |  | advices the iSCSI initiator to release a lock at the target lun when the storage medium transitions away from iSCSI; this option clears its value after a successful release |

CONF_ISCSI_INITIATOR_NAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d8 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | returns the used initiator name; only applicable when iSCSI is connected |
| Write |  | void |  | l_serv |  | not supported |

CONF_ISCSI_INITIATOR_NAME_EXTENTION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d9 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | returns the used initiator name extention; used for identification only |
| Write |  | p_string |  | l_serv |  | set the used initiator name extention; used for identification only |

CONF_ISCSI_SERVER_STATE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a2b |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the state of the iscsi server (0: server down, 1: server running) |
| Write |  | t_dword |  | l_serv |  | set the iscsi server state (0: shutdown server, 1: start server) |

NOTE
The iscsi server is also started or stopped when you write the command CONF_STORAGE_LIST. If the storage list is empty or only contains entries with the 'iSCSI export' field set to 'For local use only' (0x00), the server is stopped if it is running cause no targets and luns would be provided. If the list contains at least one entry with the 'iSCSI export' field set to 'Make storage available through iSCSI' (0x01), the server is started, if not already running, to provide the iscsi service.
CONF_ISCSI_MNI

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aa0 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | monitor iscsi targets. |
| Write |  | p_octet |  | l_serv |  | monitor iscsi targets. |

Request Payload Structure
Sequence of (max 64):

16 | 32
Target Descriptor 28 Bytes ...
8 | 24 |

Target Descriptor

16 | 32
Target Address 8 Bytes ...
Action 1 Bytes | Reserved 3 Byte
Reserved 16 Bytes ...
8 | 24 |
Target Address
16 | 32
Target IP 4 Bytes
Target Index 1 Byte | Reserved 3 Bytes
8 | 24 |
Action Values:
DELETE |  | 0x00
ADD |  | 0x01

Response Payload Structure
Sequence of (max 64):

16 | 32
Target Descriptor 28 Bytes ...
8 | 24 |

Target Descriptor

16 | 32
Target Address 8 Bytes ...
Action 1 Byte | Status 1 Byte | Error 1 Byte | Reserved 1 Byte
Starttime 4 Bytes
Session Status 1 Byte | Session Error 1 Byte | Reconnects 2 Byte
Reserved 4 Bytes
Uptime 4 Bytes
8 | 24 |
Target Address See request packet for details. Action The value of the request packet. Zero in messages. Status Values:
FAIL |  | 0x00
SUCCESS |  | 0x01
Error Values:
ISCSI_MNI_ERR_INV_TARG |  | 0x01
ISCSI_MNI_ERR_FULL |  | 0x02
ISCSI_MNI_ERR_TARG_PRES |  | 0x03
ISCSI_MNI_ERR_NOT_FOUND |  | 0x04
ISCSI_MNI_ERR_INTERN |  | 0x05
When an action request fails, this error field is set. On success or messages, this fild is zero. ISCSI_MNI_ERR_INV_TARG - if the assigned target address is invalid (e.g. zero). ISCSI_MNI_ERR_FULL - if the maxium of 64 iscsi targets is reached and a request packet with the ADD action was sent. ISCSI_MNI_ERR_TARG_PRES - if a request packet if the ADD action was sent and the target address is already monitored. ISCSI_MNI_ERR_NOT_FOUND - if a request packet if the DELETE action was sent and the target address is not currently monitored. Target IP The ip address of the iscsi target. Target Index The index of the iscsi target. Starttime The time when the monitoring process was started (in seconds since 2000). Session Status Values:
OFFLINE |  | 0x00
ONLINE |  | 0x01
ERROR |  | 0x02
Session Error Values:
ISCSI_ERR_CONNECT |  | 0x31
ISCSI_ERR_LOGIN |  | 0x34
ISCSI_ERR_INV_TARG_IDX |  | 0x35
ISCSI_ERR_PWD |  | 0x36
ISCSI_ERR_PROTO |  | 0x37
ISCSI_ERR_TARG_NOT_REACH |  | 0x38
ISCSI_ERR_NO_MEM |  | 0x3a
ISCSI_ERR_SESS_CREATE |  | 0x3b
ISCSI_ERR_INV_PARAMS |  | 0x3c
ISCSI_ERR_SESS_NOT_FOUND |  | 0x3d
ISCSI_ERR_DISCONN |  | 0x3e
ISCSI_ERR_TIMEOUT |  | 0x3f
ISCSI_ERR_SOCK |  | 0x5f
ISCSI_SOCK_CLOSED |  | 0x7f
ISCSI_ERR_TCP_CONN_RST |  | 0x8f
ISCSI_ERR_IP_ZERO |  | 0xa0
Reconnects The number of times the session was reconnected since the begin of the monitoring process. Uptime The number of seconds the session is online.

Use this command to monitor iscsi targets.
If you write this command, all the targets of the request packets are added/delete to the current monitoring list.
If you read this command, you will get the description of all currently monitored iscsi targets in the response packet.
Every time the status of a monitored target changes, a message is sent out with the current status of this target.
CONF_ISCSI_AUTH

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ab0 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | l_user |  | see detailed description |
| Write |  | p_octet |  | l_serv |  | see detailed description |

Payload Structure
Sequence of (BVIP enc/dec: 2, generic_dll: 8):

16 | 32
Authentication Descriptor 140 Bytes ...
8 | 24 |

Authentication Descriptor

16 | 32
Target Address 8 Bytes ...
Type 4 Bytes
Params 128 Bytes ...
8 | 24 |
Target Address The address of the iscsi target. If this field is set to zero, it is used as the default entry for authenticaion.
16 | 32
Target IP 4 Bytes
Target Index 1 Byte | Reserved 3 Bytes
8 | 24 |
Target IP The ip address of the iscsi target. If this field is set to -1 (0xFFFFFFFF), this descriptor is used for all remaining iscsi ips, for that no explicit descriptor is provided (default). Target Index The target index of the iscsi target. If this field is set to -1 (0xFF), this descriptor is used for all remaining iscsi targets with the same ip, for that no explicit descriptor is provided (default). NOTE For an iscsi session, all authentication descriptors are searched for the target address. If this address is found, the authentication information is used. If that descriptor is not found, but the array contains a descriptor with the same ip and the target index set to default (0xFF), the information in this record is used instead. If that descriptor is not found, but the array contains an descriptor with the ip address set to default (0xFFFFFFFF), the information in this record is used instead. If that descriptor is not found, no authentication will be performed for that iscsi session.
Type Values:
NONE |  | 0
CHAP |  | 1
Params
Type = CHAP.
16 | 32
User 64 Bytes ...
Password 64 Bytes ...
8 | 24 |
User The CHAP user name that is used for authentication. Password The CHAP password that is used for authentication. NOTE On a read command, the characters of the password are replaced by the '*'. On a write command, the password is only stored, if not all characters equal the '*' sign. Otherwise the old stored value is retained.

CONF_HD_MAX_NUMBER_OF_PARTITIONS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0900 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | obsolete (always 1 now for devices with video in) |
| Write |  | void |  | l_user |  | not supported |

CONF_HD_MAX_SLICES_PER_TRACK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x090a |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the max number of time slices in a track |
| Write |  | void |  | l_user |  | not supported |

CONF_HD_MAX_ALARM_TRACKS_PER_PARTITION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0919 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get max number of alarm tracks for one partition |
| Write |  | void |  | l_user |  | not supported |

CONF_HD_PARTITIONS_RECORDING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x091a |  | yes (1 - primary recording ,2 - secondary recording) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | list of numbers of partitions (DWORDS) or cams in case of span recording with running recording |
| Write |  | void |  | l_user |  | not supported |

CONF_HD_PARTITION_RECORDING

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a03 |  | yes (partition or cam for span recording) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | recording status of partition or cam if span recording for primary recording (1 = running, 0 = not running) |
| Write |  | t_dword |  | l_user |  | not supported |

CONF_HD_PARTITION_RECORDING_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a4d |  | yes (partition or cam for span recording) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | recording status of this cam for secondary recording (1 = running, 0 = not running) |
| Write |  | t_dword |  | l_user |  | not supported |

CONF_HD_PARTITION_FILE_INFO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0901 |  | partition |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | void |  | l_user |  | not supported |

Payload Structure (sequence of)

16 | 32
Start Time 4 Bytes
Stop Time 4 Bytes
Flags 32 Bits
File ID 4 Bytes
8 | 24 |

Start Time
Seconds since 2000.
Stop Time
Seconds since 2000.
Flags
Values:

Bit 0 |  | Recording Runing (actual recording is running on this file or recording not closed regulary)
Bit 1 |  | Recording Overwriting (recording takes place in a ring and old recording data will be overwritten)
Bit 2 |  | Alarm Input (there are input alarms in this file)
Bit 3 |  | Alarm Motion (there are motion alarms in this file)
Bit 4 |  | New Alarm (only file info message)
Bit 5 |  | Video Loss (there are video loss in this file)
Bit 6 |  | Time Recording (changed semantic from earlier versions)
Bit 7 |  | Alarm Recording (changed semantic from earlier versions)
Bit 8-15 |  | Track Fill Level (fill level in percent, always 100 % on filled ring recording)
Bit 16 |  | Alarm Remote (there are virtual/remote alarms in this file, see CONF_HD_MGR_SIGNAL_ALARM)
Bit 17 |  | pre alarm recording ring (not relevant for file info msg)
Bit 18-20 |  | Reserved
Bit 21 |  | Offline (VRM only)
Bit 22 |  | Protected (VRM only)
Bit 23-28 |  | Time Zone (Quarter hours)
Bit 29 |  | Time Zone Sign
Bit 30-31 |  | Reserved

NOTE: If this command is used get to file information on a span formated disk, the Session ID paramter must be set (a connect primitive must have been preceded). The num paramter (partition) has no meaning then, since a span has always only one partition. Alarm Recording und Time Recording flags changed semantic Alarm Recording flag marks a file that includes a pre alarm recording configured by a pre alarm time in the recording profiles, Time Recording flag marks the the files including normal time recording and/or post alarm. That means a closed File including pre and post alarm recordings will always have alarm and time recording flag set.
CONF_HD_PARTITION_PROP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x090b |  | yes (partition or cam if span recording mode) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | obsolete |
| Write |  | p_octet |  | l_serv |  | (obsolete) see detailed description (effect takes place on next mounted span) (video type is obsolete, depends on CONF_CODER_VIDEO_TYPE_RESTRICTION settings) |

Payload Structure

Number 4 Bytes
Char 1 1 Byte | 62 x 1 Byte | Char 64 1 Byte
Total Size 4 Bytes
Reserved 4 Bytes
Video Type 1 Byte | Reserved 1 Byte | Storage Type 1 Byte | Enc. Preset 1 Byte
Number Of Alarm Tracks (obsolete) 4 Bytes
Size Of Alarm Track (obsolete) 4 Bytes
Video input channel 4 Bytes
Encoder index 1 Byte | Reserved 3 Bytes
Reserved 32 Bytes ...

Char 1 - 64
Name of the partition (obsolete).
Size (obsolete)
In Megabyte
Video Type (obsolete, depends on CONF_CODER_VIDEO_TYPE_RESTRICTION settings)
Values:

No |  | 0x00
Mpeg2 |  | 0x01
Mpeg4 |  | 0x03
H264 |  | 0x04

Storage Type (obsolete)
Values:

Linear |  | 0x00
Ring |  | 0x01

Enc. Preset
Number of the encoder preset 1 - 8. (obsolete here, can bet set in the recording profiles)
Size Of Alarm Track (obsolete)
In Megabytes.
Video input channel
Bitfield of used video channels (Bit0=channel 1...).
Encoder index
Number of the encoder instance. (obsolete here, can bet set in the recording profiles)
CONF_HD_PARTITION_PROP for Span Recording
This command cannot be set while the recording is running.
CONF_HD_PARTITION_PROP_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a4e |  | yes (cam) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | obsolete, payload as in CONF_HD_PARTITION_PROP |
| Write |  | p_octet |  | l_serv |  | (obsolete)partition properties for secondary recording( effect takes place on next mounted span), payload is the same as the command CONF_HD_PARTITION_PROP |

CONF_HD_SIZE_MB

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x090c |  | yes (0: default pm, >0: storage medium type) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | read the total size of a local storage in megabytes |
| Write |  | - |  | l_serv |  | not writable |

CONF_HD_PARTITION_GEO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x090d |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | obsolete |
| Write |  | p_octet |  | l_serv |  | obsolete |

CONF_HD_RECORD_SCHEDULE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a0b |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read primary recording schedule, see detailed description |
| Write |  | p_octet |  | l_serv |  | set primary recording schedule(effect takes place imidiately), see detailed description |

Payload Structure

Sat. 1 4 Bits | 94 x 4 Bits | Sat. 96 4 Bits | Sun. 1 4 Bits | 94 x 4 Bits | Sun. 96 4 Bits
Mon. 1 4 Bits | 94 x 4 Bits | Mon. 96 4 Bits | Tue. 1 4 Bits | 94 x 4 Bits | Tue. 96 4 Bits
Wed. 1 4 Bits | 94 x 4 Bits | Wed. 96 4 Bits | Thu. 1 4 Bits | 94 x 4 Bits | Thu. 96 4 Bits
Fri. 1 4 Bits | 94 x 4 Bits | Fri. 96 4 Bits |

Sat. 1 - 96
96 entries of recording profile numbers for Saturday, each represents the recording profile for a 15 min time period. First entry is from 00:00 to 00:15. The following entries are for the following 15 min time periods until 24:00.
Values:

recording off |  | 0
recording profile numbers |  | 1-10

Sun. 1 - 96
96 entries of recording profile numbers for Sun.
Mon. 1 - 96
96 entries of recording profile numbers for Mon.
Tue. 1 - 96
96 entries of recording profile numbers for Tue.
Wed. 1 - 96
96 entries of recording profile numbers for Wed.
Thu. 1 - 96
96 entries of recording profile numbers for Thu.
Fri. 1 - 96
96 entries of recording profile numbers for Fri.
HD_RECORD_SCHEDULE
This command reads/writes the recording schedule for all cameras (primary and secondary recording). The entries are 4 bit each and represent a recording profile for a 15 min time period(payload 336 bytes total). The recording profiles with same profile number can be different for each camera. See command HD_RECORD_PROFILES. The schedule will be written to the storage medium. In case of span recording mode (see CONF_RECORD_MODE_SPANS) the schedule will be only read from or stored in the config. This schedule is used as default schedule for each span that is mounted by this device for recording.
CONF_HD_RECORD_SCHEDULE_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a49 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | obsolete, only on global schedule for primary and secondary recording |
| Write |  | p_octet |  | l_serv |  | obsolete, only on global schedule for primary and secondary recording on all cams |

CONF_HD_RECORD_HOLIDAYS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a0c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read holiday schedule list for primary recording, see detailed description |
| Write |  | p_octet |  | l_serv |  | write holiday schedule list (effect takes place imidately), see detailed description |

Payload Structure

holiday schedule entry 1 52 Bytes ...
| N x 52 Bytes
holiday schedule entry N 52 Bytes ...

holiday schedule entry 1 - N
schedule entry specifing a holiday and it's recording schedule. max. 25 entries.
CONF_HD_RECORD_HOLIDAYS
This command reads/writes the Holiday table for the primary recording. On holidays the recording uses the special schedule instead of the standard schedule. The table contains N entries (max. 25) each entry specifies one or more holidays in a row followd by a recording schedule. the payload sends only valid holiday entries, so the size of N depends on the number of valid entries in the table.
Holiday Schedule Entry Structure

day 1 Byte | month 1 Byte | year 1 Byte | number of days 1 Byte
reco 1 4 Bits | 94 x 4 Bits | reco 96 4 Bits |

day
day of the month, which is a holiday
Values:

invalid |  | 0
day of the month |  | 1 - 31

month
month of the year
Values:

invalid |  | 0
jan |  | 1
feb to nov |  | 2 - 11
dec |  | 12

year
year since 2000
Values:

year 2000 to 2255 |  | 0 - 255

number of days
number of days that follow the specified holiday, which are also scheduled as holidays. If only the specified date is the holiday, this field should be set to 1.
Values:

invalid |  | 0
number of days |  | 1 - 255

record schedule 1 - 96
this is the recocording schedule containing 96 entries of recording profile numbers for the holiday, each represents the recording profile for a 15 min time period. First entry is from 00:00 to 00:15. The following entries are for the following 15 min time periods until 24:00.
Values:

recording off |  | 0
recording profile numbers |  | 1 -10

CONF_HD_RECORD_PROFILES

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a0d |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read recording profiles, see detailed description |
| Write |  | p_octet |  | l_serv |  | set recording profiles (effect takes place imidiatly), see detailed description |

Payload Structure

Recording Profile 1 56 Bytes ...
8 x 56 Bytes | Recording Profile 10 56 Bytes ...

Recording Profile 1 - 10
10 recording profiles for the cammera specified by the num parameter, see detailed description for a recording profile
HD_RECORD_PROFILES
Read/Write the ten recording profiles for a camera, payload 560 bytes total. The profiles will be written to the storage medium. In case of ram recording (see CONF_STORAGE_MEDIUM_TYPE), the profiles will be also stored in the config and will be used as default profiles for future ram recordings. In case of span recording mode (see CONF_RECORD_MODE_SPANS) the profiles will be only read from or stored in the config. These profiles are used as default profiles for each span that is mounted by this cam for span recording.
recording profile structure

16 | 32
flags 8 Bits | video preset nr 1 Byte | post alarm video preset nr 1 Byte | encoder index 1 Byte
intra only 1 Byte | intra only qual post alarm 1 Byte | profile name 34 Bytes ...
...
...
...
...
...
...
...
... 34 Bytes
pre alarm time 2 Byte | post alarm time 2 Byte
motion alarm 4 Bytes
alarm input and remote alarm 4 Bytes
video loss alarm 4 Bytes
8 | 24 |

flags
Flags:

ALARM_RECORDING |  | 0x01 |  | flag for alarm recording, if set alarm recording on the alarm tracks will be active
AUDIO_RECORDING_DISABLE |  | 0x02 |  | flag for audio recording, if set audio will be disabled for recording
META_RECORDING_DISABLE |  | 0x04 |  | flag for meta recording, if set meta will be disabled for recording

video preset nr
video preset number used for recording
Values:

no recording on this profile |  | 0
video preset nr |  | 1 - 8

post alarm video preset nr
video preset number used for recording after occurence of an alarm
Values:

not set, uses video preset nr if set |  | 0
video preset nr for post alarm |  | 1 - 8

encoder index
index of the encoder stream starting with 0
intra only recording
for intra only recording, not supported by all devices
intra only recording quality post alarm
for intra only recording, qualitty after ocurrence of an alarm, not supported by all devices
profile name
profile name is a zero terminated string
pre alarm time
only relevant for alarm recording, if set, this time in seconds is the time the recording will be stored up to the alarm event
post alarm time
if set, this time in seconds is the time after an alarm event for that the post alarm video preset is used if set. After this time elapses, the recording will return to the standard video preset nr, if alarm recording, the recording will also stop the recording on the actual track and start a new one
motion alarm
The bits represents the activation. Bit 0 <-> Alarm Nbr. 0; Bit 1 <-> Alarm Nbr. 1; ... ... ; Bit 31 <-> Alarm Nbr. 31
alarm input and remote alarm
The bits represents the activation. Bit 0 <-> Alarm Nbr. 0; Bit 1 <-> Alarm Nbr. 1; ... ... ; Bit 27 <-> Alarm Nbr. 27 for alarm inputs, Bit 28 <-> Virt. Alarm Nbr. 3; ... ... ; Bit 31 <-> Virt. Alarm Nbr. 0 (reverse order) for virtual alarms caused by rcp command CONF_VIRTUAL_ALARM_STATE
video loss alarm
The bits represents the activation. Bit 0 <-> Alarm Nbr. 0; Bit 1 <-> Alarm Nbr. 1; ... ... ; Bit 31 <-> Alarm Nbr. 31
CONF_HD_RECORD_PROFILES_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a91 |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read recording profiles for secondary recording, payload is the same as in CONF_HD_RECORD_PROFILES |
| Write |  | p_octet |  | l_serv |  | set recording profiles for secondary recording (effect takes place imidiatly) , payload is the same as in CONF_HD_RECORD_PROFILES |

CONF_HD_RECORD_PROFILES_V2

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ad0 |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read recording profiles |
| Write |  | p_octet |  | l_serv |  | write recording profiles |

Payload Structure

Recording Profile 1 56 Bytes ...
8 x 56 Bytes | Recording Profile 10 56 Bytes ...

Recording Profile 1 - 10
10 recording profiles for the cammera specified by the num parameter, see detailed description for a recording profile
HD_RECORD_PROFILES_V2
Read/Write the ten recording profiles for a camera, payload 560 bytes total. The profiles will be written to the device configuration. These profiles are used as default profiles for each span that is mounted by this cam for span recording.
recording profile structure

16 | 32
flags 8 Bits | stream config nr 1 Byte | post alarm stream config nr 1 Byte | encoder index 1 Byte
post alarm profile 1 Byte | reserved 1 Byte | profile name 34 Bytes ...
...
...
...
...
...
...
...
... 34 Bytes
pre alarm time 2 Byte | post alarm time 2 Byte
motion alarm 4 Bytes
alarm input and remote alarm 4 Bytes
video loss alarm 4 Bytes
8 | 24 |

flags
Flags:

ALARM_RECORDING |  | 0x01 |  | flag for alarm recording, if set alarm recording on the alarm tracks will be active
AUDIO_RECORDING_DISABLE |  | 0x02 |  | flag for audio recording, if set audio will be disabled for recording
META_RECORDING_DISABLE |  | 0x04 |  | flag for meta recording, if set meta will be disabled for recording

stream config nr
stream configuration number used for recording
Values:

no recording on this profile |  | 0
stream configuration nr for pre alarm |  | 1 - 2

post alarm stream config nr
stream configuration used for recording after occurence of an alarm
Values:

not set, uses stream config nr if set |  | 0
stream configuraton nr for post alarm |  | 1 - 2

encoder index
index of the encoder stream starting with 0
post alarm profile
encoder profile for postalarm, only some values of the profile will be used to modify the uses encoder profile for the post alarm stream
Values:

not set, no modification of the actual enc profile |  | 0
encoder profile nr for post alarm configuration |  | 1 - 8

profile name
profile name is a zero terminated string
pre alarm time
only relevant for alarm recording, if set, this time in seconds is the time the recording will be stored up to the alarm event
post alarm time
if set, this time in seconds is the time after an alarm event for that the post alarm video preset is used if set. After this time elapses, the recording will return to the standard video preset nr, if alarm recording, the recording will also stop the recording on the actual track and start a new one
motion alarm
The bits represents the activation. Bit 0 <-> Alarm Nbr. 0; Bit 1 <-> Alarm Nbr. 1; ... ... ; Bit 31 <-> Alarm Nbr. 31
alarm input and remote alarm
The bits represents the activation. Bit 0 <-> Alarm Nbr. 0; Bit 1 <-> Alarm Nbr. 1; ... ... ; Bit 27 <-> Alarm Nbr. 27 for alarm inputs, Bit 28 <-> Virt. Alarm Nbr. 3; ... ... ; Bit 31 <-> Virt. Alarm Nbr. 0 (reverse order) for virtual alarms caused by rcp command CONF_VIRTUAL_ALARM_STATE
video loss alarm
The bits represents the activation. Bit 0 <-> Alarm Nbr. 0; Bit 1 <-> Alarm Nbr. 1; ... ... ; Bit 31 <-> Alarm Nbr. 31
CONF_HD_RECORD_PROFILES_V2_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ad1 |  | cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get recording profiles for secondary recording, payload is the same as in CONF_HD_RECORD_PROFILES_V2 |
| Write |  | p_octet |  | l_serv |  | set recording profiles for secondary recording, payload is the same as in CONF_HD_RECORD_PROFILES_V2 |

CONF_HD_ALARM_MOTION

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0916 |  | yes (partition) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | alarm motion - obsolete |
| Write |  | flag |  | l_serv |  | write alarm motion - obsolete |

CONF_HD_ALARM_INPUT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0917 |  | yes (partition) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | alarm input - obsolete |
| Write |  | flag |  | l_serv |  | write alarm input - obsolete |

CONF_HD_MGR_START

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0913 |  | yes (partition or cam) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | return TRUE when manager is on or when primary span recording is on and device is in span recording mode |
| Write |  | flag |  | l_serv |  | start the recording manager. Can cause recording if time/alarm recording selected. If in span recording mode the set span recording to on. |

CONF_HD_MGR_START_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a46 |  | yes (partition or cam) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | return TRUE when secondary span recording is on and device is in span recording mode |
| Write |  | flag |  | l_serv |  | start the recording manager. Can cause recording if time/alarm recording selected. If in span recording mode the set span recording to on. |

CONF_HD_MGR_STOP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0914 |  | partition or cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | return TRUE when manager is off or when primary span recording is off and device is in span recording mode |
| Write |  | flag |  | l_serv |  | stop/start the recording manager and set config to primary recording off:1/on:0. |

CONF_HD_MGR_STOP_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a47 |  | partition or cam |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | return TRUE when secondary span recording is off |
| Write |  | flag |  | l_serv |  | stop/start the recording manager and set config to secondary recording off:1/on:0. |

CONF_HD_MPEG4_ACTIVE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x093c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | (obsolete) signals an active hdd MPEG4 partition |
| Write |  | - |  | l_serv |  | not supported |

CONF_HD_RECORDING_REPORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a1c |  | yes (cam) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get recording report from actual primary recording on a cam, |
| Write |  | p_octet |  | l_serv |  | not supported |

This comand reads the recording report of an actual running recording of a cam. The recording report contains information about RTP and VDP packets as well as VDP allocation of a running recording. The cam is specified by the num parameter.
Version 1

16 | 32
start_counting_time 4 Bytes
VDP_allocation_no_wait 4 Bytes
VDP_allocation_wait 4 Bytes
VDP_allocation_failed 4 Bytes
8 | 24 |

start_counting_time
time, since when the VDP allocation counting was started, this should be the time when the recording had started or since the last clear of the report.
VDP_allocation_no_wait
number of allocated VDPs since start_counting_time without blocking
VDP_allocation_wait
number of allocated VDPs since start_counting_time with blocking a time
VDP_allocation_failed
number of VDPs that couldn't allocated, because waiting for the at the block pool timed out or failed. Means also an rtp packet had to be discarded.
Version 2

16 | 32
Version 1 Byte | Reserved 3 Bytes
Start Seconds 4 Bytes
Start Milliseconds 4 Bytes
VDP Allocation No Wait 4 Bytes
VDP Allocation Wait 4 Bytes
VDP Allocation Fail 4 Bytes
Encoder Data 48 Bytes ...
Storage Data 48 Bytes ...
Network Data 48 Bytes ...
Reserved 48 Bytes ...
8 | 24 |

Version
Version information.
Start Seconds
Timestamp in seconds since 2000 when the counting of recording data started.
Start Milliseconds
Milliseconds of the timestamp when the counting of recording data started.
VDP Allocation No Wait
Number of VDP allocation operation performed without waiting.
VDP Allocation Wait
Number of VDP allocation operation performed with waiting.
VDP Allocation Fail
Number of VDP allocation operation failed.
Encoder Data

16 | 32
Video RTP Packet Count 4 Bytes
Video Byte Count 4 Bytes
Reserved 4 Bytes
Audio RTP Packet Count 4 Bytes
Audio Byte Count 4 Bytes
Reserved 4 Bytes
Meta Packet Count 4 Bytes
Meta Byte Count 4 Bytes
Reserved 4 Bytes
Reserved 12 Bytes ...
8 | 24 |
Video RTP Packet Count Number of video RTP packets that are deliverd to the recording. Video Byte Count Number of video bytes that are deliverd to the recording. Audio RTP Packet Count Number of audio RTP packets that are delivered to the recording. Audio Byte Count Number of audio bytes that are deliverd to the recording. Meta RTP Packet Count Number of meta RTP packets that are delivered to the recording. Meta Byte Count Number of meta bytes that are deliverd to the recording.

Storage Data

16 | 32
(Video + Audio) VDP Packet Count 4 Bytes
(Video + Audio) Byte Count 4 Bytes
Reserved 4 Bytes
Audio VDP Packet Count 4 Bytes
Audio Byte Count 4 Bytes
Reserved 4 Bytes
Meta VDP Packet Count 4 Bytes
Meta Byte Count 4 Bytes
Reserved 4 Bytes
Reserved 12 Bytes ...
8 | 24 |
Video VDP Packet Count Number of video + audio VDP packets that are written to storage (since fw 4.0 there are vdp packets containing video and audio data mixed, these packets will be counted here and not in the "Audio VDP Packet Count" field). Video Byte Count Number of video + audio bytes that are written to storage (since fw 4.0 there are vdp packets containing video and audio data mixed, these packet bytes will be counted here and not in the "Audio Byte Count" field). Audio VDP Packet Count Number of audio VDP packets that are written to storage. Audio Byte Count Number of audio bytes that are written to storage. Meta Packet Count Number of meta VDP packets that are written to storage. Meta Byte Count Number of meta bytes that are written to storage.

Network Data

16 | 32
Bytes Read 4 Bytes
Bytes Write 4 Bytes
Reserved 40 Bytes ...
8 | 24 |
Bytes Read Number of Bytes that are read from storage. Bytes Write Number of Bytes that are written to storage.

CONF_HD_RECORDING_REPORT_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a4f |  | yes (cam) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get recording report from actual secondary recording on a cam, payload same as in command CONF_HD_RECORDING_REPORT |
| Write |  | p_octet |  | l_serv |  | not supported |

CONF_RECORDING_STATUS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a9b |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get the current recording status, |
| Write |  | p_octet |  | l_serv |  | not supported |

Request Structure

16 | 32
Camera 1 Byte | Recording Index 1 Byte | Reserved 50 Bytes ...
...
8 | 24 |

Camera
The camera index.
Recording Index
Values:

Primary |  | 1
Secondary |  | 2

Response Structure

16 | 32
Camera 1 Byte | Recording Index 1 Byte | Status 1 Byte | Error 1 Byte
Current Recording Span 8 Bytes ...
Reserved 4 Bytes
Datarate 4 Bytes
packet alloc no wait 4 Bytes
packet alloc wait 4 Bytes
packet alloc failed 4 Bytes
recent time period 4 Bytes
packets recorded high 4 Bytes
packets recorded low 4 Bytes
packets lost high 4 Bytes
packets lost low 4 Bytes
8 | 24 |

Camera
The camera index.
Recording Index
Values:

Primary |  | 1
Secondary |  | 2

Status
Values:

OFFLINE |  | 1
IDLE |  | 2
PEND |  | 3
RUNNING |  | 4
ERROR |  | 5

Error
See error codes of CONF_SPAN_USE_STATUS.
Current Recording Span
The address of the span the camera is recording to.

16 | 32
IP 4 Bytes
Target Index 1 Byte | Lun 1 Byte | Span Index 2 Byte
8 | 24 |
IP The ip address of the storage. Target Index In index of the iscsi target. Lun The lun indentifier. Span Index The index of the span.

Datarate
The datarate that is written to the storage.
packet alloc no wait
recently alloc no wait vdp packets (1.5 kbyte) since recent time period
packet alloc wait
recently alloc wait vdp packets (1.5 kbyte) since recent time period (indicates problems of the recording get its data to the drive)
packet alloc failed
recently alloc failed vdp packets (1.5 kbyte) since recent time period (indicates problems of the recording get its data to the drive, corrupt data stream)
recent time period
time period in which the packet allock counter were counted
packets recorded high
high part (32 bits network order) of a 64 bit counter for all recorded packets of this recording since device start up (packets counted by "packet alloc no wait" and "packet alloc wait" not included)
packets recorded low
low part (32 bits network order) of a 64 bit counter for all recorded packets of this recording since device start up (packets counted by "packet alloc no wait" and "packet alloc wait" not included)
packets lost high
high part (32 bits network order) of a 64 bit counter for all packets, which couldn't be recorded by this recording since device start up (packets counted by "packet alloc failed" not included)
packets lost low
low part (32 bits network order) of a 64 bit counter for all packets, which couldn't be recorded by this recording since device start up (packets counted by "packet alloc failed" not included)
CONF_RECORDING_RETENTION_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a30 |  | yes (camera) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the primary recording retention time for a camera (in seconds). |
| Write |  | t_dword |  | l_serv |  | set the primary recording retention time for a camera (in seconds). (effect takes place on next mounted span) |

CONF_RECORDING_RETENTION_TIME_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a48 |  | yes (camera) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the secondary recording retention time for a camera (in seconds). |
| Write |  | t_dword |  | l_serv |  | set the secondary recording retention time for a camera (in seconds). (effect takes place on next mounted span) |

CONF_REMOTE_REC_DEVICE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a85 |  | yes (max 8) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_string |  | noprot |  | Get the ip address of the remote recording device (max. 50 characters). |
| Write |  | p_string |  | l_serv |  | Set the ip address of a remote recording device (max. 50 characters). |

CONF_REC_MGNT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a89 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | Read the type of the recording management (0 = LOCAL, 1 = VRM, 2 = VRM+ANR, 3 = ONLY LOCAL, 4 = DUAL VRM) |
| Write |  | t_octet |  | l_serv |  | Set the type of the recording management (0 = LOCAL, 1 = VRM, 2 = VRM+ANR, 3 = ONLY LOCAL, 4 = DUAL VRM) (not possible to change settings while recording, changes will stop recording, clear span list and clear the deystination for local recording setting) |

CONF_HD_MGR_REC_STATUS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aae |  | yes (cam) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | p_octet |  | l_serv |  | not supported |

Payload Structure

16 | 32
rec state 1 Byte | rec preset 1 Byte | enc preset 1 Byte | flags 1 Byte
8 | 24 |

rec state
state of the recording, state OFF not in payload of msg
Values:

OFF |  | 0
NO RECORDING |  | 1
STAND BY |  | 2
PRE ALARM RECORDING |  | 3
ALARM RECORDING |  | 4
POST ALARM RECORDING |  | 5

rec preset
actual used recording preset from 1 to 10 or 0 if no preset is used
enc preset
actual used encoder preset from 1 to 8 or 0 if no preset is used
flags
these flags show the alarm states and the recording mode
Values:

alarm recording mode |  | 0x01
input alarm |  | 0x02
motion alarm |  | 0x04
video loss |  | 0x08
virtual alarm |  | 0x10
reserved for extension |  | 0x80

CONF_HD_MGR_REC_STATUS
This command shows the state for a recording. It can be read and it will be send at state changes. State changes are the change of rec state or rec preset only. Within the Msg there is no distiction between the state OFF and NO RECORDING. That means no msg will be send on the state change between this two states. The msg will never contain the state OFF but the read response maybe. OFF state means the recording is configured to off by set it to stop. NO RECORDING can be caused by many things e.g. no recording on the schedule, no storage present and so on. STAND BY means there is recording on the schedule but not at the moment. The recording scheduler waits for the time to start the recording. All the other states indicating a running recording.
CONF_HD_MGR_REC_STATUS_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aaf |  | yes (cam) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | same as CONF_HD_MGR_REC_STATUS but for secondary recording (see cmd CONF_HD_MGR_REC_STATUS) |
| Write |  | p_octet |  | l_serv |  | not supported |

CONF_HD_FILE_INFO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x091d |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | void |  | noprot |  | read not supported (only for messages), |
| Write |  | void |  | l_serv |  | not supported |

Payload Structure

16 | 32
start time 32 Bits
end time 32 Bits
flags 32 Bits
file id 32 Bits
span ip 4 Bytes
target idx 1 Byte | lun 1 Byte | span idx 16 Bits
cam 1 Byte | recording idx 1 Byte | reserved 2 Bytes
8 | 24 |

start time
start time in seconds since 2000 of the recording file
end time
end time in seconds since 2000 of the recording file
flags
file info flags, see CONF_HD_PARTITION_FILE_INFO
file id
File ID on the file unique per span
span ip
Span ip address
target idx
target index of the span
lun
lun of the span
span idx
span index
cam
camera from 1 to ...
recording idx
recording index (primary or secondary)
Values:

primary |  | 1
secondary |  | 2

CONF_HD_FILE_INFO
This message is used for updating actual recording files, it will be send periodically about every second by the recording device, that is running the recording on that file. The message informs about the start and end time changes of an file. For uniqe idetification, the message includes the span address and a file id. it also has the information about the recording cam (attention: in older firmware the file info msg only has the first 4 payload fields(from start time to file id))
CONF_HD_FILE_INFO_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a64 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | void |  | noprot |  | read not supported (only for messages), see definition CONF_HD_FILE_INFO |
| Write |  | void |  | l_serv |  | not supported |

CONF_HD_RELOAD_PARTITION_FILE_INFO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x091e |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | not supported (message signals an obsolete file list (num==partition)) |
| Write |  | void |  | l_serv |  | not supported |

CONF_HD_RECORDING_ACTIVE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0908 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 1: yes 0: no (message only, a request on this command always returns zero) |
| Write |  | - |  | l_serv |  | not supported |

CONF_START_RECORD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0acc |  | yes (1 - primary recording, 2 - secondary recording) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Start recording on choosen cams, payload needs a variable count pairs of 32 bit fiels for cam state (posibble states: 1 : on, 0 : off) and 32 bit fiels for cam selection mask, this mask will layed over the state bit field and can be used to choose the cams specific cams, other cams will be ignored, each bit field pair represents 32 cams: first pair - cam 1 to cam 32, second pair -cam 33 to cam 64 and so on |
| Write |  | p_octet |  | l_serv |  | Start recording on choosen cams, payload needs a variable count pairs of 32 bit fiels for cam state (posibble states: 1 : on, 0 : off) and 32 bit fiels for cam selection mask, this mask will layed over the state bit field and can be used to choose the cams specific cams, other cams will be ignored, each bit field pair represents 32 cams: first pair - cam 1 to cam 32, second pair -cam 33 to cam 64 and so on |

CONF_SET_REC_BUFFER_SIZE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ae1 |  | yes (line) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get size of recording buffer in bytes (generic dll only) first 4 bytes : DWORD rec_idx second 4 bytes : DWORD size in bytes(return direction) |
| Write |  | p_octet |  | l_serv |  | set size of recording buffer in bytes (generic dll only, default 5 MB, max 6 MB) first 4 bytes : DWORD rec_idx second 4 bytes : DWORD size in bytes |

CONF_HD_REPLAY_START

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0902 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_int |  | noprot |  | returns t_int parameter in percent of realtime replay (default +100%); 0 if suspended or stopped; Session ID is needed |
| Write |  | t_int |  | l_user |  | start a HD replay at the current position; t_int parameter in percent of realtime replay (default +100%); negative values will result in a reverse replay; Session ID is needed |

CONF_HD_REPLAY_STOP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0903 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | flag |  | noprot |  | 1=replay is stopped; 0=replay is in progress |
| Write |  | flag |  | l_user |  | stop a current HD replay; replay pointer will not be affected; Session ID is needed |

CONF_HD_REPLAY_STOP_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0904 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | p_octet |  | l_user |  | see detailed description |

Payload Structure

16 | 32
Seconds 4 Bytes
Milliseconds 4 Bytes
8 | 24 |

Seconds
Absolute time in seconds since 1.1.2000 00:00h.
This command will return a write error if the timeposition is outside a recording set. The Session ID is needed. A value of zero clears the stop marker.
CONF_HD_REPLAY_SEEK_TIME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0905 |  | no |  | yes (every second) |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | p_octet |  | l_user |  | see detailed description |

Payload Structure

16 | 32
Seconds 4 Bytes
Rtp Timestamp 4 Bytes
8 | 24 |

Seconds
Absolute time in seconds since 1.1.2000 00:00h.
Rtp Timestamp
Only in message. Rtp timestamp of the first replayed RTP packet of this second.
This command will return a write error if the timeposition is outside a recording set. The Session ID is needed.
CONF_HD_REPLAY_SEEK_IFRAME

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0907 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_int |  | noprot |  | obsolete |
| Write |  | t_int |  | l_user |  | set the replay pointer to the beginning of the next frame/last I-Frame(s); parameter t_int counted in frames relative to the current frame; Session ID is needed |

CONF_HD_REPLAY_EVENT_INFO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x091f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | p_octet |  | l_user |  | read only |

Payload Structure

16 | 32
Event Time 4 Bytes
Flags 4 Bytes
8 | 24 |

Event Time
Seconds since 2000.
Flags
Values:

Bit 0 |  | Motion Alarm
Bit 1 |  | Input Alarm
Bit 2 |  | Video Loss
Bit 3 |  | Virtual alarm (see CONF_VIRTUAL_ALARM_STATE)

CONF_HD_REPLAY_EVENT_INFO
List of recorded alarm events in backward order, since fw 4.0 events are only alarm state changes. Max size of the list is 128 entries. The command needs a valid replay session and the end time in secconds since 2000.
CONF_HD_REPLAY_PARTITION_EVENT_INFO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x091c |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get the last 512 alarm events of the partition (obsolete) |
| Write |  | p_octet |  | l_user |  | read only |

CONF_HD_REPLAY_MOTION_SAMPLES

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x095d |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | p_octet |  | l_user |  | read only |

Payload Structure

16 | 32
Sec. End 4 Bytes
Sample Interval 4 Bytes
Maximum Sample Bytes 4 Bytes
Bytes Per Sample 4 Bytes
8 | 24 |

Sample Interval
Values:

Seconds |  | 0
Minutes |  | 1
Houres |  | 2

Maximum Sample Bytes
Values:

Seconds |  | 0

Bytes Per Sample
1, 2, 4, 8. Time is included.
Read motion samples of a recording. Session ID required.
CONF_HD_REPLAY_FAST_INTRA_DELAY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x095e |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get the delay (in 10ms) between the frames in intra only replay mode |
| Write |  | t_dword |  | l_user |  | set the delay (in 10ms) between the frames in intra only replay mode |

CONF_HD_REPLAY_FAST_INTRA_FPS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ac2 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | get max frames per second for intra only replay mode |
| Write |  | t_dword |  | l_user |  | set max frames per second for intra only replay mode (0 = default) |

CONF_HD_REPLAY_LIVE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0963 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | obsolete |
| Write |  | t_dword |  | l_user |  | obsolete |

CONF_HD_REPLAY_SIZE_INFO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0906 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | see detailed description |
| Write |  | % |  | l_user |  | % |

Request Packet

16 | 32
Starttime 4 Bytes
Stoptime 4 Bytes
8 | 24 |

Starttime
In seconds since 2000.
Stoptime
In seconds since 2000.
Reply Packet

16 | 32
Max Size 8 Bytes ...
Min. Number Of Rtp Packets (will tend to be more) 4 Bytes ...
8 | 24 |

Max Size
In Bytes.
Replay session id required. Start time and stop time has to be within one file.
CONF_HD_REPLAY_VCD_LAYER

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09c8 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | requested vcd layer 0=no vcd data, 1=layer1 ,2=layer2,..; replay session id required |
| Write |  | t_dword |  | l_user |  | requested vcd layer 0=no vcd data, 1=layer1 ,2=layer2,..; replay session id required |

CONF_HD_REPLAY_VCD_CONFIG_ID

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a5f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | requested vcd config ID 0=all vcd data, 1=config1 data, 2=config2 data,..; replay session id required |
| Write |  | t_dword |  | l_user |  | requested vcd config 0=all data, 1=config1 data ,2=config2 data,..; replay session id required |

CONF_FORMAT_FS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d0 |  | storage medium (0=DEFAULT is recording storage device, 1=recording storage device, 2=RAMDISK) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | check the filesystem of a storage device status (0= no device present, 1=FAT32 not supported, 2=no FAT32 present, 3=FAT32 not mounted, 4=device is FAT32 mounting, 5=FAT32 format is running, 6=only FAT32, 7=FAT32 including recording, files 8=FAT32 including recording files and replay tools) |
| Write |  | t_dword |  | noprot |  | format a file system (FAT32) and creates files for the recordings and writes the tools for replay depending on the size of the storage device, returns TRUE if the request could be successfully queued, CONF_FORMAT_FS_STATUS messages report the progress and status about the format |

CONF_FORMAT_FS_STATUS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d1 |  | yes (file system nr, 1 - recording storage device, 2 - RAMDISK) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | status and progress of a running format requested by CONF_FORMAT_FS |
| Write |  | p_octet |  | noprot |  | status and progress of a running format requested by CONF_FORMAT_FS, see detailed description |

Payload Structure

16 | 32
step 1 Byte | status 1 Byte | progress 2 Byte
8 | 24 |

step
Which step of the formating (FAT32 Formatting including creating recording files or copy replay tools)
Values:

HD_STEP_FORMAT_FS |  | 0x00
HD_STEP_COPY_TOOLKIT |  | 0x01

status
reports the state of formatting. The format can be in state of running, failed or successfully finished. The last one is devided in the two states of HD_FORMAT_STATUS_FINISHED which means FAT32 including recording files and replay tools were created and HD_FORMAT_STATUS_SKIPPED which means that only the FAT32 was created because the storage device was not the needed size for recording.
Values:

HD_FORMAT_STATUS_FAILED |  | 0xff
HD_FORMAT_STATUS_RUNNING |  | 0x00
HD_FORMAT_STATUS_SKIPPED |  | 0x01
HD_FORMAT_STATUS_FINISHED |  | 0x02

progress
value from 0 to 100 represent the progress of the format including copy replay tools in percent.
Values:

progress in percent |  | 0 to 100

CONF_FORMAT_FS_STATUS
the message reports the status and progress of a running format. The formatting takes two steps that is first formating FAT32 including creating the recording files and second copy the replay tools. The progress is reported about the whole formatting. The status reports the state of each formatting step. A successful format should always end with a message with 100 percent progress, step should be copy toolkit and status should be HD_FORMAT_STATUS_FINISHED or HD_FORMAT_STATUS_SKIPPED if the storage device is too small for recording (e.g. RAMDISK). A failed format should finish with a status HD_FORMAT_STATUS_FAILED at any progress and step. After this final messages no futher message will follow.
CONF_FORMAT_FS_SPAN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e6 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | format the lun into spans. |
| Write |  | p_octet |  | l_serv |  | format the lun into spans. (not allowed while recording on this lun) |

Payload Structure

16 | 32
Server IP 4 Bytes
Target IDX 1 Byte | Lun IDX 1 Byte | Span Cnt 2 Byte
Span Size 4 Bytes
8 | 24 |

Server IP
The iSCSI server ip address
Values:

Local connected USB disk |  | ff.ff.ff.ff
iSCSI Server |  | valid ip address

Target IDX
Index of the iSCSI server target. The index of the desired target can be obtained from the reply to an iSCSI discover.
Lun IDX
Index of the lun of the specified target.
Span Cnt
Number of spans the lun shall be formated with
Span Size
Size of each span in megabyte. (1 MB = 1024 x 1024 Bytes)
Note
The reply packet will contain the values of the actually formated spans and size. If the product of the span count and the span size in the request packet exceeds the size of the current lun, only as many as possible spans are formatted. If the product is less than the available lun space, the back part of the lun will be unused.
Specific Error Types

SPAN_ERR_INTERNAL |  | 0x01
SPAN_ERR_NOT_MNTD |  | 0x05
SPAN_ERR_INV_FS |  | 0x06
SPAN_ERR_INV_LUN_NFO |  | 0x07
SPAN_ERR_RD_ONLY |  | 0x0a
SPAN_ERROR_OLD_LUN_NFO |  | 0x20
ISCSI_ERROR_CONNECT |  | 0x31
ISCSI_ERROR_INV_LUN |  | 0x33
ISCSI_ERROR_LOGIN |  | 0x34
ISCSI_ERROR_INV_TRG_IDX |  | 0x35

Note: A list of all defined error types can be found in the Appendix.
CONF_FORMAT_FS_SPANS_STATUS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09f5 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | status and progress of a running format requested by CONF_FORMAT_FS_SPANS, see detailed description |
| Write |  | p_octet |  | l_serv |  | status and progress of a running format requested by CONF_FORMAT_FS_SPANS, see detailed description |

Payload Structure

16 | 32
step 1 Byte | status 1 Byte | progress 2 Byte
ip 4 Bytes
target_idx 1 Byte | lun 1 Byte | reserved 2 Byte
8 | 24 |

step
Which step of the formating (FAT32 Formatting including creating spans and clearing span headers)
Values:

HD_STEP_FORMAT_FS |  | 0x00
HD_STEP_CLEAR_SPAN_HEADER |  | 0x02

status
reports the state of formatting. The format can be in state of running, failed or successfully finished. success means the creation of the fat32 file system and the empty spans or clearing the span headers was successfully.
Values:

HD_FORMAT_STATUS_FAILED |  | 0xff
HD_FORMAT_STATUS_RUNNING |  | 0x00
HD_FORMAT_STATUS_FINISHED |  | 0x02

progress
value from 0 to 100 represent the progress of the format including the creation of the empty recording spans and clearing the header files.
Values:

progress in percent |  | 0 to 100

ip
ip of the storage device or lun, that is formatting
target_idx
Target Index of the storage device from 0 to 255.
lun
Lun of the storage device from 0 to max. 255.
reserved
2 Bytes reserved
CONF_FORMAT_FS_SPANS_STATUS
this message reports the status and progress of a running format. The formatting includes the creation of the FAT32 file system (step: HD_STEP_FORMAT_FS) and clearing of the span header files(step: HD_STEP_CLEAR_SPAN_HEADER). The progress is reported about the whole formatting. A successful format should always end with a message with 100 percent progress at step HD_STEP_CLEAR_SPAN_HEADER and status should be HD_FORMAT_STATUS_FINISHED. A failed format should finish with a status HD_FORMAT_STATUS_FAILED at any progress and any step. After these final messages no futher messages will follow. The whole formatting takes two steps HD_STEP_FORMAT_FS and HD_STEP_CLEAR_SPAN_HEADER. First step HD_STEP_FORMAT_FS will run up to 90 percent and will end with a 90 percent progress message and status HD_FORMAT_STATUS_FINISHED if successful. Then the last step HD_STEP_CLEAR_SPAN_HEADER will follow from 90 to 100 percent and will also end with a HD_FORMAT_STATUS_FINISHED status if successfull, which is also as mentioned earlier the final success message.
CONF_SPAN_ADDRESS_LIST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e7 |  | yes (1 - primary spanlist, 2 - secondary spanlist) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | See detailed description. |
| Write |  | p_octet |  | l_serv |  | See detailed description. |

Payload Structure

Span Address 1 8 Bytes ...
(n-2) x 8 Bytes | Span Address n 8 Bytes ...

Span Address 1 - n
For the structure of a span address so description below.

16 | 32
Server IP 4 Bytes
Target IDX 1 Byte | Lun IDX 1 Byte | Span IDX 2 Byte
8 | 24 |
Server IP The iSCSI server ip address. Values:
Local connected USB disk |  | ff.ff.ff.ff
iSCSI Server |  | Valid IP address
Target IDX Index of the iSCSI server target. The index of the desired target can be obtained from the reply to an iSCSI discover. Lun IDX Index of the lun of the specified target. Span IDX Index of the span in the specified lun.

Write request
On a write request, a list of max n (n=512) span addresses must be supplied. List entrys that are zero are not used by the unit for recording. The unit uses the supplied ordering of the list and begins with the first entry. The order of the supplied list is the preferred order, not the guaranted order. There are some cases, in which the device changes the use order (e.g. one target not reachable).
If the device is already recording on spans (a span list is already present on the device), the new list must contain the span addresses, that the unit is currently recording on. The latter information can be obtained by reading the current span address list form the unit and check the corresponding write lock header (if the units IP and MAC address is found this means the unit is recording). If the unit receives a list and the span addresses of the spans the device is currently recording on is not present, the list is rejected (not saved in the configuration) and an error is returned
Read Request
The reply to an read request always contains up to n (n=512) entrys. The response in case of an empty span list is one zeroed span entry.
Message
A message of this cmd tag will be send always, if somone sets the span address lists by using rcp set spans list commands or if the span list is cleared by indirectly by changing other settings of the device (e.g. rec mgmt).
Specific Error Types

SPAN_ERR_INTERNAL |  | 0x01
SPAN_ERR_INV_ADDR_LIST |  | 0x04

Note: A list of all defined error types can be found in the Appendix.
CONF_SPAN_ADDRESS_LIST_NEW

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a52 |  | yes (1 - primary spanlist, 2 - secondary spanlist) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | See detailed description of CONF_SPAN_ADDRESS_LIST |
| Write |  | p_octet |  | l_serv |  | See detailed description of CONF_SPAN_ADDRESS_LIST (no need to include mounted spans in list) |

CONF_SPAN_HDR_ACCESS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09e8 |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Access span header information. |
| Write |  | p_octet |  | l_serv |  | Access span header information. |

Payload Structure

16 | 32
Server IP 4 Bytes
Target IDX 1 Byte | Lun IDX 1 Byte | Span IDX 2 Byte
Span Header N Bytes ...
8 | 24 |

Server IP
The iSCSI server ip address.
Values:

Local connected USB disk |  | ff.ff.ff.ff
iSCSI Server |  | Valid IP address

Target IDX
Index of the iSCSI server target. The index of the desired target can be obtained from the reply to an iSCSI discover.
Lun IDX
Index of the lun of the specified target.
Span IDX
Index of the span in the specified lun.
Span Header
Data of the span header. Length and structure differs for the specified header type. The header type is specified with the numeric descriptor:
Values:

LOCK HEADER |  | 0x01
16 | 32
Lock owner IP 4 Bytes
Lock owner MAC 6 Bytes ...
| Reserved 2 Byte
8 | 24 |
Lock owner IP IP address of the unit that holds the write lock of the span. Lock owner MAC Hardware address of the unit that holds the write lock of the span NOTE: In the request packet, the header values are ignored (may be zero). The reply contains the values read or written. On write requests, the local IP and MAC addresses are converted to ascii strings and written to the file LCKxxxxx.txt (xxxx = span index) on disk. On read requests, the ascii strings of that file are scanned into binary values and send with the reply.
MANAGER HEADER |  | 0x02
16 | 32
Manager Header Data N Bytes (max. 1024) ...
8 | 24 |
Manager Header Data Transparent header data of the storage manager The reply always returns the 1024 Bytes of the manager header file MGRxxxx.txt (xxxx = span index).
UNIT HEADER |  | 0x03
16 | 32
Span owner IP 4 Bytes
Span owner MAC 6 Bytes ...
| Span owner Camera 2 Byte
Retention Time 4 Bytes
Modification seal random 4 Bytes
Modification seal time 4 Bytes
Recording 1 Byte | reserved 3 Bytes
8 | 24 |
Span owner IP IP address of the unit that holds the write lock of the span. Span owner MAC Hardware address of the unit that holds the write lock of the span Span owner Camera The index of the camera the unit uses for recording. Retention Time Retention Time for the recordings on this span in sec since 2000 Modification seal random random number set on the last modifacation of this span, this random will be set on each write access on any span header or on starting or stopping a recording of a device on this span, there will be also updates while a device is recording in a period of several minutes Modification seal time this information is the time of the last modification on this span that causes a modification seal update Recording for dual recording, 1 - primary recording, 2 - secondary recording, if this value is not set then default is primary recording NOTE: In the read request packet, the header values are ignored (may be zero). In the write requst packet, only the camera field is evaluated, the values for IP and MAC are taken from local configuration. The reply packet contains the values read or written. On write requests, the local IP and MAC addresses and the supplied camera value are converted to ascii strings and written to the file UNTxxxxx.txt (xxxx = span index) on disk. On read requests, the ascii strings of that file are scanned into binary values and send with the reply. The modification seal values cannot be set by this command as write request directly, they will be set automatically on span header write requests or on starting or stopping a recording. The content of this fields will be ignored in a write request.

Specific Error Types:

SPAN_ERR_INTERNAL |  | 0x01
SPAN_ERR_INV_SPN_IDX |  | 0x02
SPAN_ERR_INV_HDR_TYPE |  | 0x03
SPAN_ERR_NOT_MNTD |  | 0x05
SPAN_ERR_INV_FS |  | 0x06
SPAN_ERR_INV_LUN_NFO |  | 0x07
SPAN_ERR_BAD_HDR_CKSM |  | 0x08
SPAN_ERR_RD_ONLY |  | 0x0a
ISCSI_ERROR_CONNECT |  | 0x31
ISCSI_ERROR_INV_LUN |  | 0x33
ISCSI_ERROR_LOGIN |  | 0x34
ISCSI_ERROR_INV_TRG_IDX |  | 0x35

Note: A list of all defined error types can be found in the Appendix.
CONF_RECORD_MODE_SPANS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09f6 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_octet |  | noprot |  | returns 0x00 if span recording is off, 0x01 if on |
| Write |  | t_octet |  | l_serv |  | Set span recording mode to on 0x01 or off 0x00 (obsolete, device is always in mode on) |

CONF_START_SPAN_RECORD

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09f7 |  | yes (1 - primary recording, 2 - secondary recording) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | returns the 4 bytes bitmap of span recording for the cameras 4 bytes bitmap (1 : on, 0 : off) for each cam (bit 0 -> cam 1 bit 1 -> cam 2 ...) |
| Write |  | p_octet |  | l_serv |  | Start span recording on choosen cameras first 4 bytes bitmap (1 : on, 0 : off) for each cam (bit 0 -> cam 1 bit 1 -> cam 2 ...), last 4 bytes bit mask for setting only choosen cameras (bit 0 -> cam 1 bit 1 -> cam 2 ...) |

CONF_SPAN_PARTITION_PROP

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09fa |  | yes (camera) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | return partition properties for primary span recording (4 bytes) video type (1 byte: 0= NO, 1=MPEG2, 3=MPEG4), reserved (3 byte) |
| Write |  | p_octet |  | l_serv |  | (obsolete and not supported anymore) |

CONF_SPAN_PARTITION_PROP_ALARM

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09fb |  | yes (camera) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | obsolete and not supported anymore |
| Write |  | p_octet |  | l_serv |  | obsolete and not supported anymore |

CONF_SPAN_PARTITION_PROP_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a4b |  | yes (camera) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | return partition properties for secondary span recording (4 bytes) video type (1 byte: 0= NO, 1=MPEG2, 3=MPEG4), reserved (3 byte) |
| Write |  | p_octet |  | l_serv |  | (obsolete and not supported anymore) |

CONF_SPAN_PARTITION_PROP_ALARM_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a4c |  | yes (camera) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | obsolete and not supporded anymore |
| Write |  | p_octet |  | l_serv |  | obsolete and not supported anymore |

CONF_SPAN_USE_STATUS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09f8 |  | cam |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | usage status of a span, see detailed description |
| Write |  | p_octet |  | l_serv |  | not supported |

Payload Structure

16 | 32
use status message 1 12 Bytes ...
use status message 2 12 Bytes ...
8 | 24 |

use status message 1 - 2
Upto 2 span use status messages. If no span is in use by the camera specified by num, the reply payload size will be 0. In case of the rcp message the payload contains always 1 span use status message.
Span Use Status Message Structure

16 | 32
err/spec code 1 Byte | status 1 Byte | cam 2 Bytes
ip 4 Bytes
target_idx 1 Byte | lun 1 Byte | span_idx 2 Byte
8 | 24 |

error/special code
additional error or status code to the status, for status HD_SPAN_USE_STATUS_ERROR_MOUNT see section "status HD_SPAN_USE_STATUS_ERROR_MOUNT error codes", for status RELEASE and RELEASE_UNUSED see section "status RELEASE error codes", for status MOUNTED see section "status MOUNTED special codes"
status
use status of this span
Values:

MOUNTED |  | 0x00
RELEASE |  | 0x01
RELEASE_UNUSED |  | 0x02
ERROR |  | 0x03
RECORDING |  | 0x04
PENDING_SPAN_REQUEST |  | 0x05
HD_SPAN_USE_STATUS_RETENTION_TIME |  | 0x06
HD_SPAN_USE_STATUS_RELEASE_REMOUNT_INTENDED |  | 0x07
HD_SPAN_USE_STATUS_ERROR_WRT_UNT_HDR |  | 0x10
HD_SPAN_USE_STATUS_ERROR_FORMAT_REC_REGION |  | 0x11
HD_SPAN_USE_STATUS_ERROR_MOUNT |  | 0x12
HD_SPAN_USE_STATUS_ERROR_RETENTION_TIME |  | 0x13

If the status is PENDING_SPAN_REQUEST, the ip will be 255.255.255.255, target index and lun will be 255, and span index will be 65535, which should be interpreted as still unknown, because this cam had requested a span, but it doesn't know yet which span it gets.
Status HD_SPAN_USE_STATUS_RELEASE_REMOUNT_INTENDED means, the cam has released the block but has left the span lock, because it will try to remount the span later. The span is stored in the span history for remount(see CONF_SPAN_HISTORY).
cam
which cammera is or was using the reported span
ip
ip of the storage device (ISCSI)
target_idx
Target Index of the storage device from 0 to 255.
lun
Lun of the storage device from 0 to max. 255.
span_idx
Index of the span on the storage device.
CONF_SPAN_USE_STATUS
This messages reports the use status of a span for this device and which cammera for primary recording. If a span was opened for a planned recording, this message will be send with status MOUNTED. If the mounting fails status will be ERROR. If a span was closed after recording status will be RELEASE, if it was closed before a recording ever took place, status will be RELEASE_UNUSED. HD_SPAN_USE_STATUS_RETENTION_TIME status will be send as message if the first time an retention time update took place on the span. In case of a read request the reply payload cantains this status message upto twice. the command can be used to query the actual used spans from a camera specified by the num parameter. the status for a span can be RECORDING, if the cam is actual recording on this span or MOUNTED, if the span is mounted and prepared for a future recording by this camera.
status HD_SPAN_USE_STATUS_ERROR_MOUNT error codes
Values:

none |  | 0x00
SPAN_ERROR_INTERNAL |  | 0x01
SPAN_ERROR_INV_SPN_IDX |  | 0x02
SPAN_ERROR_INV_HDR_TYPE |  | 0x03
SPAN_ERROR_INV_ADDR_LIST |  | 0x04
SPAN_ERROR_NOT_MNTD |  | 0x05
SPAN_ERROR_INV_FS |  | 0x06
SPAN_ERROR_INV_LUN_NFO |  | 0x07
SPAN_ERROR_BAD_HDR_CKSM |  | 0x08
SPAN_ERROR_INV_IDX |  | 0x09
SPAN_ERROR_RD_ONLY |  | 0x0a
SPAN_ERROR_NO_REC_DAT |  | 0x0b
SPAN_ERROR_INV_PART_NFO |  | 0x0c
SPAN_ERROR_SPAN_REQUEST_FAILED |  | 0x0e
SPAN_ERROR_SPAN_REQUEST_RETENTION_TIME |  | 0x0f
SPAN_ERROR_REMOUNT_REFUSED |  | 0x10
ISCSI_ERROR_CONNECT |  | 0x31
ISCSI_ERROR_INV_LUN |  | 0x33
ISCSI_ERROR_LOGIN |  | 0x34
ISCSI_ERR_PWD |  | 0x36
ISCSI_ERR_PROTO |  | 0x37
ISCSI_ERR_TARG_NOT_REACH |  | 0x38
ISCSI_ERR_NO_MEM |  | 0x3a
ISCSI_ERR_SESS_CREATE |  | 0x3b
ISCSI_ERR_INV_PARAMS |  | 0x3c
ISCSI_ERR_SESS_NOT_FOUND |  | 0x3d
ISCSI_ERR_DISCONN |  | 0x3e
ISCSI_ERR_TIMEOUT |  | 0x3f
ISCSI_ERR_SOCK |  | 0x5f
ISCSI_ERR_TARG_PM |  | 0x6f
ISCSI_SOCK_CLOSED |  | 0x7f
ISCSI_ERR_TCP_CONN_RST |  | 0x8f
ISCSI_ERR_INTR_NOT_SUPP |  | 0x9f
ISCSI_ERR_IP_ZERO |  | 0xa0
ISCSI_ERR_OUT_OF_RES |  | 0xa1
HDD_ERROR_TIMEOUT |  | 0x12
HDD_ERROR_CREATE_FAILED |  | 0x22
HDD_ERROR_ACCESS_DENIED |  | 0x32
HDD_ERROR_DEVICE_PRESENT_TIMEOUT |  | 0x42
HD_PMM_ERROR_LUN_LOCK |  | 0x52
HD_PMM_ERROR_INVALID_ACCESS |  | 0x62
HD_PMM_ERROR_LUN_MGMT_FILE_NOT_FOUND |  | 0x72
HD_PMM_ERROR_LUN_WRITE_PROTECTED |  | 0x82
HD_PMM_ERROR_COMMON |  | 0xf2

status RELEASE error codes
Values:

none |  | 0x00
HD_PMM_RELEASE_ERROR_HD_MGR_ERROR |  | 0x01
HD_PMM_RELEASE_ERROR_SPAN_LIST_INCONSISTENCY |  | 0x02
HD_PMM_RELEASE_ERROR_RECORD_HANDLE_DISMISS_ERROR |  | 0x03
HD_PMM_RELEASE_ERROR_BIG_TIME_JUMP |  | 0x04
HD_PMM_RELEASE_ERROR_CLOSED_WHILE_MOUNTING |  | 0x05
HD_PMM_RELEASE_ERROR_INITIAL_MOUNT_ABORT |  | 0x06
HD_PMM_RELEASE_ERROR_INITIAL_MOUNT_UNFINISHED |  | 0x07
HD_PMM_RELEASE_ERROR_NEXT_SPAN_NOT_MOUNTED |  | 0x08
HD_PMM_RELEASE_ERROR_RECORDING_ERROR |  | 0x09
HD_PMM_RELEASE_ERROR_ENCODER_ERROR |  | 0x0a
HD_PMM_RELEASE_ERROR_REPLACE |  | 0x0b |  | (release was caused by CONF_SPAN_SWITCH command)
HD_PMM_RELEASE_ERROR_SWITCH_REQUEST |  | 0x0c |  | (release was caused by CONF_SPAN_SWITCH command)

status MOUNTED special codes
Values:

standard mount |  | 0x00
HD_MOUNT_CODE_REMOUNTED |  | 0x01

CONF_SPAN_USE_STATUS_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a4a |  | cam |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | span use status for secondary recording, payload as in CONF_SPAN_USE_STATUS |
| Write |  | p_octet |  | l_serv |  | not supported |

CONF_SPAN_PARTITION_FILE_INFO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a2d |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Read the file info of a span. |
| Write |  | void |  | l_serv |  | not supported |

Payload Structure

16 | 32
iSCSI Server IP 4 Bytes
Target IDX 1 Byte | LUN 1 Byte | Span IDX 2 Byte
8 | 24 |

iSCSI Server IP
The iSCSI server ip address.
Target IDX
Index of the iSCSI server target. The index of the desired target can be obtained from the reply to an iSCSI discover.
LUN
The logical unit.
Span IDX
Index of the span in the specified lun.
Response Structure
For the payload structure of the response see documentation of HD_PARTITION_FILE_INFO.
CONF_EXPORT_SPAN

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a2e |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Retrieve a span of the devices storage. |
| Write |  | p_octet |  | l_serv |  | not supported |

Request Payload Structure

16 | 32
Recording Camera 12 Bytes ...
Lun Addr 8 Bytes ...
Reserved 12 Bytes ...
Overwrite Retention Time 4 Bytes
Reserved 4 Bytes
8 | 24 |

Recording Camera
The address of the device the span is assigned to.

16 | 32
IP 4 Bytes
MAC 6 Bytes ...
| Recording Index 1 Byte | Camera 1 Byte
8 | 24 |
IP The ip address of the recording device. MAC The hardware address of the recording device. Recording Index 1 = Primary Recording, 2 = Secondary Recording Camera The camera index.

Lun Addr
The address of the lun a span is desired from.

16 | 32
IP 4 Bytes
Target IDX 1 Byte | LUN 1 Byte | Reserved 2 Byte
8 | 24 |
IP The ip address of the iscsi target. Target IDX The index of the target. LUN The logical unit number.

Overwrite Retention Time
If this field is set (> 0) and no free spans are available, spans with retention times that are lower or equal to the specified retention time are accounted for export. In this case the recording with the retention time that expires next is overwritten.
Response and Message Payload Structure

16 | 32
Recording Camera 12 Bytes ...
Span Address 8 Bytes ...
Last Recording 16 Bytes ...
State 1 Byte | Reserved 3 Bytes
8 | 24 |

Recording Camera
The address of the device the span is assigned to (see request payload description for details).
Span Address
The address of the span the device exports. If this field is zero, no span is exported.

16 | 32
IP 4 Bytes
Target IDX 1 Byte | LUN 1 Byte | Span IDX 2 Byte
8 | 24 |
IP The ip address of the iscsi target. Target IDX The index of the target. LUN The logical unit number. Span IDX The index of the span on the lun.

Last Recording
The address of the span the device exports.

16 | 32
Recording Camera 12 Bytes ...
Retention Time 4 Bytes
8 | 24 |
Recording Camera The id of the camera of the recording that is overwritten. Field is zero, if there was no recording on this span. See request packet for detailed description. Retention Time The retention time (seconds since 2000) of the recording that is overwritten.

State
Values:

SUCCESS |  | 0x00
NO SPAN AVAILABLE |  | 0x01
STORAGE OFFLINE |  | 0x02
INVALID SPAN MANAGER ADDRESS |  | 0x03
ACCESS DENIED |  | 0x04

A list of span manager the recording is using can be obtained by the command CONF_REC_SPAN_MGR.
CONF_CAM_REC_SPANS

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a8f |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Retrieve the list of recording spans of a camera from a span manager on a managed lun. |
| Write |  | % |  | l_serv |  | % |

Request Payload Structure

16 | 32
Recording Camera 12 Bytes ...
Lun Address 8 Bytes ...
8 | 24 |

Recording Camera
The address of the camera for which recording spans are to be queried.

16 | 32
IP 4 Bytes
MAC 6 Bytes ...
| Recording Index 1 Byte | Camera 1 Byte
8 | 24 |
IP The ip address of the recording device. MAC The hardware address of the recording device. This field may be zero if you search for recordings without considering the mac. Recording Index 1 = Primary Recording, 2 = Secondary Recording Camera The camera index.

Lun Address
The address of the lun on which recording spans for a camera are searched.

16 | 32
IP 4 Bytes
Target IDX 1 Byte | LUN 1 Byte | Reserved 2 Byte
8 | 24 |
IP The ip address of the iscsi target. Target IDX The index of the target. LUN The logical unit number.

Response and Message Payload Structure

Recording Camera 12 Bytes ...
Lun Address 8 Bytes ...
N x Span Recording Info 16 Bytes ...

Recording Camera
The address of the recording camera (see request payload description for details).
Lun Address
The address of the lun of the recording spans (see request payload description for details).
Span Recording Info
Recording info about the spans the camera recorded.

16 | 32
Span Index 2 Byte | S 1 | Timezone 7 Bits | Flags 1 Byte
Start Time 4 Bytes
Stop Time 4 Bytes
Reserved 2 Bytes | File Count 2 Bytes
8 | 24 |
Span Index The span index in the current lun. S The timezone sign. Timezone Timezone in quarter hours. Flags Values:
Bit 0 |  | Continous Recording
Bit 1 |  | Recording Running
Bit 2 |  | Migrated Recording
Start Time Seconds since 2000. Stop Time Seconds since 2000. File Count The number of files that are stored in this span.

CONF_REC_SPAN_MGR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a36 |  | yes (1 - primary recording, 2 - secondary recording) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  |  |
| Write |  | p_octet |  | l_serv |  |  |

Payload Structure
Sequence of (max 8):

16 | 32
Span Mananger IP address 4 Bytes
Storage IP address 4 Bytes
Target Index 1 Byte | Lun 1 Byte | Reserved 2 Byte
Priority 2 Bytes | Flags 2 Byte
8 | 24 |

Span Mananger IP address
The IP address of the device the span manager is running on.
Storage IP address
The iSCSI IP address of the storage.
Target Index
The iSCSI target index.
Lun
The iSCSI lun of the storage.
Priority
Priority is NOT SUPPORTED yet!
Flags
Values:

OVERWRITE_OLDEST_RECORDINGS |  | 0x0001

If the flag OVERWRITE_OLDEST_RECORDINGS is set and no free spans are available on all span manager of the devices recording span manager list, the recording with the retention time that expires next is overwritten.
Use this command to edit the recording span manager list. This list is consulted every time when a device is recording in VRM mode an its span list runs out resources. The entry with the highest priority is picked out of this list, the corresponding span manager is contacted and queried for spans. If the span manager ís not accessable or will not return a span for some reason (maybe it has no more free spans to export), the entry with the next lower priority is picked out of the list.
CONF_SPAN_REC_COPY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a55 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | List the currently running span recording copy processes. |
| Write |  | p_octet |  | l_serv |  | Copy recordings from a source span to a destination span. |

Request Packet Structure

16 | 32
Source Span 8 Bytes ...
Destination Span 8 Bytes ...
File Index 4 Bytes
Offset 4 Bytes
Duration 4 Bytes
Velocity 4 Bytes
Action 1 Byte | Flags 1 Byte | Reserved 2 Byte
Reserved 16 Bytes ...
8 | 24 |

Source Span
The address of the span from which the data is to be copied.

16 | 32
iSCSI IP 4 Bytes
Target Idx 1 Byte | Lun 1 Byte | Span Idx 2 Byte
8 | 24 |
iSCSI IP The ip address of the iscsi server Target Idx The index of the target on the iscsi server. Lun The logical unit. Span Idx The index of the span.

Destination Span
The address of the span to which the data is to be copied. For the structure of the span address see the description of the field Source Span.
NOTE: The address of the destination span can be used to uniquely identify the copy process in the system, because it is not possible to run more than one copy on the same destination span simultaneously. If a second copy process is tried to be invoked on the same destination span, this command fails.
File Index
The index of the file in the list obtained by the command CONF_HD_SPAN_PARTITION_FILE_INFO. If this index exceeds the number of entries in the list, the error code ERR_INV_SRC_FILE is returned with the response packet.
Offset
The offset from the beginning of the file in seconds. If this value exceeds the total number of seconds of the file, the error code ERR_FILE_OFF_TOO_BIG is returned with the response packet. A value of 0 accords to a copy from the beginning of the file.
Duration
The number of seconds to copy. If the sum of offset and duration seconds exceeds the number of seconds of the file, the duration seconds are clipped to the maximum number left from the specified offset. The maxium value accords to a copy till the end of the file.
Velocity
The speed (in percent of realtime) at which the copy process runs.
Action
Use this field to control (start/stop) the copy process. Only the Velocity-field can be updated.
Values:

START |  | 0x00
UPDATE |  | 0x01
STOP |  | 0x02

Flags
Additional copy options.
Values:

COPY_UNT_HDR |  | 0x01
FMT_REC_REG |  | 0x02
APPEND_TO_LAT_REC |  | 0x04
MERGE_TO_LAT_REC |  | 0x08

If the flag COPY_UNT_HDR is set, the values of the unit header of the source span are copied into the unit header of the destination span.
If the flag FMT_REC_REG is set, all previous recordings on the destination span are deleted. All destination spans with invalid recording regions are formated, too.
If the flag APPEND_TO_LAT_REC is set, the video data is appended to the latest slice in the destination span. If this flag is set with FMT_REC_REG simultaneously, an error is returned.
If the flag MERGE_TO_LAT_REC is set, the the new slice is merged to the latest slice in the destination span. If this flag is set with APPEND_TO_LAT_REC simultaneously, APPEND_TO_LAT_REC is ignored.
Response and Message Packet Structure

16 | 32
Source Span 8 Bytes ...
Destination Span 8 Bytes ...
File Index 4 Bytes
Offset 4 Bytes
Duration 4 Bytes
Velocity 4 Bytes
Status 1 Byte | Error 1 Byte | Reserved 2 Byte
Copy Seconds 4 Bytes
Copied Until 4 Bytes
Kilobytes Copied 4 Bytes
Datarate 4 Bytes
8 | 24 |

Source Span
See description of the request packet.
Destination Span
See description of the request packet.
File Index
See description of the request packet.
Offset
See description of the request packet.
Duration
See description of the request packet.
Velocity
See description of the request packet.
Status
Values:

INITIALIZING |  | 0x00
COPYING |  | 0x01
DONE |  | 0x02
CLOSING |  | 0x03
ERROR |  | 0x04

Error
Set to zero in a request packet. An error code is returned in the response packet, if the creation of the copying process fails.
Values:

ERR_INTERNAL |  | 0x01
ERR_MAX_COPY_EXCEED |  | 0x02
ERR_NO_ACT_COPY_2_DST |  | 0x03
ERR_DST_SPAN_IN_USE |  | 0x04
ERR_ACCESS_SRC_SPAN |  | 0x05
ERR_ACCESS_DST_SPAN |  | 0x06
ERR_FMT_REC_REG |  | 0x07
ERR_INV_SRC_FILE |  | 0x08
ERR_FILE_OFF_TOO_BIG |  | 0x09
ERR_RD_SRC_UNT_HDR |  | 0x0A
ERR_WR_DST_UNT_HDR |  | 0x0B
ERR_WR_DST_LCK_HDR |  | 0x0C
ERR_REPL_OPEN |  | 0x0D
ERR_REC_OPEN |  | 0x0E
ERR_REPL_START |  | 0x0F
ERR_REC_START |  | 0x10
ERR_DST_SPAN_FULL |  | 0x11
ERR_TIMEOUT |  | 0x12
ERR_MERGE_FAILED |  | 0x13
ERR_DST_FMT_VERSION |  | 0x14

Copy Seconds
The number of seconds the copy process is running.
Copied Until
A timestamp (Seconds since 2000) to which the copy process progressed till now.
Kilobytes Copied
The number of kilobytes transferred to the destination span.
NOTE: To determine the network traffic, you have to multiply this value with two.
Datarate
The rate at which data is written to the destination span. NOTE: To determine the network traffic, you have to multiply this value with two.
Read
If the command is to be read, the request packet may be empty. The response packet contains a list of all currently active copy processes and their statistics.
Write
The write request contains parameters for a copy process that is to be started, stopped or updated. Only the following fields can be updated: Duration, Velocity. The response packet to a write command contains the parameters and statistics for that copy process.
CONF_SPAN_SWITCH

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a53 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | not supported |
| Write |  | p_octet |  | l_serv |  | switch spans, see detailed description |

Payload Structure

16 | 32
ip recording span 4 Bytes
target_idx 1 Byte | lun 1 Byte | span_idx 2 Byte
ip premounted span 4 Bytes
target_idx 1 Byte | lun 1 Byte | span_idx 2 Byte
flags 16 Bits | recording 1 Byte | reserved 1 Byte
8 | 24 |

ip recording span
the ip of the actual recording span
target_idx
the target index of the actual recording span
lun
the lun of the actual recording span
span_idx
the span index of the actual recording span
ip premounted span
the ip of the premounted span
target_idx
the target index of the premounted span
lun
the lun of the premounted span
span_idx
the span index of the premounted span
flags
these flags are used to specify the behav. of the command
Flags:

FORCE |  | 0x0001
CHECK_PREMOUNTED |  | 0x0002
REPLACE_PREMOUNTED |  | 0x0004
SWITCH_SPAN |  | 0x0008
TARGET_RETREAT |  | 0x0010
TARGET_REINTRODUCE |  | 0x0020
ERROR_CHECK_PREMOUNTED |  | 0x4000
ERROR_CHECK_RECORDING |  | 0x8000

recording
select a recording
Values:

primary recording |  | 1
secondary recording |  | 2

CONF_SPAN_SWITCH
This command can be used to influence the span usage of the recording. It is able to cause a replace of the premounted span and or switch to the next premounted span.
The flag SWITCH_SPAN causes the switch to the next span and releasing the actual recording span. Flag REPLACE_PREMOUNTED will cause the release of the premounted span and mounting another one if available. If both flags are activated, the premounted block will be replaced, as soon as a new premounted span is mounted and available, the next step switch to premounted span will be performed. Before replacing the premounted span, the actual recording span will be checked, if the replace could get in conflict with a device internal triggered span switch. In that case the whole Span switch command will fail with rcp error RCP_ERROR_TRY_LATER, no switch or replace will be performed.
When performing a switch to next span job, the recording span address in the payload will be checked. If on execution of this job the recording span doesn't match the recording span from the payload, the switch will not be performed. When performing a replace premounted span job, the premounted span address in the payload will be checked. If on execution of this job the premounted span doesn't match the premounted span from the payload, the replace will not be performed. The idea of these checks is to avoid conflicts with the automatic span switching of the recording, that can lead to gaps in the recording and unwanted waste of recording spans. The flag FORCE will skip these checks. Flag CHECK_PREMOUNTED is only relevant for the switch to next span job without replacing the premounted span and without FORCE flag. If this flag is active on switching ton next span, the premounted span parameter in the payload will be matched against the actual premounted span. If no match the switch won't be performed. If this flag including the FORCE flag isn't set on switch, a negative match will be performed on the premounted span. The TARGET_RETREAT Bit means, than a complete retreate from this target is intended, the span history will be modified in order to avoid a remount on that target. That state will stay active for that target until the device records on a new target and adds a span from the new target to the history, or if the span history will be cleared or the the target will be reintroduced with the bit TARGET_REINTRODUCE. The TARGET_REINTRODUCE Bit is needed to undo a TARGET_RETREAT action, which is specialy in the case needed, when a device shall return to a target, from that it had retreated erlier and no recording took place on another target between these events. In that case the remount feature for that target is still disabled. The TARGET_REINTRODUCE Bit will reenable the remount feature for that target without the nessessarity of clearing the whole span history.
Warning: A possible conflict, when requesting a replace of the premounted span with an automatic span switch of the recording that causes gaps in the recording is unavoidable. So an excesive usage of replacing premounted spans should be avoided.
CONF_HD_SET_VRM_LOCK

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a5d |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | not supported |
| Write |  | p_octet |  | l_serv |  | Write or clear the vrm lock. |

Payload Structure

16 | 32
IP 4 Bytes
target idx 1 Byte | lun 1 Byte | reserved 2 Byte
flags 32 Bits
8 | 24 |

IP
IP Address of the storage device
target idx
Target index of the storage device
lun
Lun of the storeage device
flags
flags
Flags:

SET_VRM_LOCK |  | 0x01

CONF_HD_SET_VRM_LOCK
This command sets or clears the vrm lock on a lun. If the flag SET_VRM_LOCK is set the vrm lock will be written, otherwise it will be cleared.
CONF_SPAN_FILES_DIR

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0aa1 |  | yes (entry index 1 - 4) |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Read the path entry end exported iscsi addr. (gen dll only) |
| Write |  | p_octet |  | l_serv |  | Set path to span files (gen dll only). |

Payload Structure (write/in)

Action 4 Bytes
reserved 8 Bytes ...
Path name 1 1 Byte | N x 1 Byte | Path name N 1 Byte |

Action
specifies the action, you can set an entry or clear an entry
Values:

clear entry |  | 0
set entry |  | 1

Path name 1 - N
zero terminated ascii string containing the full path to a span formated storage mounted on windows or directory containing the span files, the path should not end with a '\', payload size must be set, that it includes the zero termination
Payload Structure (read; write/out)

exported ip 32 Bits
target index 1 Byte | lun 1 Byte | reserved 2 Byte
error 32 Bits
path 1 1 Byte | N x 1 Byte | path N 1 Byte |

exported ip
ip of the exported lun, specified by the directory path.
target index
target index of the exported lun, specified by the directory path.
lun
lun id of the exported lun, specified by the directory path.
error
Error code, in case of set path failed. Is always 0 in the payload of read direction. Only relevant for return payload of write direction.
Values:

no error |  | 0
invalid directory path |  | 1
invalid lun info file |  | 2
common error |  | 3

path 1 - N
path to a mounted span formatted storage or directory containing the span files.
CONF_SPAN_FILES
This command allows to set the path to a mounted span formatted storage or directory. You have to send the in payload to set the path. The min payload size is 16 bytes. The max path name length is 1024 bytes including the zero termination. payload size must be set to the size that includes the zero termination but min size is 16 bytes even in case of an empty string (at least zero termination). You can set up to 4 pathes. Use the num param to specify the index of an entry. If you set the path it will check the path. To pass this check, at least a valid Lun info file (INFO.TXT) has to exist. The span are needed later when accessing the storage(e.g header access, replay). The response to the write direction is has the out payload format. If success the error field is zero and the payload includes the set path and the exported lun address. This storage is now accessable by using this address for other commands. if the set failes, the error field is non zero and contains an error code. It is allowed to set path on an index that was already set. The old values will be overwritten, but remember that the effect takes place later, if there are still open references based on the old entry (e.g. running replay, header access).
The cmd can be used for read direction. The response payload contains the export lun address and the path. error code is always zero. If the entry is empty, the path is empty and has only the zero termination.
CONF_SPAN_HISTORY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ace |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | read span history |
| Write |  | p_octet |  | l_serv |  | clear span history or add a span history entry |

Payload Structure

cam 16 Bits | rec idx 16 Bits
action 16 Bits | cnt 16 Bits
span address 1 8 Bytes ...
N x 8 Bytes | span address N 8 Bytes ...

cam
camera line from 1 to max cam
rec idx
recording index from 1 to 2
action
action to do in this command, the command can show the span history, clear the complete history, add a new entry to the history, or show the remount span
Values:

show (read direction only) |  | 0
add(write direction only) |  | 1
clear(write direction only) |  | 2
show remount(read direction only) |  | 3

cnt
number of span address following in this command payload. For action show you can specifie the max number of span history entries to show for in payload. the reply payload will then return a max. of this number of span address. max 8.
span address 1 - N
range of span address from 0 to cnt, maximum 8.
span address content (8 bytes)

ip address |  | 4 bytes
target index |  | 1 byte
lun |  | 1 byte
span index |  | 2 bytes

CONF_SPAN_HISTORY
This command is used by the device to store the span history in the device config, that means it adds (action add) an span adress entry to the config, for each recorded span. The history can be seen by read commando and action show. The history can be cleared by sending a action clear command.
CONF_ACCESS_LUN_MGMT_FILE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0ae2 |  | yes |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Access span header information. |
| Write |  | p_octet |  | l_serv |  | Access lun management information. |

Payload Structure

16 | 32
ip 32 Bits
targ idx 8 Bits | lun 8 Bits | reserved 6 Bytes ...
data n Bytes(max 504 bytes)
8 | 24 |

ip
ip address of the lun
targ idx
target index of the lun
lun
lun
data
user data to read/write from/to the lun mgmt file
CONF_ACCESS_LUN_MGMT_FILE
This command can be used to acces the lun managment file. This exists only on span formatted luns, which were formatted by firmware /generic dll versions, that are able to create this file. Older versions cannot do this. The file name is "lunmgmt.bin". the max size which can be stored is 504 bytes. The in payload for reading or writing this command has to be at least a size of 12 bytes and includes the lun address for read/write from/to lun mgmt file. The response on the read direction includes the user data from the lun mgmt file. The data length will be the remayning bytes from the respons payload size minus the lun address and the reserved bytes (12 bytes together). Same in write direction. The payload size determines the number of bytes to write to the lun mgmt file(max 504 bytes).
CONF_STORAGE_REPORT

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09cf |  | yes (Only span-recording: 1=cam1, 2=cam2, ...) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get information about the storage device |
| Write |  | p_octet |  | l_serv |  | not supported |

Request packet
To get information about a storage device, a read packet with no payload must be send to the rcp server.
Response packet
The server reply will have the following structure:

Type 1 Byte | Availability 1 Byte | Access Type 1 Byte | IO Error Type 1 Byte
IO Error Count 4 Bytes
Throughput Read 4 Bytes
Throughput Write 4 Bytes
iSCSI Login Connection 1 4 Bytes
N x 4 Bytes | iSCSI Login Connection N 4 Bytes ...

Type
Values:

None |  | 0x00
RAM Recording |  | 0x03
iSCSI |  | 0x04
USB |  | 0x05
IDE |  | 0x08
Compact Flash |  | 0x09

Availability
Values:

Unknown |  | 0x00
No |  | 0x01
Yes |  | 0x02
locked by another device |  | 0x03

Access Type
Values:

Unknown |  | 0x00
Read Only |  | 0x01
Read Write |  | 0x02

IO Error Type
Values:

None |  | 0x00
Read |  | 0x01
Write |  | 0x02

IO Error Count
Number of arised I/O errors.
Throughput Read
Kilobytes read from device.
Throughput Write
Kilobytes written to device.
iSCSI Login Connection 1 - N
Fields present only if device type is iSCSI
Sequence of:

16 | 32
Phase 2 Bytes | Error 2 Bytes
8 | 24 |

Phase
Indicates the phase, the iSCSI client has reached on login.
Error
Indicates the error that happend in that state.
CONF_STORAGE_REPORT_SECONDARY

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a50 |  | yes (Only span-recording: 1=cam1, 2=cam2, ...) |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | get information about the storage device of secondary recording, payload same as in command CONF_STORAGE_REPORT |
| Write |  | p_octet |  | l_serv |  | not supported |

CONF_STORAGE_MEDIUM_TYPE

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d3 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | t_dword |  | noprot |  | read the storage medium type (None = 0, USB = 5, IDE = 8, CF = 9, SD = 11) (obsolete) |
| Write |  | t_dword |  | l_serv |  | set the storage medium type (None = 0, USB = 5, IDE = 8, CF = 9)(obsolete and not usable anymore) |

CONF_STORAGE_MEDIUM_AVAIL

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x09d4 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | list of dwords with available storage medium types (first dword USB, second dword iSCSI, third dword RAM) |
| Write |  | void |  | l_serv |  | not supported |

CONF_STORAGE_LIST

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a37 |  | no |  | no |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | Read the device storage list. |
| Write |  | p_octet |  | l_serv |  | Write the stuff. (, not supported while recording is running) |

Payload Structure
Sequence of (max 16):

16 | 32
Storage Descriptor 20 Bytes ...
8 | 24 |

Storage Descriptor

16 | 32
Storage Type 4 Bytes
IP Address 4 Bytes
Target Index 1 Byte | Lun 1 Byte | Fmt Progress 1 Byte | Utilization 1 Byte
iSCSI export 1 Byte | Span Manager 1 Byte | Mgr Status 1 Byte | Mgr Error 1 Byte
Recording Migration Status 4 Bytes
8 | 24 |
Storage Type The type of the storage. Values:
FILE |  | 0x02
RAM |  | 0x03
ISCSI |  | 0x04
USB |  | 0x05
IDE |  | 0x08
CF |  | 0x09
IP Address The IP address of the iscsi server. Set to zero, if the storage type is not iscsi. Target Index The target index on the iscsi server. Set to zero, if the storage type is not iscsi. Lun The iscsi lun. Set to zero, if the storage type is not iscsi. Fmt Progress If the storage is in state formatting, the field indicates the formatting progress in percentage. Utilization If the storage is span formatted, this field indicates the amount capacity used (in percentage). iSCSI export Values:
For local use only |  | 0x00
Make storage available through iSCSI |  | 0x01
Span Manager Values:
Span manager off |  | 0x00
Span manager on |  | 0x01
Span format lun and start span manager |  | 0x02
Migrate lun and start span manager |  | 0x03
Mgr Status The status of the span manager in the response packet. Set to zero in the request packet. Values:
INACTIVE |  | 0x00
STARTING |  | 0x01
FORMATING |  | 0x02
MIGRATING |  | 0x03
OFFLINE |  | 0x04
ONLINE |  | 0x05
STOPPING |  | 0x06
ERROR |  | 0x07
Mgr Error If the span manager status is ERROR, this field contains details of the error that occurred. See command CONF_SPAN_USE_STATUS for possible error codes. Migration Status
16 | 32
Stage 1 Byte | Progress 1 Byte | Error 1 Byte | Reserved 1 Byte
8 | 24 |
Stage The current migration stage. Values:
INIT |  | 0x00
FORMAT SPANS |  | 0x01
UPDATE HEADER |  | 0x02
COPY DATA |  | 0x03
DONE |  | 0x04
Progress The progress of the current stage in percentage. Error Code A possible error code.

Use this command to configure and manage local or remote storage. The storage list may contain up to 16 entries. If a remote (iscsi) storage is to be managed, the lun address has to be specified. Realize, that if you export an remote storage, the device will have preformance drawbacks cause the ip- and iscsi-stack will be passed through twice. Prefer to access the remote storage directly instead.
The storage devices will be exported through iscsi in the order of this list (storage devices with the 'iSCSI export' field set to 'For local use only' [0x00] are omitted) and the storage will appear in the same place of the target name list of an iscsi discovery on that device.
NOTE
If the storage list is empty or only contains entries with the 'iSCSI export' field set to 'For local use only' (0x00), the iscsi server is stopped, if it is running, cause no targets and luns would be provided. If the list contains at least one entry with the 'iSCSI export' field set to 'Make storage available through iSCSI' (0x01), the iscsi server is started, if not already running, to provide the iscsi service. The iscsi server can be controlled through the command CONF_ISCSI_SERVER_STATE too.
CONF_STORAGE_IO

| Tag code |  | NumDes |  | Message |  | SNMP Support |
| 0x0a61 |  | no |  | yes |  | no |
| Datatype |  | Access Level |  | Description |
| Read |  | p_octet |  | noprot |  | List the currently running storage io tasks. |
| Write |  | p_octet |  | l_serv |  | Start or stop a storage io task. |

Request Packet Structure

16 | 32
Lun Address 8 Bytes ...
Start Burst Size 4 Bytes
End Burst Size 4 Bytes
Burst Size Duration 4 Bytes
Burst Size Increase 4 Bytes
Repeat 4 Bytes
Maximum Read Rate 4 Bytes
Maximum Write Rate 4 Bytes
Mode 2 Byte | Flags 2 Byte
ID 4 Bytes
Action 1 Byte | Reserved 3 Bytes
Reserved 44 Bytes ...
8 | 24 |

Lun Address
The address of the storage.

16 | 32
iSCSI IP 4 Bytes
Target Idx 1 Byte | Lun 1 Byte | Reserved or Span Idx 2 Byte
8 | 24 |
iSCSI IP The ip address of the iscsi server Target Idx The index of the target on the iscsi server. Lun The logical unit. Span Idx The index of the span. Only used, if the flag RESTRICT TO SPAN is set.

Start Burst Size
The size in LBAs of the burst the test starts with. This value must be lower or equal to the end burst size.
End Burst Size
The size in LBAs of the burst the test ends with. This value may be clipped to the maximum burst value of the storage.
Burst Size Duration
The number of milliseconds each bust size is read and written.
Burst Size Increase
The number of LBAs the burst size is increased after each burst-duration.
Maximum Read Rate
The maximum datarate that is read in KBit/sec.
Maximum Write Rate
The maximum datarate that is written in KBit/sec.
Repeat
The number of times the test is repeated which means how often the specified burst sequence is run.
Mode
The test may run in the following modes. The modes RECORDING SIMULATION, LATENCY and REPLAY SIMULATION use different fields in the request packet which are not documented yet.
Values:

LINEAR |  | 0x0000
RANDOM |  | 0x0001
RECORDING SIMULATION |  | 0x0002
LATENCY |  | 0x0003
REPLAY SIMULATION |  | 0x0004

If the mode is set to LINEAR then the test reads/write from/to consecutive lba addresses. If the maximum lba is reached and the STORAGE_IO_FLAG_MAX_LBA_END flag is set, the test stops. Otherwise the test wraps its lba pointer to the beginning of its storage.
If the mode is set to RANDOM then the test reads/write from/to randomly chosen lba addresses of the storage.
Flags
Flags to set some options.
Values:

READ ONLY |  | 0x0001
WRITE ONLY |  | 0x0002
KEEP DATA |  | 0x0008
VERIFY WRITE |  | 0x0010
EXP BURST INCREASE |  | 0x0020
ERROR STOP |  | 0x0040
RESTRICT TO SPAN |  | 0x0080
ISCSI SESSION EXCLUSIVE |  | 0x0100
MAX LBA END |  | 0x0200

If the READ ONLY flag is set, only read operations are performed. May not be used simultaneously with the WRITE ONLY flag.
If the WRITE ONLY flag is set, only write operations are performed. May not be used simultaneously with the READ ONLY flag.
If the KEEP DATA flag is set, all lbas that are written are read before so that no recording data should be destroyed. Be careful that no one else writes to this lun simultaneously. In the latter case data on the storage could be lost.
If the VERIFY WRITE flag is set, every lba that was written is read afterwards to verify that the data was correctly written.
If the EXP BURST INCREASE flag is set, the field 'Burst Size Increase' is ignored. Instead the burst size is doubled after each rnu.
If the ERROR STOP flag is set, the tests stops when an io error occurrs.
If the RESTRICT TO SPAN flag is set, the tests only uses the span of the lun, which is specified in the 'Span Idx' field of the lun-address.
If the ISCSI SESSION EXCLUSIVE flag is set, the tests use an exclusive iscsi session which is not shared among other tests.
If the MAX LBA END flag is set, the tests stops when the write pointer reaches the maximum lba address of the lun/span (only in sequential access mode).
ID
Identifier of the storage io. Set to zero when starting a new storage io. Set to the from the start request returned value for stopping a storage io.
Action
Values:

STOP |  | 0x00
START |  | 0x01

Response and Message Packet Structure

16 | 32
Lun Address 8 Bytes ...
Start Burst Size 4 Bytes
End Burst Size 4 Bytes
Burst Size Duration 4 Bytes
Burst Size Increase 4 Bytes
Repeat 4 Bytes
Maximum Read Rate 4 Bytes
Maximum Write Rate 4 Bytes
Mode 2 Byte | Flags 2 Byte
ID 4 Bytes
Status 1 Byte | Error 1 Byte | Reserved 2 Bytes
Reapeat Count 4 Bytes
Current Burst Size 4 Bytes
Current Offset 4 Bytes
Current Read Datarate 4 Bytes
Current Write Datarate 4 Bytes
Read Bytes 4 Bytes
Write Bytes 4 Bytes
Read Operations 4 Bytes
Write Operations 4 Bytes
Read Errors 4 Bytes
Write Errors 4 Bytes
8 | 24 |

Lun Address
See request packet structure for details.
Start Burst Size
See request packet structure for details.
End Burst Size
See request packet structure for details.
Burst Size Duration
See request packet structure for details.
Burst Size Increase
See request packet structure for details.
Repeat
See request packet structure for details.
Maximum Read Rate
See request packet structure for details.
Maximum Write Rate
See request packet structure for details.
Mode
See request packet structure for details.
Flags
See request packet structure for details.
ID
Identifier of the storage io. This value must be specified on actions other than start.
Status
Values:

STOPPING |  | 0x00
STARTING |  | 0x01
RUNNING |  | 0x02
DONE |  | 0x03
ERROR |  | 0x04

Error
Values:

INTERNAL |  | 0x01
LUN |  | 0x02
INVALID PARAMS |  | 0x03
READ |  | 0x04
WRITE |  | 0x05
WRITE VALIDATE |  | 0x06

Repeat Count
The number of turns the test repeated so far.
Current Burst Size
The number of LBAs of the current burst.
Current Offset
The current position of the i/o pointer in percentage of the whole storage. This value is not significant in random access mode.
Current Read Datarate
The current read datarate in KBit/s.
Current Write Datarate
The current write datarate in KBit/s.
Read Bytes
The number of bytes that were read since the test was started.
Write Bytes
The number of bytes that were written since the test was started.
Read Operations
The number of read operations successfully performed since the test was started.
Write Operations
The number of write operations successfully performed since the test was started.
Read Errors
The number of read errors since the test was started.
Write Errors
The number of read errors since the test was started.
Appendix - specific error codes
Each rcp command can generate an generic RCP fault as described in the chapter "Rcp Protocol Procedure". Additional command specific error codes are defined. If an command specific error occurs the Response is 2 bytes long. The first byte is set to RCP_ERROR_COMMAND_SPECIFIC (0x1f), the second byte is set to the specific fault.
The following command specific errors are defined:
Storage specific error codes
Span errors

SPAN_ERROR_INV_SPN_IDX |  | 0x02
SPAN_ERROR_INV_HDR_TYPE |  | 0x03
SPAN_ERROR_INV_ADDR_LIST |  | 0x04
SPAN_ERROR_NOT_MNTD |  | 0x05
SPAN_ERROR_INV_FS |  | 0x06
SPAN_ERROR_INV_LUN_NFO |  | 0x07
SPAN_ERROR_BAD_HDR_CKSM |  | 0x08
SPAN_ERROR_INV_IDX |  | 0x09
SPAN_ERROR_RD_ONLY |  | 0x0a
SPAN_ERROR_NO_REC_DAT |  | 0x0b
SPAN_ERROR_INV_PART_NFO |  | 0x0c
SPAN_ERROR_CONV_REC |  | 0x0d
SPAN_ERROR_SPAN_REQUEST_FAILED |  | 0x0e
SPAN_ERROR_SPAN_REQUEST_RETENTION_TIME |  | 0x0f
SPAN_ERROR_OLD_LUN_NFO |  | 0x20

HDD PMM errors

HD_PMM_ERROR_TIMEOUT |  | 0x12
HD_PMM_ERROR_CREATE_FAILED |  | 0x22
HD_PMM_ERROR_ACCESS_DENIED |  | 0x32
HD_PMM_ERROR_DEVICE_PRESENT_TIMEOUT |  | 0x42
HD_PMM_ERROR_LUN_LOCK |  | 0x52
HD_PMM_ERROR_COMMON |  | 0xf2

ISCSI errors

ISCSI_ERR_CONNECT |  | 0x31
ISCSI_ERR_INV_LUN |  | 0x33
ISCSI_ERR_LOGIN |  | 0x34
ISCSI_ERR_INV_TARG_IDX |  | 0x35
ISCSI_ERR_PWD |  | 0x36
ISCSI_ERR_PROTO |  | 0x37
ISCSI_ERR_TARG_NOT_REACH |  | 0x38
ISCSI_ERR_NO_MEMORY |  | 0x3a
ISCSI_ERR_SESS_CREATE |  | 0x3b
ISCSI_ERR_INV_PARAMS |  | 0x3c
ISCSI_ERR_SESS_NOT_FOUND |  | 0x3d
ISCSI_ERR_DISCONN |  | 0x3e
ISCSI_ERR_TIMEOUT |  | 0x3f
ISCSI_ERR_SOCK |  | 0x5f
ISCSI_ERR_TARG_PM |  | 0x6f
ISCSI_SOCK_CLOSED |  | 0x7f
ISCSI_ERR_TCP_CONN_RESET |  | 0x8f
ISCSI_ERR_INTR_NOT_SUPP |  | 0x9f
ISCSI_ERR_IP_ZERO |  | 0xa0
ISCSI_ERR_OUT_OF_RESOURCES |  | 0xa1