Release Notes

Release Notes

Keywords: Version information, version upgrade

Abstract: This document provides detailed version information and upgrade procedure for IPC\_G6102-B5015P10D1702C30.

Acronym:

| Acronym | Full Name |
| --- | --- |
| IPC | IP Camera |

Content

[1 Version Information 3](#_Toc484080487)

[1.1 Version Number 3](#_Toc484080488)

[1.2 Release History 3](#_Toc484080489)

[1.3 Version Mapping Table 3](#_Toc484080490)

[1.4 Feature and Change Description 4](#_Toc484080491)

[1.1 Upgrade Overview 4](#_Toc484080492)

[1.1.1 Version Upgrade Environment 4](#_Toc484080493)

[1.1.2 Version Upgrade Modes 4](#_Toc484080494)

[1.2 Upgrade Procedure 4](#_Toc484080495)

[1.2.1 Upgrade Through the Web 4](#_Toc484080496)

# Version Information

## Version Number

IPC\_G6102-B5015P10D1702C30

## Release History

Table 1 Released versions

| Version No. | Basic Version No. | Released On | Remarks |
| --- | --- | --- | --- |
| IPC\_G6102-B5015P10D1702C30 | IPC\_G6102-B5013P12D1611C35 | 2017-06-01 | Improved release |

## Version Mapping Table

Table 2 Product models and corresponding versions

|  |  |
| --- | --- |
| Product Series | IPC Series |
| Series | IPC2124SR3、IPC324ER3、 IPC3614SR3、IPC314SR、IPC2122SR3、IPC742SR9、IPC744SR5、IPC3612ER3、IPC322SR3、IPC2222SR5、IPC2224SR5、IPC3634ER3、IPC814SR |
| Models | **IPC2124SR3 series:** IPC2124SR3-DPF36、IPC2124SR3-DPF60、IPC2124SR3-DPF120  IPC2124SR3-DPF36-16G、IPC2124SR3-DPF60-16G、IPC2124SR3-APF40、IPC2124SR3-APF60 |
| **IPC324ER3 series:** IPC324ER3-DVPF28、IPC324ER3-DVPF36、IPC324ER3-DVPF60 |
| **IPC3614SR3 series:**IPC3614SR3-DPF28、IPC3614SR3-DPF36、IPC3614SR3-DPF60  IPC3614SR3-DPF28M、IPC3614SR3-DPF36M、IPC3614SR3-DPF60M |
| **IPC314SR series:** IPC314SR-DVPF28、IPC314SR-DVPF36 |
| **IPC2122SR3 series：**IPC2122SR3-UPF36、IPC2122SR3-UPF40、IPC2122SR3-UPF60、IPC2122SR3-PF40-B、IPC2122SR3-PF60-B、IPC2122SR3-APF40-C、IPC2122SR3-APF60-C |
| **IPC742SR9 series：**IPC742SR9-PZ30-32G |
| **IPC744SR5 series：**IPC744SR5-PF40-32G、IPC744SR5-PF60-32G |
| **IPC3612ER3 series：**IPC3612ER3-PF28-B、IPC3612ER3-PF40-B、IPC3612ER3-PF60-B |
| **IPC322SR3 series：**IPC322SR3-DVSPF28-B、IPC322SR3-DVSPF40-B、IPC322ER3-DUVPF28-B、IPC322ER3-DUVPF40-B、IPC322SR3-UVPF28-B、IPC322SR3-UVPF40-B |
| **IPC2222SR5 series：**IPC2222SR5-UPF40-B、IPC2222SR5-UPF60-B |
| **IPC2224SR5 series：**IPC2224SR5-PF40-B、IPC2224SR5-PF60-B、IPC2224SR5-UPF40-B、IPC2224SR5-UPF60-B |
| **IPC3634ER3 series:** IPC3634ER3-DPZ28 |
| **IPC814SR series:**IPC814SR-DVSPF16、IPC814SR-DVPF16 |
| Target file name | IPC\_G6102-B5015P10D1702C30.zip |

## Feature and Change Description

None.

## Upgrade Overview

### Version Upgrade Environment

#### Network Architecture for Upgrade

Figure 1 Network architecture



As shown in this figure, the version files are stored on the PC that is connected to the IPCs through the network.


### Version Upgrade Modes

You can upgrade through the Web.

## Upgrade Procedure

### Upgrade Through the Web

* + - * 1. Log in to the Web interface as **admin** (default password: 123456).
        2. Click **Setup** > **Maintenance** > **Device Maintenance**. The **Device Maintenance** page is displayed.



* + - * 1. Click **Browse** in the **Firmware Upgrade** area. In the **Select** dialog box that appears, select the upgrade file package, for example, IPC\_G6102-XXXXX.zip, and then click **Open.**
        2. Click **Upgrade**. You cannot operate on other pages during the upgrade process.
        3. Wait till the upgrade is completed. A message appears to indicate successful upgrade and prompt you to log in again after the device restarts.

No part of this manual may be reproduced or transmitted in any form or by any means without prior written consent of our company.

The information in this manual is subject to change without notice.